; Finger Printer Sensor Reader 
; (c) Copyright 2011 EgisTec.
;

[Version]
Signature="$CHICAGO$"
Class=SecBioDev
ClassGUID={a8e6a1b0-bce2-11dc-95ff-0800200c9a66}
provider="EgisTec"
DriverPackageType=PlugAndPlay
CatalogFile=FPSensor.cat
DriverVer=09/15/2011,3.0.14.0

[SourceDisksNames]
1=%FPSInstall%,,,

[SourceDisksFiles]
FPSensor.sys = 1


[Manufacturer]
%LTT_Corp%=LTT_Corp,NTamd64

[LTT_Corp]
%FPSensorReaderES603%=FPSensor.Dev, USB\VID_1C7A&PID_0603
%FPSensorReaderES603%=FPSensor.Dev, USB\VID_1C7A&PID_0803
%FPSensorReader%=FPSensor.Dev, USB\VID_1C7A&PID_0801
%FPSensorReader%=FPSensor.Dev, USB\VID_CD15&PID_6711

[LTT_Corp.NTamd64]
%FPSensorReaderES603%=FPSensor.Dev, USB\VID_1C7A&PID_0603
%FPSensorReaderES603%=FPSensor.Dev, USB\VID_1C7A&PID_0803
%FPSensorReader%=FPSensor.Dev, USB\VID_1C7A&PID_0801
%FPSensorReader%=FPSensor.Dev, USB\VID_CD15&PID_6711




[PreCopySection]
HKR,,NoSetupUI,,1


[ClassInstall32]
AddReg=SecBioDev_Class_Addreg

[SecBioDev_Class_Addreg]
HKR,,,,%ClassName%
HKR,,SilentInstall,,1
HKR,,Icon,,"-24"



[DestinationDirs]
FPSensor.Files.Ext = 10,System32\Drivers


[FPSensor.Dev.NTx86]
CopyFiles=FPSensor.Files.Ext
AddReg=FPSensor.AddReg

[FPSensor.Dev.NTx86.Services]
Addservice = FPSensor, 0x00000002, FPSensor.AddService

[FPSensor.Dev.NTamd64]
CopyFiles=FPSensor.Files.Ext
AddReg=FPSensor.AddReg

[FPSensor.Dev.NTamd64.Services]
Addservice = FPSensor, 0x00000002, FPSensor.AddService

[FPSensor.AddService]
DisplayName    = %FPSensor.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\FPSensor.sys
AddReg         = FPSensor.AddReg
LoadOrderGroup = Base

[FPSensor.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,FPSensor.sys
HKR,"Parameters","C3ModeEnable",0x10001,1
HKR,"Parameters","ContactSensor",0x10001,1
HKR,"Parameters","Exception",0x10001,0
HKR,"Parameters","JadeDCoffset",0x10001,54
HKR,"Parameters","JadeGain",0x10001,4
HKR,"Parameters","JadeDTVRT",0x10001,8
HKR,"DebugMsg","DEBUG",0x00010008,"111"
HKR,"Parameters",EventMessageFile,0x00020000,"%10%\System32\iologmsg.dll;%10%\system32\drivers\Eventlog.sys"
HKR,"Parameters",TypesSupported,0x00010001,7

[FPSensor.Files.Ext]
FPSensor.sys

;---------------------------------------------------------------;

[Strings]
LTT_Corp="EgisTec"
FPSensorReader="Fingerprint Reader"
FPSensorReaderES603="EgisTec ES603"
FPSensor.SvcDesc="EgisTec-Corp Fingerprint Reader Driver (FPSensor.sys)"
FPSInstall="Fingprint Sensor driver Installation Disk"
ClassName = "Secure biometric devices"

; Simplified Chinese
[Strings.0804]
LTT_Corp="EgisTec"
FPSensorReader="Fingerprint Reader"
FPSensorReaderES603="EgisTec ES603"
FPSensor.SvcDesc="EgisTec-Corp Fingerprint Reader Driver (FPSensor.sys)"
FPSInstall="Fingprint Sensor driver Installation Disk"
ClassName = "生物识别设备"

; Traditional Chinese
[Strings.0404]
LTT_Corp="EgisTec"
FPSensorReader="Fingerprint Reader"
FPSensorReaderES603="EgisTec ES603"
FPSensor.SvcDesc="EgisTec-Corp Fingerprint Reader Driver (FPSensor.sys)"
FPSInstall="Fingprint Sensor driver Installation Disk"
ClassName = "安全生物測定裝置"