; NETCOKK.INF
;
; corega FEtherII PCC-TXD LAN Card INF file for Windows 98/Me/2000
;
; Copyright (C) corega K.K. 2000

[Version]
Signature  ="$Windows NT$"
Class      =Net
ClassGUID  ={4d36e972-e325-11ce-bfc1-08002be10318}
Provider   =%corega%
LayoutFile =layout.inf
DriverVer  =2/10/2002,1.1.0.0

;
; Table of Contents
;
[Manufacturer]
%V_corega%=corega

; sections for Win98/Me
;-------------------------------------------------------------
[corega]
%CO2DPCX5%=CO2DPCX5.ndi,PCMCIA\corega_K.K.-corega_FEtherII_PCC-TXD-BC50

[CO2DPCX5.ndi]
AddReg=CO2DPCX5.ndi.reg,CO2DPCX5.params.reg
CopyFiles=CO2DPCX5.CopyFiles,Inf.CopyFiles


[CO2DPCX5.ndi.reg]
HKR,,DevLoader,0,*ndis
HKR,,DeviceVxDs,0,CO2DPCX5.sys
HKR,,EnumPropPages,0,netdi.dll
HKR,Ndi,DeviceID,0,PCMCIA\corega_K.K.-corega_FEtherII_PCC-TXD-BC50
HKR,Ndi,CardType,0,PCMCIA
HKR,NDIS,LogDriverName,0,CO2DPCX5
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0a
HKR,Ndi\Interfaces,DefUpper,0,ndis3
HKR,Ndi\Interfaces,DefLower,0,ethernet
HKR,Ndi\Interfaces,UpperRange,0,ndis3
HKR,Ndi\Interfaces,LowerRange,0,ethernet
; Install sections
HKR,Ndi\Install,ndis3,,"CO2DPCX5.ndis3"

[CO2DPCX5.ndis3]
CopyFiles=CO2DPCX5.CopyFiles

[CO2DPCX5.CopyFiles]
CO2DPCX5.SYS

[CO2DPCX5.params.reg]
HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,,NDI\params\InterruptNumber,0,1
HKR,,Ndi\params\interruptNumber,0,
HKR,,NDI\params\InterruptNumber,0,1
HKR,,NDI\params\IOBaseAddress,0,1
HKR,,NDI\params\IOBaseAddress,0,
HKR,,NDI\params\IOBaseAddress,0,1

[CO2DPCX5.Common.reg]
HKR,Ndi\params\ConnectionType,ParamDesc,,"Connection Type"
HKR,Ndi\params\ConnectionType,default,,0
HKR,Ndi\params\ConnectionType,type,,enum
HKR,Ndi\params\ConnectionType\enum,0,,"Auto-Negotiation"
HKR,Ndi\params\ConnectionType\enum,8,,"100BaseTx"
HKR,Ndi\params\ConnectionType\enum,9,,"100BaseTx Full_Duplex"
HKR,Ndi\params\ConnectionType\enum,2,,"10BaseT (Twisted_Pair)"
HKR,Ndi\params\ConnectionType\enum,3,,"10BaseT Full_Duplex"
HKR,NDI\params\ConnectionType,flag,1,20,00,00,00

; sections for Win2000
;--------------------------------------------------------------
[CO2DPCX5.ndi.NT]
Characteristics = 0x84
BusType         = 8      ; PCMCIA Bus
AddReg          = CO2DPCX5.Common.reg,CO2DPCX5.ndi.NT.reg
CopyFiles       = CO2DPCX5.NT.CopyFiles

[CO2DPCX5.ndi.NT.Services]
AddService = CO2DPCX5, 2, CO2DPCX5.Service, CO2DPCX5.AddEventLog

;-------------------------------------------------------------------------------
; Service and Driver
;
[CO2DPCX5.ndi.NT.reg]
HKR, Ndi, Service, 0, "CO2DPCX5"
HKR,Ndi\Interfaces,DefUpper,,"ndis5"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,0,"ndis5"
HKR,Ndi\Interfaces,LowerRange,0,"ethernet"

[CO2DPCX5.NT.CopyFiles]
CO2DPCX5.sys,,,2

[CO2DPCX5.Service]
DisplayName         =   %Service.DispName%
ServiceType         =   1 ;%SERVICE_KERNEL_DRIVER%
StartType           =   3 ;%SERVICE_AUTO_START%
ErrorControl        =   1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary       =   %12%\CO2DPCX5.sys
LoadOrderGroup      =   NDIS

[CO2DPCX5.AddEventLog]
AddReg = CO2DPCX5.AddEventLog.reg

[CO2DPCX5.AddEventLog.reg]
HKR,    ,   EventMessageFile,   0x00020000,"%%SystemRoot%%\System32\netevent.dll,%%SystemRoot%%\System32\drivers\CO2DPCX5.sys"
HKR,    ,   TypesSupported,     0x00010001, 7

HKR,    ,   TextModeFlags,      0x00010001,0x0001

[Inf.CopyFiles]
;CO2DPCX5.INF

[DestinationDirs]
DefaultDestDir=11
CO2DPCX5.CopyFiles=11
CO2DPCX5.NT.CopyFiles=12
Inf.CopyFiles=17        ; Windows Inf Directory

[SourceDisksNames]
1=%Disk_Desc%,,,

[SourceDisksFiles]
CO2DPCX5.SYS=1

;
; Translatable strings
;
[Strings]

; Manufacturer names
;
corega="corega K.K."

; Adapter names
;
V_corega="corega K.K."
CO2DPCX5="corega FEtherII PCC-TXD LAN Card"
Disk_Desc="corega FEtherII PCC-TXD Driver Disk"
Service.DispName    =   "corega FEtherII PCC-TXD LAN Card"

