; AX88140.INF
;
; INF file for Windows NT 5.0
;
; ASIX AX88140 Based PCI Fast Ethernet Adapter
;
; Copyright 1996-1997, ASIX Corporation
;

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %V_ASIX%
LayoutFile  = layout.inf

[Manufacturer]
%V_ASIX%=ASIX

[ASIX]
%AX88140.DeviceDesc%=AX88140.ndi, PCI\VEN_125B&DEV_1400
%AX8814XA.DeviceDesc%=AX88140.ndi, PCI\VEN_125B&DEV_1400&SUBSYS_00000000
%AX8814XB.DeviceDesc%=AX88140.ndi, PCI\VEN_125B&DEV_1400&SUBSYS_11001186
%CNETPRO110C.DeviceDesc%=AX88140.ndi, PCI\VEN_125B&DEV_1400&SUBSYS_434E4554

[AX88140.ndi.NTX86]
Characteristics = 0x84
BusType         = 5
AddReg          = AX88140.reg, AX88140.ndi.reg
CopyFiles       = AX88140.CopyFiles

[AX88140.ndi.NTX86.Services]
AddService = AX88140, 2, AX88140.Service, AX88140.EventLog

[AX88140.reg]
;HKR, ,                                      AdapterCFID,    0, 1400125B
HKR, ,                                      AdapterType,, 5
HKR, ,                                      BusType,,5
HKR, ,                                      MediaType,      0, "1"
HKR, ,                                      BusNumber,, 0
HKR, ,                                      SlotNumber,, 0

[AX88140.ndi.reg]
HKR, Ndi,                                   Service,        0, "AX88140"
HKR, Ndi\Interfaces,                        DefLower,       0, "ethernet"
HKR, Ndi\Interfaces,                        LowerRange,     0, "ethernet"
HKR, Ndi\Interfaces,                        DefUpper,       0, "ndis5"
HKR, Ndi\Interfaces,                        UpperRange,     0, "ndis5"
HKR, Ndi\Install,                           ,               0, "AX88140.Install"

HKR, Ndi\params\ConnectionType,             ParamDesc,  0, "Connection Type"
HKR, Ndi\params\ConnectionType,             default,    0, "0"
HKR, Ndi\params\ConnectionType,             type,       0, "enum"
HKR, Ndi\params\ConnectionType\enum,        "0",        0, "AutoSense"
HKR, Ndi\params\ConnectionType\enum,        "8",        0, "100BaseTx"
HKR, Ndi\params\ConnectionType\enum,        "9",        0, "100BaseTx Full_Duplex"
HKR, Ndi\params\ConnectionType\enum,        "0B",       0, "100BaseFx"
HKR, Ndi\params\ConnectionType\enum,        "0C",       0, "100BaseFx Full_Duplex"
HKR, Ndi\params\ConnectionType\enum,        "2",        0, "10BaseT (Twisted_Pair)"
HKR, Ndi\params\ConnectionType\enum,        "3",        0, "10BaseT Full_Duplex"

[AX88140.Service]
DisplayName     = %AX88140.DeviceDesc%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_AUTO_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\AX88140.sys
LoadOrderGroup  = NDIS

[AX88140.CopyFiles]
AX88140.sys,,,2

[DestinationDirs]
AX88140.CopyFiles = 12

[AX88140.EventLog]
AddReg = AX88140.AddEventLog.reg

[AX88140.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

[strings]
; Provider
; Manufacturers
V_ASIX="ASIX Electronics"
; PNP Devices
AX88140.DeviceDesc="ASIX AX88140 Based PCI Fast Ethernet Adapter"
AX8814XA.DeviceDesc="ASIX AX8814X Based PCI Fast Ethernet Adapter"
AX8814XB.DeviceDesc="ASIX AX8814X Based PCI Fast Ethernet Adapter"
CNETPRO110C.DeviceDesc="CNet PRO110 PCI Fast Ethernet Adapter"
