;
; mvykxx
; Supported hardware: Marvell Yukon Ethernet Controller
;
; (C)Copyright 2007-2013 Marvell(R).
; 
; All rights reserved.
;

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4D36E972-E325-11CE-BFC1-08002BE10318}
Provider	= %Marvell%
DriverVer=09/30/2013,20.10.11.3
CatalogFile=mvykxx.cat

[Manufacturer]
%Marvell%      = Marvell, NTamd64

[ControlFlags]

ExcludeFromSelect       = *

[Marvell.NTamd64]
 
%Yukon-Generic_1.DeviceDesc% = mvykxx.ndi, PCI\VEN_11AB&DEV_4381
%Yukon-Generic_2.DeviceDesc% = mvykxx.ndi, PCI\VEN_11AB&DEV_4370
%Yukon-Generic_2.DeviceDesc% = mvykxx.ndi, PCI\VEN_11AB&DEV_4373
%Yukon-Generic_3.DeviceDesc% = mvykxx.ndi, PCI\VEN_11AB&DEV_4382
%Yukon-Generic_4.DeviceDesc% = mvykxx.ndi, PCI\VEN_11AB&DEV_4383&CC_0200 

;-------------------------------------------------------------------------------
; 

[mvykxx.ndi.NTamd64]
DelReg          = mvykxx.delreg.common
AddReg          = mvykxx.reg, 
AddReg          = mvykxx.csum.params
AddReg          = mvykxx.addr.params
AddReg          = mvykxx.imod.params
AddReg          = mvykxx.common.params
AddReg          = mvykxx.framesize.params
AddReg          = mvykxx.wakeonmagicpacket.params
AddReg          = mvykxx.wakeonpatternmatch.params
AddReg          = mvykxx.wolw10.params
AddReg          = mvykxx.pmoffloaddefault.params
AddReg          = mvykxx.lsov2.params
AddReg          = mvykxx.link.params

Characteristics = 0x84
BusType         = 5
CopyFiles       = mvykxx.CopyFiles
*IfType         = 6             ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0             ; NdisMedium802_3
*PhysicalMediaType = 14         ; NdisPhysicalMedium802_3

[mvykxx.ndi.NTamd64.Services]
AddService      = mvyksvc, 0x02, mvyksvc.Service, common.EventLog

[mvykxx.csum.params]
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		ParamDesc,	0, %IPChecksumOffloadIPv4%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Type,		0, "enum"
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*IPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*IPChecksumOffloadIPv4,		Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	ParamDesc,	0, %TCPChecksumOffloadIPv4%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	ParamDesc,	0, %UDPChecksumOffloadIPv4%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv4,	Default,	0, "3"

HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	ParamDesc,	0, %TCPChecksumOffloadIPv6%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*TCPChecksumOffloadIPv6,	Default,	0, "3"

HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	ParamDesc,	0, %UDPChecksumOffloadIPv6%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Type,		0, "enum"
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"2",		0, %RXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"1",		0, %TXEna%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*UDPChecksumOffloadIPv6,	Default,	0, "3"

[mvykxx.addr.params]
HKR, Ndi\Params\NetworkAddress,	ParamDesc,	0, %NetworkAddress%
HKR, Ndi\Params\NetworkAddress,	Type,		0, "edit"
HKR, Ndi\Params\NetworkAddress,	LimitText,	0, "18"
HKR, Ndi\Params\NetworkAddress,	UpperCase,	0, "1"
HKR, Ndi\Params\NetworkAddress,	Default,		0, ""
HKR, Ndi\Params\NetworkAddress,	Optional,		0, "1"

[mvykxx.imod.params]
HKR, Ndi\Params\*InterruptModeration,		ParamDesc,	0, %InterruptModeration%
HKR, Ndi\Params\*InterruptModeration,		Type,		0, "enum"
HKR, Ndi\Params\*InterruptModeration\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*InterruptModeration\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*InterruptModeration,		Default,	0, "1"

HKR,, InterruptModerationRate,, "5000"

[mvykxx.common.params]
HKR,, MaxMulticast,, "32"
HKR,, MessageLog,, "3"
HKR,, *PriorityVLANTag,, "1"

[mvykxx.framesize.params]
HKR, Ndi\params\*JumboPacket,	ParamDesc,	0, %JumboPacket%
HKR, Ndi\params\*JumboPacket,	Type,		0, "enum"
HKR, Ndi\params\*JumboPacket\enum,	"0",	0, "%Bytes1514%"
HKR, Ndi\params\*JumboPacket\enum,	"1",	0, "%Bytes4088%"
HKR, Ndi\params\*JumboPacket\enum,	"2",	0, "%Bytes9014%"
HKR, Ndi\params\*JumboPacket,	Default,	0, "0"

[mvykxx.wakeonmagicpacket.params]
HKR, Ndi\Params\*WakeOnMagicPacket,		ParamDesc,	0, %WakeOnMagicPacket%
HKR, Ndi\Params\*WakeOnMagicPacket,		Type,		0, "enum"
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*WakeOnMagicPacket\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*WakeOnMagicPacket,		Default,	0, "1"

[mvykxx.wakeonpatternmatch.params]
HKR, Ndi\Params\*WakeOnPattern,		ParamDesc,	0, %WakeOnPatternMatch%
HKR, Ndi\Params\*WakeOnPattern,		Type,		0, "enum"
HKR, Ndi\Params\*WakeOnPattern\enum,	"1",		0, %Enabled%
HKR, Ndi\Params\*WakeOnPattern\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*WakeOnPattern,		Default,	0, "1"

[mvykxx.wolw10.params]
HKR,, WakeUpSpeed,, "2"

[mvykxx.pmoffloaddefault.params]
HKR,, *PMNSOffload,,	"1"
HKR,, *PMARPOffload,,	"1"

[mvykxx.lsov2.params]
HKR, Ndi\Params\*LsoV2IPv4,			ParamDesc,	0, %LsoV2IPv4%
HKR, Ndi\Params\*LsoV2IPv4,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV2IPv4\enum,	"1",	0,	%Enabled%
HKR, Ndi\Params\*LsoV2IPv4\enum,	"0",	0,	%Disabled%
HKR, Ndi\Params\*LsoV2IPv4,	Default,	0,	"1"

HKR, Ndi\Params\*LsoV2IPv6,			ParamDesc,	0, %LsoV2IPv6%
HKR, Ndi\Params\*LsoV2IPv6,			Type,		0, "enum"
HKR, Ndi\Params\*LsoV2IPv6\enum,	"1",	0,	%Enabled%
HKR, Ndi\Params\*LsoV2IPv6\enum,	"0",	0,	%Disabled%
HKR, Ndi\Params\*LsoV2IPv6,	Default,	0,	"1"

[mvykxx.link.params]

HKR, Ndi\Params\*FlowControl,		ParamDesc,	0, %FlowControl%
HKR, Ndi\Params\*FlowControl,		Type,		0, "enum"
HKR, Ndi\Params\*FlowControl\enum,	"3",		0, %TXRXEna%
HKR, Ndi\Params\*FlowControl\enum,	"0",		0, %Disabled%
HKR, Ndi\Params\*FlowControl,		Default,	0, "3"

HKR,Ndi\Params\*SpeedDuplex,      ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,      Type,       0, "enum"
HKR,Ndi\Params\*SpeedDuplex,      Default,    0, "0"
HKR,Ndi\Params\*SpeedDuplex\enum, "0",        0, %Autosense%
HKR,Ndi\Params\*SpeedDuplex\enum, "1",        0, %10MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "2",        0, %10MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "3",        0, %100MHD%
HKR,Ndi\Params\*SpeedDuplex\enum, "4",        0, %100MFD%
HKR,Ndi\Params\*SpeedDuplex\enum, "6",        0, %1000MFD%

[mvykxx.reg]
HKR, Ndi\Interfaces, UpperRange,, "ndis5"
HKR, Ndi\Interfaces, LowerRange,, "ethernet"
HKR, Ndi, Service,, "mvyksvc"

;-----------------------------------------------------------------------------
;
; Enable MSI Section
;
;-----------------------------------------------------------------------------
[mvykxx.ndi.NTx86.HW]
AddReg			= mvykxx.msisupport
[mvykxx.msisupport]
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 1

;-----------------------------------------------------------------------------
;
; This section contain the keys which will be deleted. These are old keys
; which are not any more supported in newest INF.
;
;-----------------------------------------------------------------------------
[mvykxx.delreg.common]
HKR, Ndi\Params\BatterySpeedSettings
HKR, Ndi\Params\BatteryLinkDetectionMode
HKR, Ndi\Params\WakeUpSpeed
HKR, Ndi\Params\WakeFromShutdown
HKR, Ndi\Params\FixedIntMod

HKR,, BatteryLinkDetectionMode
HKR,, BatterySpeedSettings
HKR,, FixedIntMod

[mvyksvc.Service]
DisplayName	= %mvykxx.DriverDesc%
ServiceType	= 1
StartType = 3
ErrorControl = 1
ServiceBinary  = %12%\mvykxx.sys
LoadOrderGroup = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile,	0x00020000, "%%SystemRoot%%\System32\Drivers\mvykxx.sys"
HKR,, TypesSupported,	0x00010001, 7

[SourceDisksNames]
1 = %DriverDisk%,,,

[SourceDisksFiles]
mvykxx.sys	= 1,,

[mvykxx.CopyFiles]
mvykxx.sys,,,2

[DestinationDirs]
DefaultDestDir = 12
mvykxx.CopyFiles=	12

;-----------------------------------------------------------------------------
;
; Localizable Strings
;
;-----------------------------------------------------------------------------
[Strings]

Marvell = "Marvell"
FlowControl = "Flow Control"
InterruptModeration = "Interrupt Moderation"
IPChecksumOffloadIPv4 = "IPv4 Checksum Offload"
JumboPacket = "Jumbo Packet"
LsoV2IPv4 = "Large Send Offload V2 (IPv4)"
LsoV2IPv6 = "Large Send Offload V2 (IPv6)"
ReceiveBuffers = "Receive Buffers"
SpeedDuplex = "Speed & Duplex"
TCPChecksumOffloadIPv4 = "TCP Checksum Offload (IPv4)"
TCPChecksumOffloadIPv6 = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadIPv4 = "UDP Checksum Offload (IPv4)"
UDPChecksumOffloadIPv6 = "UDP Checksum Offload (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"

NetworkAddress = "Network Address"
10MFD = "10 Mbps Full Duplex"
10MHD = "10 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
1000MFD = "1.0 Gbps Full Duplex"
Autosense = "Auto Negotiation"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
Disabled = "Disabled"
Enabled = "Enabled"
RXEna = "Rx Enabled"
TXEna = "Tx Enabled"
TXRXEna = "Rx & Tx Enabled"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Chinese (Taiwan)
[Strings.0404]
Marvell = "Marvell"
FlowControl = "流控制"
InterruptModeration = "中斷模式"
IPChecksumOffloadIPv4 = "卸載IPv4校驗和"
JumboPacket = "巨型包"
LsoV2IPv4 = "大量傳送負載 V2(IPv4)"
LsoV2IPv6 = "大量傳送負載 V2(IPv6)"
ReceiveBuffers = "接收緩衝區"
SpeedDuplex = "速度和雙工"
TCPChecksumOffloadIPv4 = "卸載TCP校驗和(IPv4)"
TCPChecksumOffloadIPv6 = "卸載TCP校驗和(IPv6)"
UDPChecksumOffloadIPv4 = "卸載UDP校驗和(IPv4)"
UDPChecksumOffloadIPv6 = "卸載UDP校驗和(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "網路位址"
10MFD = "10 Mbps 全雙工"
10MHD = "10 Mbps 半雙工"
100MFD = "100 Mbps 全雙工"
100MHD = "100 Mbps 半雙工"
1000MFD = "1.0 Gbps 全雙工"
Autosense = "自動感應"
Bytes1514 = "1514 位元組"
Bytes4088 = "4088 位元組"
Bytes9014 = "9014 位元組"
Disabled = "禁用"
Enabled = "啟用"
RXEna = "啟用Rx"
TXEna = "啟用Tx"
TXRXEna = "啟用Tx和Rx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Czech
[Strings.0405]
Marvell = "Marvell"
FlowControl = "Řízení toku"
InterruptModeration = "Zmírnění přerušení"
IPChecksumOffloadIPv4 = "Odstr.kont.souč. pro IPv4"
JumboPacket = "Jumbo Packet"
LsoV2IPv4 = "Sniž.z.rozs.od.V2(IPv4)"
LsoV2IPv6 = "Sniž.z.rozs.od.V2(IPv6)"
ReceiveBuffers = "Vyrovnávací paměti příjmu"
SpeedDuplex = "Rychlost a duplex"
TCPChecksumOffloadIPv4 = "Odstr.kon.souč.TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Odstr.kon.souč.TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Odst.kon.souč. UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Odstr.kon.souč.UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Síťová adresa"
10MFD = "10 Mb/s plně duplexní"
10MHD = "10 Mb/s poloduplexní"
100MFD = "100 Mb/s plně duplexní"
100MHD = "100 Mb/s poloduplexní"
1000MFD = "1.0 Gb/s plně duplexní"
Autosense = "Automatické vyjednávání"
Bytes1514 = "1514 Bytů"
Bytes4088 = "4088 Bytů"
Bytes9014 = "9014 Bytů"
Disabled = "Vypnuto"
Enabled = "Zapnuto"
RXEna = "Rx zapnuto"
TXEna = "Tx zapnuto"
TXRXEna = "Tx a Rx zapnuto"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Danish
[Strings.0406]
Marvell = "Marvell"
FlowControl = "Flowstyring"
InterruptModeration = "Afbrydelsesmoderering"
IPChecksumOffloadIPv4 = "IPv4 kontrolsum aflastning"
JumboPacket = "Jumbopakke"
LsoV2IPv4 = "Stor forsend. aflast. V2(IPv4)"
LsoV2IPv6 = "Stor forsend. aflast. V2(IPv6)"
ReceiveBuffers = "Modtagebuffere"
SpeedDuplex = "Hastighed & Duplex"
TCPChecksumOffloadIPv4 = "TCP kontrols.aflast.(IPv4)"
TCPChecksumOffloadIPv6 = "TCP kontrols.aflast.(IPv6)"
UDPChecksumOffloadIPv4 = "UDP kontrols.aflast.(IPv4)"
UDPChecksumOffloadIPv6 = "UDP kontrols.aflast.(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Netværksadresse"
10MFD = "10 Mbps fuld dupleks"
10MHD = "10 Mbps halv dupleks"
100MFD = "100 Mbps fuld dupleks"
100MHD = "100 Mbps halv dupleks"
1000MFD = "1,0 Gbps fuld dupleks"
Autosense = "Auto-forhandling"
Bytes1514 = "1514 Byte"
Bytes4088 = "4088 Byte"
Bytes9014 = "9014 Byte"
Disabled = "Deaktiveret"
Enabled = "Aktiveret"
RXEna = "Rx aktiveret"
TXEna = "Tx aktiveret"
TXRXEna = "Tx & Rx aktiveret"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; German (Standard)
[Strings.0407]
Marvell = "Marvell"
FlowControl = "Datenflusskontrolle"
InterruptModeration = "Interrupt-Moderation"
IPChecksumOffloadIPv4 = "Verlagerung IPv4-Prüfsumme"
JumboPacket = "Jumbo-Paket"
LsoV2IPv4 = "Übernahme TCP-Segment. V2 (IPv4)"
LsoV2IPv6 = "Übernahme TCP-Segment. V2 (IPv6)"
ReceiveBuffers = "Empfangspuffer"
SpeedDuplex = "Geschwindigkeit und Duplexmodus"
TCPChecksumOffloadIPv4 = "Verlagerung TCP-Prüfsumme (IPv4)"
TCPChecksumOffloadIPv6 = "Verlagerung TCP-Prüfsumme (IPv6)"
UDPChecksumOffloadIPv4 = "Verlagerung UDP-Prüfsumme (IPv4)"
UDPChecksumOffloadIPv6 = "Verlagerung UDP-Prüfsumme (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Netzwerkadresse"
10MFD = "10 Mbit/s Vollduplex"
10MHD = "10 MBit/s Halbduplex"
100MFD = "100 MBit/s Vollduplex"
100MHD = "100 MBit/s Halbduplex"
1000MFD = "1 GBit/s Vollduplex"
Autosense = "Automatische Erkennung"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
Disabled = "Deaktiviert"
Enabled = "Aktiviert"
RXEna = "Rx aktiviert"
TXEna = "Tx aktiviert"
TXRXEna = "Tx & Rx aktiviert"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Greek
[Strings.0408]
Marvell = "Marvell"
FlowControl = "Έλεγχος ροής"
InterruptModeration = "Μετρίαση διακοπών"
IPChecksumOffloadIPv4 = "IPv4 άθρ.ελέγχου εκτός φορτ."
JumboPacket = "Μεγάλο πακέτο"
LsoV2IPv4 = "Μεγ.αποστ. εκτός φορτ.V2(IPv4)"
LsoV2IPv6 = "Μεγ.αποστ. εκτός φορτ.V2(IPv6)"
ReceiveBuffers = "Προσωρινές μνήμες λήψης"
SpeedDuplex = "Ταχύτητα & Αμφίδρομα"
TCPChecksumOffloadIPv4 = "TCP άθρ.ελέγ.εκτός φορτ.(IPv4)"
TCPChecksumOffloadIPv6 = "TCP άθρ.ελέγ.εκτός φορτ.(IPv6)"
UDPChecksumOffloadIPv4 = "UDP άθρ.ελέγ.εκτός φορτ.(IPv4)"
UDPChecksumOffloadIPv6 = "UDP άθρ.ελέγ.εκτός φορτ.(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Διεύθυνση δικτύου"
10MFD = "10 Mbps Πλήρως αμφίδρομο"
10MHD = "10 Mbps Ημι-αμφίδρομo"
100MFD = "100 Mbps Πλήρως αμφίδρομο"
100MHD = "100 Mbps Ημι-αμφίδρομo"
1000MFD = "1.0 Gbps Πλήρως αμφίδρομο"
Autosense = "Αυτόματη ανίχνευση"
Bytes1514 = "1514 διφιοσυλλαβές"
Bytes4088 = "4088 διφιοσυλλαβές"
Bytes9014 = "9014 διφιοσυλλαβές"
Disabled = "Απενεργοποιημένο"
Enabled = "Ενεργοποιημένο"
RXEna = "Λήψη ενεργός"
TXEna = "Αποστολή ενεργός"
TXRXEna = "Αποστολή & Λήψη ενεργός"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Spanish (Spain, Traditional Sort)
[Strings.040A]
Marvell = "Marvell"
FlowControl = "Control de flujo"
InterruptModeration = "Moderación de interrupción"
IPChecksumOffloadIPv4 = "Desc. suma comp.IPv4"
JumboPacket = "Paquete Jumbo"
LsoV2IPv4 = "Desc. envío grande V2(IPv4)"
LsoV2IPv6 = "Desc. envío grande V2(IPv6)"
ReceiveBuffers = "Búferes de recepción"
SpeedDuplex = "Velocidad y dúplex del enlace"
TCPChecksumOffloadIPv4 = "Desc. suma comp. TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Desc. suma comp. TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Desc. suma comp. UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Desc. suma comp. UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Dirección de red"
10MFD = "10 Mbps dúplex completo"
10MHD = "10 Mbps dúplex medio"
100MFD = "100 Mbps dúplex completo"
100MHD = "100 Mbps dúplex medio"
1000MFD = "1,0 Gbps dúplex completo"
Autosense = "Orientación automática"
Bytes1514 = "1514 bytes"
Bytes4088 = "4088 bytes"
Bytes9014 = "9014 bytes"
Disabled = "Desactivado"
Enabled = "Activado"
RXEna = "Rx activado"
TXEna = "Tx activado"
TXRXEna = "Tx y Rx activados"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Finnish
[Strings.040B]
Marvell = "Marvell"
FlowControl = "Vuonohjaus"
InterruptModeration = "Keskeytä moderaatio"
IPChecksumOffloadIPv4 = "IPv4 tarkistussumma purkaus"
JumboPacket = "Jumbo-paketti"
LsoV2IPv4 = "Sanomien lohkom. purk. V2(IPv4)"
LsoV2IPv6 = "Sanomien lohkom. purk. V2(IPv6)"
ReceiveBuffers = "Puskureiden vastaanotto"
SpeedDuplex = "Nopeus & kaksisuuntainen"
TCPChecksumOffloadIPv4 = "TCP tark.summa purk. (IPv4)"
TCPChecksumOffloadIPv6 = "TCP tark.summa purk. (IPv6)"
UDPChecksumOffloadIPv4 = "UDP tark.summa purk. (IPv4)"
UDPChecksumOffloadIPv6 = "UDP tark.summa purk. (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Verkko-osoite"
10MFD = "10 Mbps kaksisuuntainen"
10MHD = "10 Mbps yksisuuntainen"
100MFD = "100 Mbps kaksisuuntainen"
100MHD = "100 Mbps yksisuuntainen"
1000MFD = "1,0 Gbps kaksisuuntainen"
Autosense = "Autom. neuvottelu"
Bytes1514 = "1514 tavua"
Bytes4088 = "4088 tavua"
Bytes9014 = "9014 tavua"
Disabled = "Pois käytöstä"
Enabled = "Käytössä"
RXEna = "Vastaanotto otettu käyttöön"
TXEna = "Lähetys otettu käyttöön"
TXRXEna = "Läh. ja vast.otto käyt."

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; French (Standard)
[Strings.040C]
Marvell = "Marvell"
FlowControl = "Contrôle de flux"	
InterruptModeration = "Modération de l'interruption"
IPChecksumOffloadIPv4 = "DéchargTotal de contrôle IPv4"
JumboPacket = "Paquet géant"
LsoV2IPv4 = "DéchargeEnvoiImport.V2 (IPv4)"
LsoV2IPv6 = "DéchargeEnvoiImport.V2 (IPv6)"
ReceiveBuffers = "Tampons de réception"
SpeedDuplex = "Vitesse de liaison et duplex"
TCPChecksumOffloadIPv4 = "DéchargTotalContr. TCP(IPv4)"
TCPChecksumOffloadIPv6 = "DéchargTotalContr. TCP(IPv6)"
UDPChecksumOffloadIPv4 = "DéchargTotalContr. UDP(IPv4)"
UDPChecksumOffloadIPv6 = "DéchargTotalContr. UDP(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Adresse réseau"
10MFD = "10 Mbits/s duplex intégral"
10MHD = "10 Mbits/s semi-duplex"
100MFD = "100 Mbits/s duplex intégral"
100MHD = "100 Mbits/s semi-duplex"
1000MFD = "1,0 Gbits/s duplex intégral"
Autosense = "Détection automatique"
Bytes1514 = "1514 octets"
Bytes4088 = "4088 octets"
Bytes9014 = "9014 octets"
Disabled = "Désactivé(e)"
Enabled = "Activé(e)"
RXEna = "Rx activée"
TXEna = "Tx activée"
TXRXEna = "Tx & Rx activées"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Hebrew
[Strings.040D]
Marvell = "Marvell"
FlowControl = "בקרת זרימה"
InterruptModeration = "ניהול Interrupt"
IPChecksumOffloadIPv4 = "IPv4 Checksum Offload"
JumboPacket = "חבילת מידע ענקית"
LsoV2IPv4 = "Send Offload V2(IPv4) גדול"
LsoV2IPv6 = "Send Offload V2(IPv6) גדול"
ReceiveBuffers = "באפרים קליטה"
SpeedDuplex = "מהירות ודופלקס"
TCPChecksumOffloadIPv4 = "TCP Checksum Offload (IPv4)"
TCPChecksumOffloadIPv6 = "TCP Checksum Offload (IPv6)"
UDPChecksumOffloadIPv4 = "UDP Checksum Offload (IPv4)"
UDPChecksumOffloadIPv6 = "UDP Checksum Offload (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "כתובת רשת"
10MFD = "10 Mbps דו-סטרי מלא"
10MHD = "10 Mbps דו-סטרי למחצה"
100MFD = "100 Mbps דו-סטרי מלא"
100MHD = "100 Mbps דו-סטרי למחצה"
1000MFD = "‎1.0 Gbps דו-סטרי מלא"
Autosense = "משא ומתן אוטומטי"
Bytes1514 = "בתים 1514"
Bytes4088 = "בתים 4088"
Bytes9014 = "בתים 9014"
Disabled = "מנוטרל"
Enabled = "מאופשר"
RXEna = "קליטה מאופשרת"
TXEna = "שידור מאופשר"
TXRXEna = "קליטה ושידור מאופשרים"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Hungarian
[Strings.040E]
Marvell = "Marvell"
FlowControl = "Forgalomvezérlés"
InterruptModeration = "Megszakításmérséklés"
IPChecksumOffloadIPv4 = "IPv4 ell.ö. előfeld"
JumboPacket = "Jumbo csomag"
LsoV2IPv4 = "Nagycsom. előf. V2(IPv4)"
LsoV2IPv6 = "Nagycsom. előf. V2(IPv6)"
ReceiveBuffers = "Vevőpufferek"
SpeedDuplex = "Sebesség és duplexitás"
TCPChecksumOffloadIPv4 = "TCP ell.ö. előfeld (IPv4)"
TCPChecksumOffloadIPv6 = "TCP ell.ö. előfeld (IPv6)"
UDPChecksumOffloadIPv4 = "UDP ell.ö. előfeld (IPv4)"
UDPChecksumOffloadIPv6 = "UDP ell.ö. előfeld (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Hálózati cím"
10MFD = "10 Mbps teljes kétirányú"
10MHD = "10 Mbps váltakozó kétirányú"
100MFD = "100 Mbps teljes kétirányú"
100MHD = "100 Mbps váltakozó kétirányú"
1000MFD = "1,0 Gb/s teljes kétirányú"
Autosense = "Auto-negotiation"
Bytes1514 = "1514 bájt"
Bytes4088 = "4088 bájt"
Bytes9014 = "9014 bájt"
Disabled = "Letiltva"
Enabled = "Engedélyezve"
RXEna = "Rx engedélyezve"
TXEna = "Tx engedélyezve"
TXRXEna = "Tx, Rx engedélyezve"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Italian (Standard)
[Strings.0410]
Marvell = "Marvell"
FlowControl = "Controllo del flusso"
InterruptModeration = "Moderazione interrupt"
IPChecksumOffloadIPv4 = "Checksum Offload IPv4"
JumboPacket = "Pacchetto jumbo"
LsoV2IPv4 = "Large Send Offload V2(IPv4)"
LsoV2IPv6 = "Large Send Offload V2(IPv6)"
ReceiveBuffers = "Buffer di ricezione"
SpeedDuplex = "Velocità di collegamento e duplex"
TCPChecksumOffloadIPv4 = "Checksum Offload TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Checksum Offload TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Checksum Offload UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Checksum Offload UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Indirizzo di rete"
10MFD = "10 Mbps Full Duplex"
10MHD = "10 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
1000MFD = "1.0 Gbps Full Duplex"
Autosense = "Autoriconoscimento"
Bytes1514 = "1514 byte"
Bytes4088 = "4088 byte"
Bytes9014 = "9014 byte"
Disabled = "Disattivato"
Enabled = "Attivato"
RXEna = "Rx abilitato"
TXEna = "Tx abilitato"
TXRXEna = "Tx & Rx abilitati"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Japanese
[Strings.0411]
Marvell = "Marvell"
FlowControl = "フロー制御"
InterruptModeration = "割り込み節度"
IPChecksumOffloadIPv4 = "IPv4チェックサム オフロード"
JumboPacket = "ジャンボ パケット"
LsoV2IPv4 = "大容量送信オフロード V2(IPv4)"
LsoV2IPv6 = "大容量送信オフロード V2(IPv6)"
ReceiveBuffers = "受信バッファ"
SpeedDuplex = "リンク速度とデュプレックス"
TCPChecksumOffloadIPv4 = "TCPチェックサム オフロード(IPv4)"
TCPChecksumOffloadIPv6 = "TCPチェックサム オフロード(IPv6)"
UDPChecksumOffloadIPv4 = "UDPチェックサム オフロード(IPv4)"
UDPChecksumOffloadIPv6 = "UDPチェックサム オフロード(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "ネットワークアドレス"
10MFD = "10 Mbps Full Duplex"
10MHD = "10 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
1000MFD = "1.0 Gbps Full Duplex"
Autosense = "自動感知"
Bytes1514 = "1514 バイト"
Bytes4088 = "4088 バイト"
Bytes9014 = "9014 バイト"
Disabled = "オフ"
Enabled = "オン"
RXEna = "Rx 有効"
TXEna = "Tx 有効"
TXRXEna = "Tx & Rx 有効"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Korean
[Strings.0412]
Marvell = "Marvell"
FlowControl = "흐름 제어"
InterruptModeration = "인터럽트 완화"
IPChecksumOffloadIPv4 = "IPv4 검사합계 오프로드"
JumboPacket = "점보 패킷"
LsoV2IPv4 = "대량송신오프로드V2(IPv4)"
LsoV2IPv6 = "대량송신오프로드V2(IPv6)"
ReceiveBuffers = "수신 버퍼"
SpeedDuplex = "링크 속도 및 이중성"
TCPChecksumOffloadIPv4 = "TCP검사합계오프로드(IPv4)"
TCPChecksumOffloadIPv6 = "TCP검사합계오프로드(IPv6)"
UDPChecksumOffloadIPv4 = "UDP검사합계오프로드(IPv4)"
UDPChecksumOffloadIPv6 = "UDP검사합계오프로드(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "네트워크 주소"
10MFD = "10 Mbps 전이중"
10MHD = "10 Mbps 반이중"
100MFD = "100 Mbps 전이중"
100MHD = "100 Mbps 반이중"
1000MFD = "1.0 Gbps 전이중"
Autosense = "자동 감지"
Bytes1514 = "1514 바이트"
Bytes4088 = "4088 바이트"
Bytes9014 = "9014 바이트"
Disabled = "활성 해제됨"
Enabled = "활성화됨"
RXEna = "Rx 사용"
TXEna = "Tx 사용"
TXRXEna = "Tx & Rx 사용"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Dutch (Netherlands)
[Strings.0413]
Marvell = "Marvell"
FlowControl = "Flow-controle"
InterruptModeration = "Onderbrekingsremming"
IPChecksumOffloadIPv4 = "IPv4-controlesom-offload"
JumboPacket = "Jumbopakket"
LsoV2IPv4 = "Grote zendings-offload V2(IPv4)"
LsoV2IPv6 = "Grote zendings-offload V2(IPv6)"
ReceiveBuffers = "Ontvangstbuffers"
SpeedDuplex = "Snelheid & duplex"
TCPChecksumOffloadIPv4 = "TCP-controlesom-offload (IPv4)"
TCPChecksumOffloadIPv6 = "TCP-controlesom-offload (IPv6)"
UDPChecksumOffloadIPv4 = "UDP-controlesom-offload (IPv4)"
UDPChecksumOffloadIPv6 = "UDP-controlesom-offload (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Netwerkadres"
10MFD = "10 Mbps full duplex"
10MHD = "10 Mbps half duplex"
100MFD = "100 Mbps full duplex"
100MHD = "100 Mbps half duplex"
1000MFD = "1 Gbps full duplex"
Autosense = "Auto-sense"
Bytes1514 = "1514 bytes"
Bytes4088 = "4088 bytes"
Bytes9014 = "9014 bytes"
Disabled = "Uitgeschakeld"
Enabled = "Ingeschakeld"
RXEna = "Rx ingeschakeld"
TXEna = "Tx ingeschakeld"
TXRXEna = "Tx & Rx ingeschakeld"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Norwegian (Bokmal)
[Strings.0414]
Marvell = "Marvell"
FlowControl = "Flytkontroll"
InterruptModeration = "Avbrudd moderasjon"
IPChecksumOffloadIPv4 = "IPv4 Kontrollsum offload"
JumboPacket = "Jumbopakke"
LsoV2IPv4 = "Stor send offload V2(IPv4)"
LsoV2IPv6 = "Stor send offload V2(IPv6)"
ReceiveBuffers = "Mottaksbuffer"
SpeedDuplex = "Hastighet & dupleks"
TCPChecksumOffloadIPv4 = "TCP Kontrollsum offl.(IPv4)"
TCPChecksumOffloadIPv6 = "TCP Kontrollsum offl.(IPv6)"
UDPChecksumOffloadIPv4 = "UDP Kontrollsum offl.(IPv4)"
UDPChecksumOffloadIPv6 = "UDP Kontrollsum offl.(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Nettverkadresse"
10MFD = "10 Mbps full dupleks"
10MHD = "10 Mbps halv dupleks"
100MFD = "100 Mbps full dupleks"
100MHD = "100 Mbps halv dupleks"
1000MFD = "1 Gbps full dupleks"
Autosense = "Auto forhandling"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
Disabled = "Deaktivert"
Enabled = "Aktivert"
RXEna = "Rx aktivert"
TXEna = "Tx aktivert"
TXRXEna = "Tx & Rx aktivert"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Polish
[Strings.0415]
Marvell = "Marvell"
FlowControl = "Kontrola przepływu danych"
InterruptModeration = "Moderacja przerwania"
IPChecksumOffloadIPv4 = "IPv4 ob. sumy kon."
JumboPacket = "Pakiet Jumbo"
LsoV2IPv4 = "Obs. wys. du. il da. V2(IPv4)"
LsoV2IPv6 = "Obs. wys. du. il da. V2(IPv6)"
ReceiveBuffers = "Bufory odbiorcze"
SpeedDuplex = "Szybkość i Dupleks"
TCPChecksumOffloadIPv4 = "Ob. sumy kon. pak. TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Ob. sumy kon. pak. TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Ob. sumy kon. pak. UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Ob. sumy kon. pak. UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Adres sieciowy"
10MFD = "10 Mb/s pełny dupleks"
10MHD = "10 Mb/s półdupleks"
100MFD = "100 Mb/s pełny dupleks"
100MHD = "100 Mb/s półdupleks"
1000MFD = "1 Gb/s pełny dupleks"
Autosense = "Automatyczne wykrywanie"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
Disabled = "Wyłączony"
Enabled = "Włączony"
RXEna = "Bufory odbiorcze wł."
TXEna = "Bufory nadawcze wł."
TXRXEna = "Bufory nad. i odb. wł."

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Portuguese (Brazil)
[Strings.0416]
Marvell = "Marvell"
FlowControl = "Controle de Fluxo"
InterruptModeration = "Moderação de Interrupção"
IPChecksumOffloadIPv4 = "Descarga Soma de Verif. IPv4"
JumboPacket = "Pacote Jumbo"
LsoV2IPv4 = "Grande Desc. Envio V2(IPv4)"
LsoV2IPv6 = "Grande Desc. Envio V2(IPv6)"
ReceiveBuffers = "Buffers de Recepção"
SpeedDuplex = "Velocidade de Link e Duplex"
TCPChecksumOffloadIPv4 = "Desc. Soma Verif. TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Desc. Soma Verif. TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Desc. Soma Verif. UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Desc. Soma Verif. UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Endereço da Rede"
10MFD = "10 Mbps Full Duplex"
10MHD = "10 Mbps Half Duplex"
100MFD = "100 Mbps Full Duplex"
100MHD = "100 Mbps Half Duplex"
1000MFD = "1.0 Gbps Full Duplex"
Autosense = "Autodetecção"
Bytes1514 = "1514 Bytes"
Bytes4088 = "4088 Bytes"
Bytes9014 = "9014 Bytes"
Disabled = "Desativado"
Enabled = "Ativado"
RXEna = "Rx habilitado"
TXEna = "Tx habilitado"
TXRXEna = "Tx & Rx habilitado"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Romanian
[Strings.0418]
Marvell = "Marvell"
FlowControl = "Control al fluxului"
InterruptModeration = "Moderare întrerupere"
IPChecksumOffloadIPv4 = "Verificare transfer IPv4"
JumboPacket = "Cadre Jumbo"
LsoV2IPv4 = "Transfer mare date V2(IPv4)"
LsoV2IPv6 = "Transfer mare date V2(IPv6)"
ReceiveBuffers = "Buffer recepţie"
SpeedDuplex = "Viteză şi Duplex"
TCPChecksumOffloadIPv4 = "TCP Verif. transfer (IPv4)"
TCPChecksumOffloadIPv6 = "TCP Verif. transfer (IPv6)"
UDPChecksumOffloadIPv4 = "UDP Verif. transfer (IPv4)"
UDPChecksumOffloadIPv6 = "UDP Verif. transfer (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Adresă reţea"
10MFD = "10 Mbps Duplex integral"
10MHD = "10 Mbps semiduplex"
100MFD = "100 Mbps Duplex integral"
100MHD = "100 Mbps semiduplex"
1000MFD = "1 Gbps Duplex integral"
Autosense = "Auto-negociere"
Bytes1514 = "1514 octeţi"
Bytes4088 = "4088 octeţi"
Bytes9014 = "9014 octeţi"
Disabled = "Dezactivat"
Enabled = "Activat"
RXEna = "Rx activat"
TXEna = "Tx activat"
TXRXEna = "Tx şi Rx activat"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Russian
[Strings.0419]
Marvell = "Marvell"
FlowControl = "Управление потоком данных"
InterruptModeration = "Управление прерываниями"
IPChecksumOffloadIPv4 = "Разг.контр.сумм IPv4"
JumboPacket = "Большой пакет"
LsoV2IPv4 = "Разг.больш.передач V2(IPv4)"
LsoV2IPv6 = "Разг.больш.передач V2(IPv6)"
ReceiveBuffers = "Буферы приема"
SpeedDuplex = "Скорость и дуплекс"
TCPChecksumOffloadIPv4 = "Разг.контр.сумм TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Разг.контр.сумм TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Разг.контр.сумм UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Разг.контр.сумм UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Сетевой адрес"
10MFD = "10 Мбит/с полный дуплекс"
10MHD = "10 Мбит/с полудуплекс"
100MFD = "100 Мбит/с полный дуплекс"
100MHD = "100 Мбит/с полудуплекс"
1000MFD = "1,0 Гбит/с полный дуплекс"
Autosense = "Автоопределение"
Bytes1514 = "1514 байт"
Bytes4088 = "4088 байт"
Bytes9014 = "9014 байт"
Disabled = "Отключать"
Enabled = "Включать"
RXEna = "Rx включен"
TXEna = "Tx включен"
TXRXEna = "Tx & Rx включен"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Croatian
[Strings.041A]
Marvell = "Marvell"
FlowControl = "Kontrola protoka"
InterruptModeration = "Moderacija prekida"
IPChecksumOffloadIPv4 = "IPv4 Kon. zbroj bez opt."
JumboPacket = "Jumbo okvir"
LsoV2IPv4 = "V. rastereć. slanja V2(IPv4)"
LsoV2IPv6 = "V. rastereć. slanja V2(IPv6)"
ReceiveBuffers = "Spremnici prijema"
SpeedDuplex = "Brzina i dupleks"
TCPChecksumOffloadIPv4 = "TCP Kontrl. zbr. na p. (IPv4)"
TCPChecksumOffloadIPv6 = "TCP Kontrl. zbr. na p. (IPv6)"
UDPChecksumOffloadIPv4 = "UDP Kontrl. zbr. na p.(IPv4)"
UDPChecksumOffloadIPv6 = "UDP Kontrl. zbr. na p. (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Mrežna adresa"
10MFD = "10 Mbp/s puni dupleks"
10MHD = "10 Mbp/s poludupleksan"
100MFD = "100 Mbp/s puni dupleks"
100MHD = "100 Mbp/s poludupleksan"
1000MFD = "1 Gbp/s puni dupleks"
Autosense = "Automatski pregovori"
Bytes1514 = "1514 bajtova"
Bytes4088 = "4088 bajtova"
Bytes9014 = "9014 bajtova"
Disabled = "Onemogućeno"
Enabled = "Omogućeno"
RXEna = "Rx omogućeno"
TXEna = "Tx omogućeno"
TXRXEna = "Tx & Rx omogućeno"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Slovak
[Strings.041B]
Marvell = "Marvell"
FlowControl = "Kontrola toku"
InterruptModeration = "Zmiernenie prerušenia"
IPChecksumOffloadIPv4 = "Kontr. súč. vyl. IPv4"
JumboPacket = "Jumbo balík"
LsoV2IPv4 = "Vyl.veľk.odosl. V2(IPv4)"
LsoV2IPv6 = "Vyl.veľk.odosl. V2(IPv6)"
ReceiveBuffers = "Zásobníky príjmu"
SpeedDuplex = "Rýchlosť a duplex"
TCPChecksumOffloadIPv4 = "Kont.súč.vyl.TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Kont.súč.vyl.TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Kont.súč.vyl.UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Kont.súč.vyl.UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Sieťová adresa"
10MFD = "10 Mb/s plný duplex"
10MHD = "10 Mb/s polovičný duplex"
100MFD = "100 Mb/s plný duplex"
100MHD = "100 Mb/s polovičný duplex"
1000MFD = "1 Gb/s plný duplex"
Autosense = "Automatická negociácia"
Bytes1514 = "1514 Byteov"
Bytes4088 = "4088 Byteov"
Bytes9014 = "9014 Byteov"
Disabled = "Vypnuté"
Enabled = "Zapnuté"
RXEna = "Rx zapnuté"
TXEna = "Tx zapnuté"
TXRXEna = "Tx a Rx zapnuté"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Swedish
[Strings.041D]
Marvell = "Marvell"
FlowControl = "Flödeskontroll"
InterruptModeration = "Funktion för avbrottsbegränsning"
IPChecksumOffloadIPv4 = "IPv4 överföring av checks."
JumboPacket = "Jumbopaket"
LsoV2IPv4 = "Stor överföring V2(IPv4)"
LsoV2IPv6 = "Stor överföring V2(IPv6)"
ReceiveBuffers = "Mottagningsbuffert"
SpeedDuplex = "Hastighet & duplex"
TCPChecksumOffloadIPv4 = "TCP överför. checks.(IPv4)"
TCPChecksumOffloadIPv6 = "TCP överför. checks.(IPv6)"
UDPChecksumOffloadIPv4 = "UDP överför. checks.(IPv4)"
UDPChecksumOffloadIPv6 = "UDP överför. checks.(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Nätverksadress"
10MFD = "10 Mbit/s full duplex"
10MHD = "10 Mbit/s halv duplex"
100MFD = "100 Mbit/s full duplex"
100MHD = "100 Mbit/s halv duplex"
1000MFD = "1 Gbit/s full duplex"
Autosense = "Automatisk förhandling"
Bytes1514 = "1514 bytes"
Bytes4088 = "4088 bytes"
Bytes9014 = "9014 bytes"
Disabled = "Inaktiverad"
Enabled = "Aktiverad"
RXEna = "Rx aktiverat"
TXEna = "Tx aktiverat"
TXRXEna = "Tx & Rx aktiverade"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Turkish
[Strings.041F]
Marvell = "Marvell"
FlowControl = "Akış Kontrol"
InterruptModeration = "Kesme Ölçüsü"
IPChecksumOffloadIPv4 = "IPv4 Top.Sağl.Yüklü Değil"
JumboPacket = "Jumbo Paket"
LsoV2IPv4 = "Büy.Gönd.YüklüDeğil V2(IPv4)"
LsoV2IPv6 = "Büy.Gönd.YüklüDeğil V2(IPv6)"
ReceiveBuffers = "Alış Arabelleği"
SpeedDuplex = "Hızlı ve Çift Yönlü"
TCPChecksumOffloadIPv4 = "TCP Top.Sağl.YüklüDeğil(IPv4)"
TCPChecksumOffloadIPv6 = "TCP Top.Sağl.YüklüDeğil(IPv6)"
UDPChecksumOffloadIPv4 = "UDP Top.Sağl.YüklüDeğil(IPv4)"
UDPChecksumOffloadIPv6 = "UDP Top.Sağl.YüklüDeğil(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Ağ Adresi"
10MFD = "10 Mb/sn Tam Çift Yönlü"
10MHD = "10 Mb/sn Yarım Çift Yönlü"
100MFD = "100 Mb/sn Tam Çift Yönlü"
100MHD = "100 Mb/sn Yarım Çift Yönlü"
1000MFD = "1,0 Gb/sn Tam Çift Yönlü"
Autosense = "Otomatik Anlaşma"
Bytes1514 = "1514 Bayt"
Bytes4088 = "4088 Bayt"
Bytes9014 = "9014 Bayt"
Disabled = "Devre dışı"
Enabled = "Devrede"
RXEna = "Rx Devrede"
TXEna = "Tx Devrede"
TXRXEna = "Tx & Rx Devrede"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Slovenian
[Strings.0424]
Marvell = "Marvell"
FlowControl = "Krmiljenje pretoka"
InterruptModeration = "Združevanje prekinitev"
IPChecksumOffloadIPv4 = "Prelaganje kont. vsote IPv4"
JumboPacket = "Jumbo paket"
LsoV2IPv4 = "Prelag. pri vel. poš. V2(IPv4)"
LsoV2IPv6 = "Prelag. pri vel. poš. V2(IPv6)"
ReceiveBuffers = "Sprejemni medpomnilniki"
SpeedDuplex = "Hitrost in dupleks"
TCPChecksumOffloadIPv4 = "Prelag. kont. vsote TCP (IPv4)"
TCPChecksumOffloadIPv6 = "Prelag. kont. vsote TCP (IPv6)"
UDPChecksumOffloadIPv4 = "Prelag. kont. vsote UDP (IPv4)"
UDPChecksumOffloadIPv6 = "Prelag. kont. vsote UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Omrežni naslov"
10MFD = "10 Mbps polni dupleks"
10MHD = "10 Mbps polovični dupleks"
100MFD = "100 Mbps polni dupleks"
100MHD = "100 Mbps polovični dupleks"
1000MFD = "1 Gbps polni dupleks"
Autosense = "Samodejno pogajanje"
Bytes1514 = "1514 bajtov"
Bytes4088 = "4088 bajtov"
Bytes9014 = "9014 bajtov"
Disabled = "Onemogočeno"
Enabled = "Omogočeno"
RXEna = "Rx omogočeno"
TXEna = "Tx omogočeno"
TXRXEna = "Tx in Rx omogočeno"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Lithuanian
[Strings.0427]
Marvell = "Marvell"
FlowControl = "Srauto kontrolė"
InterruptModeration = "Pertraukių mažinimas"
IPChecksumOffloadIPv4 = "IPv4 dublių patikros užkrovimas"
JumboPacket = "Maksimalus paketas"
LsoV2IPv4 = "Didelio siunt. užkrov. V2(IPv4)"
LsoV2IPv6 = "Didelio siunt. užkrov. V2(IPv6)"
ReceiveBuffers = "Buferio gavimas"
SpeedDuplex = "Greitis ir dvipusiškumas"
TCPChecksumOffloadIPv4 = "TCP dublių pat. užkrov. (IPv4)"
TCPChecksumOffloadIPv6 = "TCP dublių pat. užkrov. (IPv6)"
UDPChecksumOffloadIPv4 = "UDP dublių pat. užkrov. (IPv4)"
UDPChecksumOffloadIPv6 = "UDP dublių pat. užkrov. (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "Tinklo adresas"
10MFD = "10 Mbps dvipusis"
10MHD = "10 Mbps pusiau dvipusis"
100MFD = "100 Mbps dvipusis"
100MHD = "100 Mbps pusiau dvipusis"
1000MFD = "1 Gbps dvipusis"
Autosense = "Automatinis perleidimas"
Bytes1514 = "1514 baitai"
Bytes4088 = "4088 baitai"
Bytes9014 = "9014 baitai"
Disabled = "Neleidžiama"
Enabled = "Leidžiama"
RXEna = "Rx leidžiama"
TXEna = "Tx leidžiama"
TXRXEna = "Tx ir Rx leidžiama"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Chinese (PRC)
[Strings.0804]
Marvell = "Marvell"
FlowControl = "流控制"
InterruptModeration = "中断模式"
IPChecksumOffloadIPv4 = "卸载 IPv4 校验和"
JumboPacket = "巨型包"
LsoV2IPv4 = "大量传送负载 V2(IPv4)"
LsoV2IPv6 = "大量传送负载 V2(IPv6)"
ReceiveBuffers = "接收缓冲区"
SpeedDuplex = "速度和双工"
TCPChecksumOffloadIPv4 = "卸载 TCP 校验和 (IPv4)"
TCPChecksumOffloadIPv6 = "卸载 TCP 校验和 (IPv6)"
UDPChecksumOffloadIPv4 = "卸载 UDP 校验和 (IPv4)"
UDPChecksumOffloadIPv6 = "卸载 UDP 校验和 (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "网络地址"
10MFD = "10 Mbps 全双工"
10MHD = "10 Mbps 半双工"
100MFD = "100 Mbps 全双工"
100MHD = "100 Mbps 半双工"
1000MFD = "1.0 Gbps 全双工"
Autosense = "自动感应"
Bytes1514 = "1514 个字节"
Bytes4088 = "4088 个字节"
Bytes9014 = "9014 个字节"
Disabled = "禁用"
Enabled = "启用"
RXEna = "启用 Rx"
TXEna = "启用 Tx"
TXRXEna = "启用Tx 和 Rx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Arabic (U.A.E.)
[Strings.3801]
Marvell = "Marvell"
FlowControl = "التحكم بالدفق"
InterruptModeration = "مقاطعة التوسيط"
IPChecksumOffloadIPv4 = "تحميل المجموع الاختباري لـIPv4"
JumboPacket = "حزمة كبيرة الحجم"
LsoV2IPv4 = "تحميل الإرسال الكبير V2(IPv4)"
LsoV2IPv6 = "تحميل الإرسال الكبير V2(IPv6)"
ReceiveBuffers = "المخازن المؤقتة للاستلام"
SpeedDuplex = "سريع ومزدوج"
TCPChecksumOffloadIPv4 = "تحميل المجموع الاخ. ل TCP(IPv4)"
TCPChecksumOffloadIPv6 = "تجاهل المجموعتحميل المجموع الاخ. ل TCP(IPv6)"
UDPChecksumOffloadIPv4 = "تحميل المجموع الاخ. ل UDP(IPv4)"
UDPChecksumOffloadIPv6 = "تحميل المجموع الاخ. ل UDP (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "عنوان الشبكة"
10MFD = "ازدواج كامل بسرعة 10 ميغا بت/ثانية"
10MHD = "أحادي الاتجاه بسرعة 10 ميغابت/ثانية"
100MFD = "ازدواج كامل بسرعة 100 ميغابت/ثانية"
100MHD = "أحادي الاتجاه بسرعة 100 ميغابت/ثانية"
1000MFD = "ازدواج كامل بسرعة 1.0 غيغابت/ثانية"
Autosense = "تفاوض تلقائي"
Bytes1514 = "1514 بايت"
Bytes4088 = "4088 بايت"
Bytes9014 = "9014 بايت"
Disabled = "معطَّل"
Enabled = "ممكَّن"
RXEna = "تمكين Rx"
TXEna = "تمكين Tx"
TXRXEna = "تمكين Tx وRx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Chinese (Hong Kong SAR, PRC)
[Strings.0C04]
Marvell = "Marvell"
FlowControl = "流控制"
InterruptModeration = "中斷模式"
IPChecksumOffloadIPv4 = "卸載IPv4校驗和"
JumboPacket = "巨型包"
LsoV2IPv4 = "大量傳送負載 V2(IPv4)"
LsoV2IPv6 = "大量傳送負載 V2(IPv6)"
ReceiveBuffers = "接收緩衝區"
SpeedDuplex = "速度和雙工"
TCPChecksumOffloadIPv4 = "卸載TCP校驗和(IPv4)"
TCPChecksumOffloadIPv6 = "卸載TCP校驗和(IPv6)"
UDPChecksumOffloadIPv4 = "卸載UDP校驗和(IPv4)"
UDPChecksumOffloadIPv6 = "卸載UDP校驗和(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "網路位址"
10MFD = "10 Mbps 全雙工"
10MHD = "10 Mbps 半雙工"
100MFD = "100 Mbps 全雙工"
100MHD = "100 Mbps 半雙工"
1000MFD = "1.0 Gbps 全雙工"
Autosense = "自動感應"
Bytes1514 = "1514 位元組"
Bytes4088 = "4088 位元組"
Bytes9014 = "9014 位元組"
Disabled = "禁用"
Enabled = "啟用"
RXEna = "啟用Rx"
TXEna = "啟用Tx"
TXRXEna = "啟用Tx和Rx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Chinese (Singapore)
[Strings.1004]
Marvell = "Marvell"
FlowControl = "流控制"
InterruptModeration = "中断模式"
IPChecksumOffloadIPv4 = "卸载 IPv4 校验和"
JumboPacket = "巨型包"
LsoV2IPv4 = "大量传送负载 V2(IPv4)"
LsoV2IPv6 = "大量传送负载 V2(IPv6)"
ReceiveBuffers = "接收缓冲区"
SpeedDuplex = "速度和双工"
TCPChecksumOffloadIPv4 = "卸载 TCP 校验和 (IPv4)"
TCPChecksumOffloadIPv6 = "卸载 TCP 校验和 (IPv6)"
UDPChecksumOffloadIPv4 = "卸载 UDP 校验和 (IPv4)"
UDPChecksumOffloadIPv6 = "卸载 UDP 校验和 (IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "网络地址"
10MFD = "10 Mbps 全双工"
10MHD = "10 Mbps 半双工"
100MFD = "100 Mbps 全双工"
100MHD = "100 Mbps 半双工"
1000MFD = "1.0 Gbps 全双工"
Autosense = "自动感应"
Bytes1514 = "1514 个字节"
Bytes4088 = "4088 个字节"
Bytes9014 = "9014 个字节"
Disabled = "禁用"
Enabled = "启用"
RXEna = "启用 Rx"
TXEna = "启用 Tx"
TXRXEna = "启用Tx 和 Rx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"

;------------------------------------------------------------------------------
; Chinese (Macau SAR)
[Strings.1404]
Marvell = "Marvell"
FlowControl = "流控制"
InterruptModeration = "中斷模式"
IPChecksumOffloadIPv4 = "卸載IPv4校驗和"
JumboPacket = "巨型包"
LsoV2IPv4 = "大量傳送負載 V2(IPv4)"
LsoV2IPv6 = "大量傳送負載 V2(IPv6)"
ReceiveBuffers = "接收緩衝區"
SpeedDuplex = "速度和雙工"
TCPChecksumOffloadIPv4 = "卸載TCP校驗和(IPv4)"
TCPChecksumOffloadIPv6 = "卸載TCP校驗和(IPv6)"
UDPChecksumOffloadIPv4 = "卸載UDP校驗和(IPv4)"
UDPChecksumOffloadIPv6 = "卸載UDP校驗和(IPv6)"
WakeOnMagicPacket="Wake on magic packet"
WakeOnPatternMatch="Wake on pattern match"
NetworkAddress = "網路位址"
10MFD = "10Mbps 全雙工"
10MHD = "10Mbps 半雙工"
100MFD = "100Mbps 全雙工"
100MHD = "100Mbps 半雙工"
1000MFD = "1.0 Gbps 全雙工"
Autosense = "自動感應"
Bytes1514 = "1514 位元組"
Bytes4088 = "4088 位元組"
Bytes9014 = "9014 位元組"
Disabled = "禁用"
Enabled = "啟用"
RXEna = "啟用Rx"
TXEna = "啟用Tx"
TXRXEna = "啟用Tx和Rx"

DriverDisk = "Marvell Yukon Ethernet Controller Installation Disk"
Yukon-Generic_1.DeviceDesc = "Marvell Yukon 88E8059 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_2.DeviceDesc = "Marvell Yukon 88E8075 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_3.DeviceDesc = "Marvell Yukon 88E8079 Family PCI-E Gigabit Ethernet Controller"
Yukon-Generic_4.DeviceDesc = "Marvell Yukon 88E8080 Family PCI-E Gigabit Ethernet Controller"
mvykxx.DriverDesc = "NDIS Miniport Driver for Marvell Yukon Ethernet Controller"
