; Copyright (c) 2009-2014  Intel Corporation  
; **********************************************************************************************  
; **********************************************************************************************  
; **    Filename:  iaAHCIB.inf 
; **    Revision:  DRIVER_INFO 
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver  
; **               Installs: RSTe AHCI Controller Miniport 
; **********************************************************************************************  
[Version]  
Signature="$Windows NT$"  
Provider=%INTEL%  
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}  
Class=SCSIAdapter  
CatalogFile=iaAHCIB.cat
DriverVer=05/21/2015,4.3.0.1198
; 
[PackageInfo]  
Name=AHCIB  
; 
[SourceDisksNames]  
1 = %DiskId1%,,,""  
[DestinationDirs]  
DefaultDestDir = 12  
; 
[ControlFlags]  
ExcludeFromSelect = *  
; 
[Manufacturer]  
%INTEL% = INTEL, NTamd64.6.1
; 
[iaStorB_Service_Inst] 
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorB.sys 
LoadOrderGroup = SCSI miniport  
AddReg         = pnpsafe_pci_addreg  
; 
[iaStorB_EventLog_Inst] 
AddReg = iaStorB_EventLog_AddReg 
; 
[iaStorB_EventLog_AddReg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorB.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
; 
[iaStorF_Service_Inst]  
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorF.sys  
; 
[iaStorF_EventLog_Inst]  
AddReg = iaStorF_EventLog_AddReg  
; 
[iaStorF_EventLog_AddReg]  
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll" 
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
;  
;********************************************************  
;*  
;* 64-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 64-bit architecture specific INF file entries  
;* required to install a driver as a 64-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.amd64]   
iaStorB.sys = 1,,,  
iaStorF.sys = 1,,,  
;  
[INTEL.NTamd64.6.1]
;Windows_7_x64 and later
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_8D62&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_1F32&CC_0106
;   
[iaStorB_inst.NTamd64] 
CopyFiles=@iaStorB.sys
CopyFiles=@iaStorF.sys   
; 
[iaStorB_inst.NTamd64.HW]
AddReg = iaStorF_addreg   
AddReg = msi_addreg 
AddReg = storport_addreg 
; 
[iaStorB_inst.NTamd64.Services] 
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst 
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst  
; 
[iaStorF_addreg]  
; Layer the RST Filter driver under all Disk class devices as a lower disk class filter  
; 
HKLM, System\CurrentControlSet\Control\Class\{4d36e967-e325-11ce-bfc1-08002be10318}, LowerFilters, 0x00010008, iaStorF  
; 
[pnpsafe_pci_addreg] 
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars  
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb 
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001  
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x0000000b 
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8) 
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001 
; 
[DefaultInstall]
OptionDesc = %ServiceDescription%
CopyINF = iaAHCIB.inf
;
[DefaultInstall.Services]
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst 
AddService = iaStorF, , iaStorF_Service_Inst, iaStorF_EventLog_Inst
;
[Strings]  
;  
; Localizable Strings  
;  
diskId1 = "RSTe AHCI Installation Disk"  
;server 
PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ series chipset sSATA AHCI Controller"
PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ series chipset sSATA AHCI Controller"
; 
INTEL = "Intel Corporation" 
ServiceDescription = "Intel(R) C600+/C220+ series chipset sSATA AHCI Controller"
; Non-Localizable Strings  
;  
SPSVCINST_ASSOCSERVICE = 0x00000002  
REG_MULTI_SZ           = 0x00010000  
REG_EXPAND_SZ          = 0x00020000  
REG_TYPE_DWORD         = 0x00010001  
SERVICE_KERNEL_DRIVER  = 1  
SERVICE_BOOT_START     = 0  
SERVICE_ERROR_NORMAL   = 1 
; 
; MSI enables.  
[msi_addreg]   
HKR, Interrupt Management, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1  
; 
[storport_addreg] 
;;; Enables/Disables Idle Power Management for StorPort 
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000001
;;; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255) 
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF 
;
