; AEC68x5.INF for Windows 2000/XP/2003
;
; Copyright (c) 2002, ACARD Technology Corp.
; For motherboard built-in only
;
[version]
CatalogFile=AEC68x5.cat
signature="$Windows NT$"
Class=SCSIAdapter
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Provider=%Acd%
;CatalogFile= aec68X5.CAT
DriverVer=04/09/2004, 1.0.5.5

; Class Install
[ClassInstall32.NT]
Addreg=SCSIReg

[SCSIReg]
HKR,,,,%SCSIClassName%
HKR,,Installer32,,"SysSetup.Dll,ScsiClassInstaller"
HKR,,Icon,,"-10"
HKR,,LegacyInfOption,,"SCSI"

[Manufacturer]
%AEC%=ACARD

[ACARD]
%AEC68x5.DeviceDesc%  = aec68x5_Inst,  PCI\VEN_1191&DEV_000A
%AEC68x5.Processor%= NO_DRV,ACARD___RAID_PROCESSOR__1

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS

[ControlFlags]

[SourceDisksFiles]
AEC68x5.sys=1


[SourceDisksNames]
1=%DisksNames%,,,,




[NO_DRV]
;Include=machine.inf
Needs=NO_DRV

[NO_DRV.Services]
Addservice= , %SPSVCINST_ASSOCSERVICE%  ;Null Service


[aec68x5_Inst]
CopyFiles = CopySYS
;Reboot

[CopySYS]
AEC68x5.sys

[aec68x5_Inst.Services]
AddService = aec68x5, %SPSVCINST_ASSOCSERVICE%, aec68x5_Service_Inst, Miniport_EventLog_Inst

[aec68x5_Service_Inst]
ServiceType    = %SERVICE_KERNEL_DRIVER%
StartType      = %SERVICE_BOOT_START%
ErrorControl   = %SERVICE_ERROR_NORMAL%
ServiceBinary  = %12%\aec68x5.sys
LoadOrderGroup = SCSI Miniport
AddReg	       = pnpsafe_pci_addreg

;*************************************************************
;These addreg sections should be used when installins services to indicate
;which interface types are safe for PNP and which aren't.  INTERFACE_TYPE
;is defined in NTDDK.H

[pnpsafe_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001

;*************************************************************
;The EventLog entries are the same for all SCSI miniports.
[Miniport_EventLog_Inst]
AddReg = Miniport_EventLog_AddReg

[Miniport_EventLog_AddReg]
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll"
HKR,,TypesSupported,%REG_DWORD%,7

[Strings]
Acd = "ACARD"
SCSIClassName="SCSI and RAID controllers"
AEC = "Acard"
aec68x5.DeviceDesc  = "ACARD AEC-6885/6895/6896 PCI 4 Channel RAID Controller"
AEC68X5.Processor   = "ACARD RAID PROCESSOR"
DisksNames = "ACARD AEC-6885/6895/6896 PCI 4 Channel RAID Driver Installation Diskette"
;*******************************************
;Handy macro substitutions (non-localizable)
SPSVCINST_ASSOCSERVICE = 0x00000002
SERVICE_KERNEL_DRIVER  = 1
SERVICE_BOOT_START     = 0
SERVICE_ERROR_NORMAL   = 1
REG_EXPAND_SZ	       = 0x00020000
REG_DWORD	       = 0x00010001

