						
						D-Link DSB-H4SMK Windows 2000 Drivers ¡V Installation Guide
						
						
  This document describes the installation of D-Link's Windows 2000 drivers for the USB to serial function
supported by D-Link's DSB-H4SMK USB Hub Controller. The guide consists of a driver summary, a guide to
installing the drivers with generic INF files and finally a guide to uninstalling the drivers.
Driver Summary

The USB <-> Serial Port drivers include the following modules

dlkbus.sys WDM driver for serial converter
dlser2k.sys WDM driver for serial communications
dlkbus.inf INF file supporting installation of USB to Serial converter
dlser2k.inf INF file supporting installation of Serial port


Installing the Drivers

  The following section describes the installation of D-Link's Windows 2000 followed by the installation of a
serial modem on the newly installed serial port.

  Where earlier versions of D-Link drivers have been loaded on the installation machine or where problems are
being encountered please uninstall D-Link's drivers using the Windows 2000 Add/Remove Hardware Wizard
in combination with D-Link's dlkun2k utility.

  D-Link's DLKUN2K utility should be used to uninstall the drivers in conjunction with Add/Remove
Hardware - it does not replace it. Uninstall the device using the Add/Remove Hardware, select Generic USB Hub
and remove it.
Then run DLKUN2K to complete the uninstallation.

 1. First copy driver and INF files onto a floppy.
 2. Please insert the D-Link DSB-H4SMK driver flopy diskette.
 3. This brings up the "Found New Hardware Wizard" , and select "Install the software automatically(Recommended)".
 4. After clicking "NEXT" , it will search the driver. 
 5. It will display two Description of the frame .
 6. Selecting the item which location is "a:\win2k&xp\dlkbus.inf" , and clicked "NEXT".
 7. When coping the driver , it will display a 'Hardware Installation' message , and clicked "Continue Anyway" .
 8. Select "Finish".
 9. This is then repeated with the "Found New Hardware Wizard" , and select "Install the software automatically(Recommended)". 
10 .After clicking "NEXT" , it will search the driver.
11. It will display two Description of the frame .
12. Selecting the item which location is "a:\win2k&xp\dlkport.inf" , and clicked "NEXT".
13. When coping the driver , it will display a 'Hardware Installation' message , and clicked "Continue Anyway" .
14. Finish.

This is then repeated with the Found New Hardware Wizard ¡¥Searching for Drivers' for the USB Serial Port.
Once this has completed successfully the installation can be checked as follows
My Computer -> Control Panel -> System -> Hardware -> Device Manager ¡V>View

First select to view by connection
Advanced Configuration and Power Interface (ACPI) BIOS -> Microsoft ACPI-Compliant System -> PCI Bus -> 
PCI to USB Host Controller -> USB Root Hub -> Generic USB Hub -> USB Serial Converter -> USB Serial Port (COMx)

Then select to view by type
Ports (COM & LPT) -> USB Serial Port (COMx)

Plug modem serial cable socket into USB to serial cable dongle. Select
My Computer -> Control Panel -> Phone and Modem

Select Add Modem ¡V and proceed to load Windows xp drivers for modem.

  If an .INF file is available for the modem of choice then Windows will complete plug and play interrogation
of the modem and configure it as required, otherwise the modem will be installed as a standard modem.
To test the modem
My Computer -> Control Panel -> Phone and Modem
select the modem of interest then
Properties -> Diagnostics -> Query Modem

  Alternatively connect to the internet through an ISP, remembering to change settings to use the newly
installed modem.

  

