;
; This is a Setup information file for monitors 
; supported in the Windows 95 retail product.
;
; Copyright (c) 1998, Hansol Electronics

[version]
signature="$CHICAGO$"
Class=Monitor
Provider=%Hansol%
ClassGUID={4D36E96E-E325-11CE-BFC1-08002BE10318}

;-------------------------------------------------
; Manufacturers
;-------------------------------------------------
[Manufacturer]
%Hansol%=Hansol

;-------------------------------------------------
; Driver sections
;-------------------------------------------------
[Hansol]
%Mazellan17px%=Mazellan17px, Monitor\HSL06A5
%Mazellan17ax%=Mazellan17ax, Monitor\HSL06A6
%Mazellan15ax%=Mazellan15ax, Monitor\HSL05DD
%Mazellan14px%=Mazellan14px, Monitor\HSL0579
%Mazellan14ax%=Mazellan14ax, Monitor\HSL057A

%Mazellan700P%=Mazellan700P, Monitor\HSL06A5
%Mazellan700A%=Mazellan700A, Monitor\HSL06A6
%Mazellan500P%=Mazellan500P, Monitor\HSL05DE
%Mazellan500A%=Mazellan500A, Monitor\HSL05DD
%Mazellan500M%=Mazellan500M, Monitor\HSL05DD
%Mazellan400P%=Mazellan400P, Monitor\HSL0579
%Mazellan400A%=Mazellan400A, Monitor\HSL057A

%Mazellan900P%=Mazellan900P, Monitor\HSL076D
%Mazellan701P%=Mazellan701P, Monitor\HSL06A8
%Mazellan701A%=Mazellan701A, Monitor\HSL06A7
%Mazellan501P%=Mazellan501P, Monitor\HSL05DF
%Mazellan_500A%=Mazellan_500A, Monitor\HSL05E0
%Mazellan_400P%=Mazellan_400P, Monitor\HSL057C
%Mazellan401A%=Mazellan401A, Monitor\HSL057B

%900P%=900P, Monitor\HSL076D
%701P%=701P, Monitor\HSL06A8
%701A%=701A, Monitor\HSL06A7
%501P%=501P, Monitor\HSL05DF
%500A%=500A, Monitor\HSL05E0
%400P%=400P, Monitor\HSL057C
%401A%=401A, Monitor\HSL057B

%Hansol400F%=Hansol400F.Install, Monitor\HSL0515
%400F%=400F.Install, Monitor\HSL012C
%500F%=500F.Install, Monitor\HSL01F4

%710P%=710P, Monitor\HSL06AB
%710A%=710A, Monitor\HSL06AA
%710Aplus%=710Aplus, Monitor\HSL06AA

;-------------------------------------------------
; Install sections
;-------------------------------------------------
[Mazellan17px]
DelReg=Del_Current_Reg
AddReg=Mazellan17px.Add, 1600, DPMS

[Mazellan17ax]
DelReg=Del_Current_Reg
AddReg=Mazellan17ax.Add, 1280, DPMS

[Mazellan15ax]
DelReg=Del_Current_Reg
AddReg=Mazellan15ax.Add, 1024, DPMS

[Mazellan14px]
DelReg=Del_Current_Reg
AddReg=Mazellan14px.Add, 1024, DPMS

[Mazellan14ax]
DelReg=Del_Current_Reg
AddReg=Mazellan14ax.Add, 1024, DPMS

[Mazellan700P]
DelReg=Del_Current_Reg
AddReg=Mazellan700P.Add, 1600, DPMS

[Mazellan700A]
DelReg=Del_Current_Reg
AddReg=Mazellan700A.Add, 1280, DPMS

[Mazellan701A]
DelReg=Del_Current_Reg
AddReg=Mazellan701A.Add, 1280, DPMS

[Mazellan501P]
DelReg=Del_Current_Reg
AddReg=Mazellan501P.Add, 1280, DPMS

[Mazellan500P]
DelReg=Del_Current_Reg
AddReg=Mazellan500P.Add, 1280, DPMS

[Mazellan500A]
DelReg=Del_Current_Reg
AddReg=Mazellan500A.Add, 1024, DPMS

[Mazellan500M]
DelReg=Del_Current_Reg
AddReg=Mazellan500M.Add, 1024, DPMS

[Mazellan400P]
DelReg=Del_Current_Reg
AddReg=Mazellan400P.Add, 1024, DPMS

[Mazellan400A]
DelReg=Del_Current_Reg
AddReg=Mazellan400A.Add, 1024, DPMS

[Mazellan401A]
DelReg=Del_Current_Reg
AddReg=Mazellan401A.Add, 1024, DPMS

[Mazellan900P]
DelReg=Del_Current_Reg
AddReg=Mazellan900P.Add, 1600, DPMS

[Mazellan701P]
DelReg=Del_Current_Reg
AddReg=Mazellan701P.Add, 1600, DPMS

[Mazellan_400P]
DelReg=Del_Current_Reg
AddReg=Mazellan_400P.Add, 1024, DPMS

[Mazellan_500A]
DelReg=Del_Current_Reg
AddReg=Mazellan_500A.Add, 1024, DPMS

[900P]
DelReg=Del_Current_Reg
AddReg=900P.Add, 1600, DPMS

[701P]
DelReg=Del_Current_Reg
AddReg=701P.Add, 1600, DPMS

[701A]
DelReg=Del_Current_Reg
AddReg=701A.Add, 1280, DPMS

[501P]
DelReg=Del_Current_Reg
AddReg=501P.Add, 1280, DPMS

[400P]
DelReg=Del_Current_Reg
AddReg=400P.Add, 1024, DPMS

[500A]
DelReg=Del_Current_Reg
AddReg=500A.Add, 1024, DPMS

[401A]
DelReg=Del_Current_Reg
AddReg=401A.Add, 1024, DPMS

[Hansol400F.Install]
DelReg=Del_Current_Reg
AddReg=Hansol400F.AddReg, 1024, DPMS

[400F.Install]
DelReg=Del_Current_Reg
AddReg=400F.AddReg, 1024, DPMS

[500F.Install]
DelReg=Del_Current_Reg
AddReg=500F.AddReg, 1024, DPMS
;
[710P]
DelReg=Del_Current_Reg
AddReg=710P.Add, 1600, DPMS

[710A]
DelReg=Del_Current_Reg
AddReg=710A.Add, 1280, DPMS

[710Aplus]
DelReg=Del_Current_Reg
AddReg=710Aplus.Add, 1280, DPMS

;-------------------------------------------------
; Common AddReg sections
;-------------------------------------------------
[Del_Current_Reg]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[640]
HKR,,MaxResolution,,"640,480"
[800]
HKR,,MaxResolution,,"800,600"
[1024]
HKR,,MaxResolution,,"1024,768"
[1280]
HKR,,MaxResolution,,"1280,1024"
[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

;-------------------------------------------------
; Model AddReg sections
;-------------------------------------------------
[Mazellan17px.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-85.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan17ax.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan15ax.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-54.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan14px.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-54.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan14ax.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-50.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan700P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-85.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan700A.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan701A.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-160.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan501P.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-150.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan500P.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan500A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-54.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan500M.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-54.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan400P.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-54.0,50.0-120.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan400A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-50.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan401A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-50.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan900P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-96.0,47.0-150.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan701P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-86.0,47.0-150.0,+,+"
HKR,,ICMProfile,1,9

[Mazellan_400P.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-55.0,47.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Mazellan_500A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-58.0,47.0-120.0,-,-"
HKR,,ICMProfile,1,9

[900P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-96.0,47.0-150.0,+,+"
HKR,,ICMProfile,1,9

[701P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-86.0,47.0-150.0,+,+"
HKR,,ICMProfile,1,9

[701A.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-160.0,+,+"
HKR,,ICMProfile,1,9

[501P.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-70.0,50.0-150.0,+,+"
HKR,,ICMProfile,1,9

[500A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-58.0,47.0-120.0,-,-"
HKR,,ICMProfile,1,9

[400P.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-55.0,47.0-120.0,-,-"
HKR,,ICMProfile,1,9

[401A.Add]
HKR,"MODES\1024,768",Mode1,,"30.0-50.0,50.0-120.0,-,-"
HKR,,ICMProfile,1,9

[Hansol400F.AddReg]
HKR,"MODES\640,350",Mode1,,"31.47,70.08,+,-"
HKR,"MODES\640,400",Mode1,,"31.47,70.08,-,+"
HKR,"MODES\640,480",Mode1,,"37.86,72.81,-,-"
HKR,"MODES\640,480",Mode2,,"35.00,67.00,-,-"
HKR,"MODES\640,480",Mode3,,"31.50,60.00,-,-"
HKR,"MODES\800,600",Mode1,,"35.16,56.25,+,+"
HKR,"MODES\800,600",Mode2,,"37.90,60.32,+,+"
HKR,"MODES\800,600",Mode3,,"48.08,72.19,+,+"
HKR,"MODES\832,624",Mode1,,"49.80,74.60,-,-"
HKR,"MODES\1024,768",Mode1,,"48.36,60.00,-,-"
HKR,"MODES\1024,768",Mode2,,"56.48,70.00,-,-"
HKR,"MODES\1024,768",Mode3,,"60.02,75.00,+,+"
HKR,"MODES\1024,768",Mode4,,"60.24,75.00,-,-"
HKR,,ICMProfile,1,9

[400F.AddReg]
HKR,"MODES\640,350",Mode1,,"31.47,70.08,+,-"
HKR,"MODES\640,400",Mode1,,"31.47,70.08,-,+"
HKR,"MODES\640,480",Mode1,,"31.50,60.00,-,-"
HKR,"MODES\640,480",Mode3,,"37.86,72.81,-,-"
HKR,"MODES\640,480",Mode4,,"37.50,75.00,-,-"
HKR,"MODES\800,600",Mode1,,"35.16,56.25,+,+"
HKR,"MODES\800,600",Mode2,,"37.90,60.32,+,+"
HKR,"MODES\800,600",Mode3,,"48.08,72.19,+,+"
HKR,"MODES\800,600",Mode4,,"46.88,75.00,+,+"
HKR,"MODES\1024,768",Mode1,,"48.36,60.00,-,-"
HKR,"MODES\1024,768",Mode2,,"56.48,70.00,-,-"
HKR,"MODES\1024,768",Mode3,,"60.02,75.00,+,+"
HKR,,ICMProfile,1,9

[500F.AddReg]
HKR,"MODES\640,350",Mode1,,"31.47,70.08,+,-"
HKR,"MODES\640,400",Mode1,,"31.47,70.08,-,+"
HKR,"MODES\640,480",Mode1,,"31.50,60.00,-,-"
HKR,"MODES\640,480",Mode3,,"37.86,72.81,-,-"
HKR,"MODES\640,480",Mode4,,"37.50,75.00,-,-"
HKR,"MODES\800,600",Mode1,,"35.16,56.25,+,+"
HKR,"MODES\800,600",Mode2,,"37.90,60.32,+,+"
HKR,"MODES\800,600",Mode3,,"48.08,72.19,+,+"
HKR,"MODES\800,600",Mode4,,"46.88,75.00,+,+"
HKR,"MODES\1024,768",Mode1,,"48.36,60.00,-,-"
HKR,"MODES\1024,768",Mode2,,"56.48,70.00,-,-"
HKR,"MODES\1024,768",Mode3,,"60.02,75.00,+,+"
HKR,,ICMProfile,1,9

[710P.Add]
HKR,"MODES\1600,1200",Mode1,,"30.0-95.0,47.0-160.0,+,+"
HKR,,ICMProfile,1,9

[710A.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-72.0,47.0-160.0,+,+"
HKR,,ICMProfile,1,9

[710Aplus.Add]
HKR,"MODES\1280,1024",Mode1,,"30.0-72.0,47.0-160.0,+,+"
HKR,,ICMProfile,1,9

;-------------------------------------------------
; User visible strings
;-------------------------------------------------
[Strings]
MS="Microsoft"
MonitorClassName="Monitor"
Hansol="Hansol Electronics"

Mazellan17px="Hansol Electronics Mazellan17px"
Mazellan17ax="Hansol Electronics Mazellan17ax"
Mazellan15ax="Hansol Electronics Mazellan15ax"
Mazellan14px="Hansol Electronics Mazellan14px"
Mazellan14ax="Hansol Electronics Mazellan14ax"

Mazellan700P="Hansol Electronics Mazellan700P"
Mazellan700A="Hansol Electronics Mazellan700A"
Mazellan500P="Hansol Electronics Mazellan500P"
Mazellan500A="Hansol Electronics Mazellan500A"
Mazellan500M="Hansol Electronics Mazellan500M"
Mazellan400P="Hansol Electronics Mazellan400P"
Mazellan400A="Hansol Electronics Mazellan400A"

Mazellan900P="Hansol Electronics Mazellan900P"
Mazellan701P="Hansol Electronics Mazellan701P"
Mazellan701A="Hansol Electronics Mazellan701A"
Mazellan501P="Hansol Electronics Mazellan501P"
Mazellan_500A="Hansol Electronics Mazellan_500A"
Mazellan_400P="Hansol Electronics Mazellan_400P"
Mazellan401A="Hansol Electronics Mazellan401A"

900P="Hansol Electronics 900P"
701P="Hansol Electronics 701P"
701A="Hansol Electronics 701A"
501P="Hansol Electronics 501P"
500A="Hansol Electronics 500A"
400P="Hansol Electronics 400P"
401A="Hansol Electronics 401A"

Hansol400F="Hansol Electronics Hansol400F"
400F="Hansol Electronics 400F"
500F="Hansol Electronics 500F"

710P="Hansol Electronics 710P"
710A="Hansol Electronics 710A"
710Aplus="Hansol Electronics 710Aplus"
