; P17-1A.INF Ver. 1.1 
;Monitor INF file for Fujitsu Siemens Monitor P17-1A
;Copyright 2004 Fujitsu Siemens Computers

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FUJSIE%
CatalogFile=FSCP17-1A.cat
DriverVer=04/30/2004, 1.1.0.1

[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS0510

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
DefaultDestDir=11
FUS-P17-1A.CopyFiles=23

[SourceDisksNames]
1=%DISK%,,,

[SourceDisksFiles]
FSCP171A.ICM=1

[Manufacturer]
%FUJSIE%=FUJSIE

[FUJSIE]
%FUS-P17-1A%=FUS-P17-1A.Install, Monitor\FUS0510

[FUS-P17-1A.Install]
DelReg=DEL_CURRENT_REG
AddReg=FUS-P17-1A.AddReg, 1280, DPMS
CopyFiles=FUS-P17-1A.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

; Pre-defined AddReg sections

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[FUS-P17-1A.AddReg]
HKR,"MODES\640,480",Mode1,,"31-38,55-76,-,-"
HKR,"MODES\800,600",Mode1,,"35-49,55-76,+,+"
HKR,"MODES\1024,768",Mode1,,"48-63,55-76,-,-"
HKR,"MODES\1280,1024",Mode1,,"30-83,55-76,+,+"

HKR,,ICMProfile,0,"FSCP171A.ICM"

[FUS-P17-1A.CopyFiles]
FSCP171A.ICM

[Strings]
DISK="Driver & Utility for P17-1A"
MonitorClassName="Monitor"
FUJSIE="Fujitsu Siemens Computers"
FUS-P17-1A="Fujitsu Siemens P17-1A"