; ###############################################################
;
;   HP_P19A.inf 
;
;   Ver. 1.0.0.0        
;   1/31/2013
;
;   Copyright (c)2013, Hewlett-Packard Development Company, L.P.
;   All Rights Reserved
;
;   This is a Microsoft Windows x86/x64 setup information 
;   file for the HP P19A LED Backlit LCD Monitor.
; 
; ###############################################################

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%HP%
CatalogFile=HP_P19A.cat
DriverVer=01/31/2013,1.0.0.0
PnpLockDown=1

[ControlFlags]
ExcludeFromSelect.nt = MONITOR\HWP3087

[ClassInstall32]
AddReg=ClassAddReg32

[ClassAddReg32]
HKR,,,,%MonitorClassName%
HKR,,Icon,,"-1"
HKR,,NoInstallClass,,1

[DestinationDirs]
DefaultDestDir=11
P19A.CopyFiles=23

[SourceDisksNames]
1=%Disk%,,,

[SourceDisksFiles]
HP_P19A.icm=1

[Manufacturer]
%HP%=HP,NTx86,NTamd64

[HP]
%P19A_A%=P19A_A.Install, Monitor\HWP3087

[HP.NTx86]
%P19A_A%=P19A_A.Install, Monitor\HWP3087

[HP.NTamd64]
%P19A_A%=P19A_A.Install, Monitor\HWP3087

[P19A_A.Install]
DelReg=DEL_CURRENT_REG
AddReg=P19A_A.AddReg, 1280, DPMS
CopyFiles=P19A.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1280]
HKR,,MaxResolution,,"1280,1024"

[DPMS]
HKR,,DPMS,,1

[P19A_A.AddReg]
HKR,"MODES\640,480",Mode1,,"24-83,50-76,-,-"
HKR,"MODES\800,600",Mode1,,"24-83,50-76,+,+"
HKR,"MODES\1024,768",Mode1,,"24-83,50-76,+,+"
HKR,"MODES\1280,720",Mode1,,"24-83,50-76,+,+"
HKR,"MODES\1280,800",Mode1,,"24-83,50-76,-,+"
HKR,"MODES\1280,960",Mode1,,"24-83,50-76,+,+"
HKR,"MODES\1280,1024",Mode1,,"24-83,50-76,+,+"
HKR,,PreferredMode,,"1280,1024,60"
HKR,,ICMProfile,0,"HP_P19A.icm"

[P19A.CopyFiles]
HP_P19A.icm

[Strings]
HP="HP"
MonitorClassName="Monitor"
P19A_A="HP P19A LED Backlit LCD Monitor"
Disk="HP P19A Driver Software"
