;
; Installation INF for 3rd party Cable Tuning Adapters
;  for use with WinTV-DCR 2650 (Model 143xxx) CableCard tuners
;
; Copyright (c) 2010-2013 Hauppauge Computer Works
;

[Version]
Signature="$CHICAGO$"
Class=USB
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
provider=%HCW%
DriverVer=03/05/2013,1.0.31064
CatalogFile=HCWe3TRIF.cat

[SourceDisksNames]
1=%Disk_Description%,,,DriverE3

[SourceDisksFiles]
HCWe3TRIF.sys = 1

[Manufacturer]
%MfgName%=Hauppauge, NTx86

[Hauppauge.NTx86]
%TA1.DeviceDesc%=HCWe3TRIF.Dev, USB\VID_05A6&PID_0008
%TA2.DeviceDesc%=HCWe3TRIF.Dev, USB\VID_07B2&PID_6002

[DestinationDirs]
HCWe3TRIF.Files.Ext = 10,System32\Drivers

[HCWe3TRIF.Dev.NT]
CopyFiles=HCWe3TRIF.Files.Ext

[HCWe3TRIF.Dev.NT.Services]
Addservice = HCWe3TRIF, 0x00000002, HCWe3TRIF.AddService

[HCWe3TRIF.AddService]
DisplayName    = %HCWe3TRIF.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\HCWe3TRIF.sys
AddReg         = HCWe3TRIF.AddReg
LoadOrderGroup = Base

[HCWe3TRIF.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,HCWe3TRIF.sys
HKR,"Parameters","MaximumTransferSize",0x10001,4096
HKR,"Parameters","DebugLevel",0x10001,2
HKR,"Parameters","BulkUsbEnable",0x10001,1

[HCWe3TRIF.Files.Ext]
HCWe3TRIF.sys

;---------------------------------------------------------------;

[Strings]
HCW="Hauppauge"
MfgName="Hauppauge"
Disk_Description="Hauppauge Tuning Adapter Installation Disk"
TA1.DeviceDesc="Hauppauge Tuning Adapter Driver (Cisco STA-1520)"
TA2.DeviceDesc="Hauppauge Tuning Adapter Driver (Motorola MTR-700)"
HCWe3TRIF.SvcDesc="Hauppauge Tuning Adapter Service"
