	 -----------------------------------
          README for AVerMedia WDM Driver
		
                 June.2000
         -----------------------------------

====================================
Install WDM Drivers for your TV card
====================================

If you want to switch your current VxD Driver to WDM Driver, the following 
shows you how to do that:

1. Remove Vxd Driver. In Device Manager, select "AVerMedia TV Series Device--
   Audio Section" and "AVerMedia TV Series Device--Video Section" devices, 
   then delete both of them.

2. In c:\windows\inf\others directory, you will find the 
   "AVerMediaTVFleeta.inf" and "AVerMediaTVFleetv.inf" files. Please delete 
   them. 

3. Restart computer. The wizard will find new devices, follow up the wizard 
   instuctions to install new driver. Note that you should indicate new 
   drivers' location to the wizard.

4. After the installation of drivers is completed, you will see the device 
   names: "AVerMedia, WDM Audio Capture", "AVerMedia, WDM Video Capture", 
   "AVerMedia, Philips WDM TvTuner", and "AVerMedia, WDM Crossbar". If you 
   see the above device names, you have succeeded the installation of divers. 

====================================
Install WDM Drivers for your TV card
====================================

If you have already installed WDM driver on Windows 2000 Professional, the 
following shows you how to upgrade driver:

1. In device manager, double-click "Sound, Video, and Game Controllers."

2. Click "AVerMedia, WDM Video Capture," right-click the device, and then 
   click Properties.

3. On the Driver tab, click Update Driver to open the Update Device Driver
   wizard. 

4. Click "Next."

5. Click "Display a list of the known drivers for this device so that I can 
   choose a specific driver" radio button.

6. On Select a Device Driver dialog, click "Have Disk..." button.

7. Browse to find "bt848.inf" which be download for web-site.

9. On Select a Device Driver dialog, click "AVerMedia, WDM Video Capture" then 
   click "Next" button.

10. Click "Yes" to install new driver.

11. Click "Next" to start instll new driver.

12. On "Digital signature not Found" dialog, Click "Yes."

13. Click "Finish."

14. Restart computer.
