; Copyright 2004, Philips Semiconductors GmbH

[Version]
signature="$CHICAGO$" ;all windows os
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%PSH%
DriverVer=04/17/2007,1.3.3.2
CatalogFile=3xHybrid.cat
CatalogFile.NTx86   = 3xHybrid.cat
CatalogFile.NTAMD64 = 3xHybr64.cat

[Manufacturer]
%PSH%=Philips, NTx86, NTAMD64

[Philips]
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7130
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134
%Hybrid.DeviceDescSilicon%  =3xHybrid.NTx86,PCI\VEN_1131&DEV_7133

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712617DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712717DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712817DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712917DE

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712217DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712317DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712417DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712517DE
;******** Subvendors
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713117DE
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713517DE
%Hybrid.DeviceDescSilicon%  =3xHybridB.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713617DE
%Hybrid.DeviceDescSilicon%  =3xHybridC.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713717DE
%Hybrid.DeviceDescSilicon%  =3xHybridD.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713817DE
%Hybrid.DeviceDescSilicon%  =3xHybridE.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720017DE
%Hybrid.DeviceDescSilicon%  =3xHybridF.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713917DE
%Hybrid.DeviceDescSilicon%  =3xHybridG.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713A17DE
%Hybrid.DeviceDescSilicon%  =3xHybridH.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720117DE
%Hybrid.DeviceDescSilicon%  =3xHybridI.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720217DE
%Hybrid.DeviceDescSilicon%  =3xHybridJ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720317DE
%Hybrid.DeviceDescSilicon%  =3xHybridK.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725017DE
%Hybrid.DeviceDescSilicon%  =3xHybridL.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_723017DE
%Hybrid.DeviceDescSilicon%  =3xHybridM.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725117DE
%Hybrid.DeviceDescSilicon%  =3xHybridN.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725217DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735017DE
%Hybrid.DeviceDescSilicon%  =3xHybridP.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735117DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735217DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725317DE
%Hybrid.DeviceDescSilicon%  =3xHybridR.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725417DE
%Hybrid.DeviceDescSilicon%  =3xHybridS.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725517DE
%Hybrid.DeviceDescSilicon%  =3xHybridT.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_730017DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725617DE
%Hybrid.DeviceDescSilicon%  =3xHybridU.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_730117DE

;---> 32 BIT SUPPORT <---
[Philips.NTx86]
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7130
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134
%Hybrid.DeviceDescSilicon%  =3xHybrid.NTx86,PCI\VEN_1131&DEV_7133

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712617DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712717DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712817DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7134&SUBSYS_712917DE

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712217DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712317DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712417DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_712517DE

;******** Subvendors
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713117DE
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713517DE
%Hybrid.DeviceDescSilicon%  =3xHybridB.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713617DE
%Hybrid.DeviceDescSilicon%  =3xHybridC.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713717DE
%Hybrid.DeviceDescSilicon%  =3xHybridD.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713817DE
%Hybrid.DeviceDescSilicon%  =3xHybridE.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720017DE
%Hybrid.DeviceDescSilicon%  =3xHybridF.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713917DE
%Hybrid.DeviceDescSilicon%  =3xHybridG.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_713A17DE
%Hybrid.DeviceDescSilicon%  =3xHybridH.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720117DE
%Hybrid.DeviceDescSilicon%  =3xHybridI.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720217DE
%Hybrid.DeviceDescSilicon%  =3xHybridJ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_720317DE
%Hybrid.DeviceDescSilicon%  =3xHybridK.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725017DE
%Hybrid.DeviceDescSilicon%  =3xHybridL.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_723017DE
%Hybrid.DeviceDescSilicon%  =3xHybridM.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725117DE
%Hybrid.DeviceDescSilicon%  =3xHybridN.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725217DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735017DE
%Hybrid.DeviceDescSilicon%  =3xHybridP.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735117DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_735217DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725317DE
%Hybrid.DeviceDescSilicon%  =3xHybridR.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725417DE
%Hybrid.DeviceDescSilicon%  =3xHybridS.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725517DE
%Hybrid.DeviceDescSilicon%  =3xHybridT.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_730017DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_725617DE
%Hybrid.DeviceDescSilicon%  =3xHybridU.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_730117DE

;---> 64 BIT SUPPORT <---
[Philips.NTAMD64]
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTAMD64,PCI\VEN_1131&DEV_7130
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTAMD64,PCI\VEN_1131&DEV_7134
%Hybrid.DeviceDescSilicon%  =3xHybrid.NTAMD64,PCI\VEN_1131&DEV_7133

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_712617DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_712717DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_712817DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTAMD64,PCI\VEN_1131&DEV_7134&SUBSYS_712917DE

%Hybrid.DeviceDescSilicon%  =3xHybridW.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_712217DE
%Hybrid.DeviceDescSilicon%  =3xHybridW.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_712317DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_712417DE
%Hybrid.DeviceDescSilicon%  =3xHybridV.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_712517DE

;******** Subvendors
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713117DE
%Hybrid.DeviceDescSilicon%  =3xHybridA.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713517DE
%Hybrid.DeviceDescSilicon%  =3xHybridB.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713617DE
%Hybrid.DeviceDescSilicon%  =3xHybridC.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713717DE
%Hybrid.DeviceDescSilicon%  =3xHybridD.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713817DE
%Hybrid.DeviceDescSilicon%  =3xHybridE.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_720017DE
%Hybrid.DeviceDescSilicon%  =3xHybridF.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713917DE
%Hybrid.DeviceDescSilicon%  =3xHybridG.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_713A17DE
%Hybrid.DeviceDescSilicon%  =3xHybridH.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_720117DE
%Hybrid.DeviceDescSilicon%  =3xHybridI.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_720217DE
%Hybrid.DeviceDescSilicon%  =3xHybridJ.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_720317DE
%Hybrid.DeviceDescSilicon%  =3xHybridK.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725017DE
%Hybrid.DeviceDescSilicon%  =3xHybridL.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_723017DE
%Hybrid.DeviceDescSilicon%  =3xHybridM.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725117DE
%Hybrid.DeviceDescSilicon%  =3xHybridN.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725217DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_735017DE
%Hybrid.DeviceDescSilicon%  =3xHybridP.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_735117DE
%Hybrid.DeviceDescSilicon%  =3xHybridO.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_735217DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725317DE
%Hybrid.DeviceDescSilicon%  =3xHybridR.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725417DE
%Hybrid.DeviceDescSilicon%  =3xHybridS.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725517DE
%Hybrid.DeviceDescSilicon%  =3xHybridT.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_730017DE
%Hybrid.DeviceDescSilicon%  =3xHybridQ.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_725617DE
%Hybrid.DeviceDescSilicon%  =3xHybridU.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_730117DE

[DestinationDirs]
SectionX32.CopyDll.NTx86      = 11
SectionX64.CopyDll.NTAMD64    = 11
SectionX32.CopyDriver.NTx86   = 10,system32\drivers
SectionX64.CopyDriver.NTAMD64 = 10,system32\drivers

[SectionX32.CopyDll.NTx86]
34CoInstaller.dll

[SectionX64.CopyDll.NTAMD64]

[SectionX32.CopyDriver.NTx86]
3xHybrid.sys

[SectionX64.CopyDriver.NTAMD64]
3xHybr64.sys

[SourceDisksNames]
1 = %AVSTRM_INSTALLATION_DISK%,,

[SourceDisksFiles]
3xHybrid.sys           = 1
3xHybr64.sys           = 1
34CoInstaller.dll      = 1


;
;*** initialization and registry entries
;

[3xHybrid.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridA.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridB.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridC.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridD.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridE.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridF.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridG.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridH.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridI.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridJ.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridK.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridL.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridM.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridN.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridO.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridP.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridQ.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridR.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridS.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridT.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridU.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridV.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybridW.NTx86.CoInstallers]
CopyFiles = SectionX32.CopyDll.NTx86
AddReg = SectionX32.DllAddReg.NTx86

[3xHybrid.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridA.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridB.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridC.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridD.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridE.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridF.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridG.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridH.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridI.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridJ.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridK.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridL.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridM.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridN.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridO.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridP.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridQ.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridR.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridS.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridT.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridU.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridV.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[3xHybridW.NTAMD64.CoInstallers]
CopyFiles = SectionX64.CopyDll.NTAMD64
AddReg = SectionX64.DllAddReg.NTAMD64

[SectionX32.DllAddReg.NTx86]
HKR,,CoInstallers32,0x00010000,"34CoInstaller.dll, CoInstallerEntry"

[SectionX64.DllAddReg.NTAMD64]

[3xHybrid.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridB.AddReg, Common.AddReg, Autodetect.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridA.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridA.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridB.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridB.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridC.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridC.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridD.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridD.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridE.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridE.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridF.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridF.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridG.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridG.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridH.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridH.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridI.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridI.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridJ.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridJ.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridK.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridK.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridL.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridL.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridM.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridM.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridN.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridN.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridO.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridO.AddReg, Common.AddReg

[3xHybridP.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridP.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridQ.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridQ.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridR.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridR.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridS.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridS.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridT.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridT.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridU.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridU.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridV.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridV.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86

[3xHybridW.NTx86]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg=3xHybrid.AddReg.NTx86, 3xHybridW.AddReg, Common.AddReg
RegisterDlls  = SectionX32.Register.NTx86


[3xHybrid.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridA.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridB.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridC.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridD.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridE.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridF.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridG.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridH.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridI.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridJ.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridK.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridL.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridM.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridN.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridO.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridP.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridQ.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridR.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridS.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridT.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridU.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridV.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybridW.NTx86.Services]
AddService=%SERVICE_NAME_X32%, 0x00000002, 3xHybrid32.ServiceInstall

[3xHybrid.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridB.AddReg, Common.AddReg, Autodetect.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridA.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridA.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridB.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridB.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridC.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridC.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridD.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridD.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridE.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridE.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridF.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridF.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridG.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridG.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridH.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridH.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridI.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridI.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridJ.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridJ.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridK.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridK.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridL.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridL.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridM.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridM.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridN.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridN.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridO.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridO.AddReg, Common.AddReg

[3xHybridP.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridP.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridQ.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridQ.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridR.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridR.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridS.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridS.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridT.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridT.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridU.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridU.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridV.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridV.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybridW.NTAMD64]
Include=ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs=KS.Registration.NT, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg=3xHybrid.AddReg.NTAMD64, 3xHybridW.AddReg, Common.AddReg
RegisterDlls  = SectionX64.Register.NTAMD64

[3xHybrid.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridA.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridB.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridC.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridD.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridE.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridF.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridG.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridH.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridI.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridJ.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridK.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridL.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridM.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridN.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridO.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridP.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridQ.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridR.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridS.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridT.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridU.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridV.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[3xHybridW.NTAMD64.Services]
AddService=%SERVICE_NAME_X64%, 0x00000002, 3xHybrid64.ServiceInstall

[SectionX32.Register.NTx86]
11,,34CoInstaller.dll,1 ;FLG_REGSVR_DLLREGISTER


[SectionX64.Register.NTAMD64]


[3xHybrid32.ServiceInstall]
DisplayName=%DISPLAY_NAME%
Description=%SERVICE_DESCRIPTION%
ServiceType=%SERVICE_KERNEL_DRIVER%
StartType=%SERVICE_DEMAND_START%
ErrorControl=%SERVICE_ERROR_IGNORE%
ServiceBinary=%12%\3xHybrid.sys
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

[3xHybrid64.ServiceInstall]
DisplayName=%DISPLAY_NAME%
Description=%SERVICE_DESCRIPTION%
ServiceType=%SERVICE_KERNEL_DRIVER%
StartType=%SERVICE_DEMAND_START%
ErrorControl=%SERVICE_ERROR_IGNORE%
ServiceBinary=%12%\3xHybr64.sys

[3xHybrid.AddReg.NTx86]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,3xHybrid.sys

; audio capture registry entries

HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,3xHybrid.SYS

HKR,Drivers,SubClasses,,"wave,mixer"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,"Philips Audio Capture Device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Philips Audio Capture Device"


; Setting FM radio of the Silicon tuner via SIF (GPIO 21 in use/ 5.5MHz)
HKR, "Audio", "FM Radio IF",0x00010001,0x729555

; Enable MCE 
;HKR, "Parameters", "MCE",0x00010001,0x01
; add audio input and output pinnames
HKR, "Parameters", "Syncronization disabled",0x00010001,0x0

; under MCE, IgnoreDVBParameter=1, prevents the driver to use the DShow DVB properties.
; -1 is used instead
HKR, "Parameters", "IgnoreDVBParameter",0x00010001,0x00

; under MCE, AutoRemove60HzStd fixes the 1st run problem with analog multi standard tuner
; like the TDA8275A. In countries with 50Hz formats, 60Hz formats are beeing removed
HKR, "Parameters", "AutoRemove60HzStd",0x00010001,0x01
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%
HKR, "Parameters", "SmallXBar",0x00010001,0x01
HKR, "Parameters", "TDA8275A_BlankVideo",0x00010001,0x01
HKR, "Parameters", "TDA8275A_UseTuningThread",0x00010001,0x00
HKR, "Parameters", "GetRegATSCModulationType",0x00010001,0x00
HKR, "Parameters", "ATSCDemodulatedMode",0x00010001,0x17




HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

[3xHybrid.AddReg.NTAMD64]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,3xHybr64.sys

; audio capture registry entries

HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,3xHybr64.sys

HKR,Drivers,SubClasses,,"wave,mixer"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,"Philips Audio Capture Device"
HKR,Drivers\mixer\wdmaud.drv,Description,,"Philips Audio Capture Device"


; Setting FM radio of the Silicon tuner via SIF (GPIO 21 in use/ 5.5MHz)
HKR, "Audio", "FM Radio IF",0x00010001,0x729555

; Enable MCE 
;HKR, "Parameters", "MCE",0x00010001,0x01
; add audio input and output pinnames
HKR, "Parameters", "Syncronization disabled",0x00010001,0x0

; under MCE, IgnoreDVBParameter=1, prevents the driver to use the DShow DVB properties.
; -1 is used instead
HKR, "Parameters", "IgnoreDVBParameter",0x00010001,0x00

; under MCE, AutoRemove60HzStd fixes the 1st run problem with analog multi standard tuner
; like the TDA8275A. In countries with 50Hz formats, 60Hz formats are beeing removed
HKR, "Parameters", "AutoRemove60HzStd",0x00010001,0x01
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%
HKR, "Parameters", "SmallXBar",0x00010001,0x01
HKR, "Parameters", "TDA8275A_BlankVideo",0x00010001,0x01
HKR, "Parameters", "TDA8275A_UseTuningThread",0x00010001,0x00



HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%VAMP_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

[Autodetect.AddReg]
HKR, "Parameters", "AutoDetect",0x00010001,0x01

[3xHybridA.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x14,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridB.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridC.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x14,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridD.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x14,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridE.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x1E,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x32,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridF.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridG.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x22,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x30,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridH.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x2B,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x32,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridI.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x1E,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x22,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridJ.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x2B,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x22,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridK.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x32,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x06,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridL.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x51,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x01,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x20,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridM.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x32,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x06,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridN.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x22,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x06,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridO.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x18,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0xFF,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x55,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x55,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x55,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridP.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x18,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x21,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x00,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridQ.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x32,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x50,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridR.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x32,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x50,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridS.AddReg]
HKR, "Parameters", "Latency Timer",0x00010001,0x40
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x21,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x22,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x50,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridT.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x17,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x3A,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x50,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridU.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x17,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x96,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x38,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x15,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x50,0x00,0x00,0x00               ; FM radio mode.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

[3xHybridV.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x04,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x3A,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,2
HKR, "AudioDecoder", "SVHS Channel",0x00010001,2
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,2
HKR, "Parameters", "Ctrl4052IC",0x00010001,0x1
HKR, "Parameters", "FMADCLevel",0x00010001,0x9


[3xHybridW.AddReg]
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x08,0x00,0x00,0x00               ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC2,0x00,0x00,0x00               ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x00,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x10,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x03,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x3A,0x00,0x00,0x00               ; Tuner IF PLL slave addr.
HKR, "AudioDecoder", "CVBS Channel",0x00010001,2
HKR, "AudioDecoder", "SVHS Channel",0x00010001,2
HKR, "AudioDecoder", "FM Radio Channel",0x00010001,2
HKR, "Parameters", "Ctrl4052IC",0x00010001,0x1
HKR, "Parameters", "FMADCLevel",0x00010001,0x9
HKR, "Audio", "Check_NICAM_I",0x00010001,0x1



[Common.AddReg]

HKR, "AudioDecoder", "Tuner Channel",0x00010001,1
;HKR, "AudioDecoder", "CVBS Channel",0x00010001,3
;HKR, "AudioDecoder", "SVHS Channel",0x00010001,3
;HKR, "AudioDecoder", "FM Radio Channel",0x00010001,1

; maps user setting to hardware video input
HKR, "VideoDecoder", "Tuner Channel",0x00010001,1
HKR, "VideoDecoder", "CVBS Channel",0x00010001,3
HKR, "VideoDecoder", "SVHS Channel",0x00010001,8
HKR, "VideoDecoder", "FM Radio Channel",0x00010001,1

; I2C Device settings
HKR, "I2C Devices", "Number of I2C Devices",0x00010001,1
HKR, "I2C Devices", "Force Registry Settings",0x00010001,1

HKR,,PageOutWhenUnopened,3,0
HKR,,DontSuspendIfStreamsAreRunning,3,00


;
;*** strings, GUIDs and names
;

[Strings]

; Proxy GUIDs

KSProxy.CLSID   = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSXBar.CLSID    = "{71F96460-78F3-11d0-A18C-00A0C9118956}"
KSTVAudio.CLSID = "{71F96462-78F3-11d0-A18C-00A0C9118956}"
KSTvTune.CLSID  = "{266EEE40-6C63-11cf-8A03-00AA006ECB65}"

; Category GUIDs

KSCATEGORY_CAPTURE                = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO                  = "{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_AUDIO                  = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"

; Our Pin Name GUIDs

VAMP_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
VAMP_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
VAMP_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
VAMP_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"

VAMP_MPEG_AES_PIN        = "{9DEC84B9-BCEF-4aac-997E-43EDD0A2D6C7}"
VAMP_MPEG_VES_PIN        = "{181CF87E-7741-47ba-8629-22347E03C64C}"
VAMP_MPEG_PS_PIN         = "{DDA87B83-65DB-4aec-82D0-79FBE67D2BB6}"

; Our Filter GUIDs

VAMP_ANLG_AUDIO_FILTER   = "{F3B951E7-8619-4ff3-91CA-03910E4BB900}"
VAMP_ANLG_CAP_FILTER     = "{BBEFB6C7-2FC4-4139-BB8B-A58BBA724000}"

; system defines

SERVICE_BOOT_START     = 0x0 
SERVICE_SYSTEM_START   = 0x1 
SERVICE_AUTO_START     = 0x2 
SERVICE_DEMAND_START   = 0x3 
SERVICE_DISABLED       = 0x4 

SERVICE_KERNEL_DRIVER  = 0x1 
SERVICE_ERROR_IGNORE   = 0x0 
SERVICE_ERROR_NORMAL   = 0x1 
SERVICE_ERROR_SEVERE   = 0x2
SERVICE_ERROR_CRITICAL = 0x3 

FLG_REGSVR_DLLREGISTER = 0x00000001

;Our strings

PSH="Philips"
PHILIPS_CUSTOM_TUNERNAME      = "713x"
30Hybrid.DeviceDesc      = "Philips SAA7130, Hybrid Capture Device"
34Hybrid.DeviceDesc      = "Philips SAA7134, Hybrid Capture Device"
33Hybrid.DeviceDesc      = "Philips SAA7133/35, Hybrid Capture Device"
AVSTRM_INSTALLATION_DISK = "3xHybrid installation disk"
DISPLAY_NAME             = "3xHybrid service"
SERVICE_NAME_X32              = "3xHybrid"
SERVICE_NAME_X64              = "3xHybr64"
SERVICE_DESCRIPTION           = "Philips SAA713x BDA Capture Driver"
Hybrid.DeviceDescSilicon=   "Philips SAA713X, Hybrid Capture Device"