; Copyright Leadtek Research Inc.
[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Leadtek"
DriverVer=03/23/2010,6.0.1012.7007
CatalogFile.ntamd64=wfsono64.cat

[Manufacturer]
"Leadtek"=Leadtek,NTamd64

[SourceDisksNames]
1="Leadtek CX23885 Drivers",,,""

[SourceDisksFiles]
wfsonora.sys=1
wf416enc.rom=1
wf23885C.rom=1
;cxtvrate.dll=1
;cpnotify.ax=1
encprxypage.ax=1
;wfcorona.ax=1
;cxtvrateWow64.dll=1
;cpnotifyWow64.ax=1
encprxypageWow64.ax=1
;wfcoronaWow64.ax=1
WFEXEC.DLL=1

[Leadtek.NTamd64]
%CX23885.DeviceDesc%=CX23885.Sonora,PCI\VEN_14F1&DEV_8852&SUBSYS_6F39107D

[CX23885.Sonora]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,SonoraXBAR.AddReg,CX23885.Xceive.AddReg,Xceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles,DSFiltersWow64.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX23885.Sonora.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration.NT,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,SonoraXBAR.AddReg,CX23885.Xceive.AddReg,Xceive.AddReg,CXTS.AddReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles,DSFiltersWow64.CopyFiles
RegisterDlls=DSFilters.RegDLL


[DestinationDirs]
CX885.CopyDrivers=10,system32\drivers
DSFilters.CopyFiles=11
DSFiltersWow64.CopyFiles=10, SysWow64

[CX885.CopyDrivers]
wfsonora.sys
wf416enc.rom
wf23885C.rom

[DSFiltersWow64.CopyFiles]
WFEXEC.DLL
;cxtvrate.dll,cxtvrateWow64.dll
;cpnotify.ax,cpnotifyWow64.ax
encprxypage.ax,encprxypageWow64.ax
;wfcorona.ax,wfcoronaWow64.ax

[DSFilters.CopyFiles]
encprxypage.ax
;cxtvrate.dll
;cpnotify.ax
;wfcorona.ax

[DSFilters.RegDLL]
11,,encprxypage.ax,1
;11,,wfcorona.ax,1
;11,,cpnotify.ax,1
;11,,cxtvrate.dll,1

[CX885.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,wfsonora.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,%MediaCategories%\%GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%
HKLM,%MediaCategories%\%GUID.PINNAME_AUDIO_OUT%,Name,,%PinName.AnalogAudioOut%
;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0xFE, 0x00, 0x00, 0x00

;
;Register the name of the 656 and MPEG pins
;
HKLM,%MediaCategories%\%GUID.PINNAME_656_OUT%,Name,,%PinName.656_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_656_IN%,Name,,%PinName.656_IN%
HKLM,%MediaCategories%\%GUID.PINNAME_MPEG_OUT%,Name,,%PinName.MpegOut%

;
;Add the property pages
;
HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,

HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Video_Properties%,,,

HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Audio_Properties%,,,

HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.MPEG_Properties%,,,

HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Diagnostic_Properties%,,,

HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,,,encprxypage.ax
HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Noise_Properties%,,,

;Register the encoder and multiplexer classes with Direct X
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,CLSID,,%GUID.Encoder%
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,FriendlyName,,%Category_Encoders%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,CLSID,,%GUID.Multiplexer%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,FriendlyName,,%Category_Multiplexers%

;Register the names of the encoder and multiplexer nodes
HKLM,%MediaCategories%\%GUID.Encoder%,Name,,%Node.Encoder%
HKLM,%MediaCategories%\%GUID.Encoder%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%GUID.Multiplexer%,Name,,%Node.Multiplexer%
HKLM,%MediaCategories%\%GUID.Multiplexer%,Display,1,00,00,00,00

HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},,,"Copy Protect Notification Filter"
HKLM,%MediaInterfaces%\{0A7AF963-6805-4f99-B284-29B680975542},IID,1,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00,00

;Wave in audio device registration
;HKR,Drivers,SubClasses,,"wave"
;HKR,Drivers\wave\wdmaud.drv, Driver,,wdmaud.drv
;HKR,Drivers\wave\wdmaud.drv,Description,,%AudioFriendlyName%

; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x00,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x00,0x00,0x00,0x00

; The following entries just for testing BDA driver
; No demod for now
HKR,"DriverData","TunerModel",0x00010001, 0x03,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
; CE6353_XC4000
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support
HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard
HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

;Add the property pages
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,wfcorona.ax
;HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
;HKLM,%MediaSets%\%GUID.CORONA_VERSION_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,

; GPIO Pin values 
; IMPORTANT !!! if any GPIO is not used - just delete the corresponding entry !!!
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","comp_select_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

;BoardType
;Palomar_NTSC=0,		// 885 + Philips NTSC Analog Tuner
;Palomar_PAL=1, 		// 885 + Philips PAL Analog Tuner
;PalomarXT=2, 		// 885 + Zarlink + Xceive
;Sonora353=3, 		// 885 + Zarlink + Xceive + 416/417
;Sonora702=4, 		// 885 + 702 + Xceive + 416/417
;PalomarX=5,		// 885 + Xceive (ExpressCard)
;PalomarCTX=6,		// 885 + Zarlink + Xceive (ExpressCard)
;PalomarDVD=7,		// 885 (ExpressCard)
;Palomar888_NTSC=8,	// 888 + Philips NTSC Analog Tuner
;Palomar888_PAL=9,	// 888 + Philips PAL Analog Tuner
;Palomar888_XT=10,		// 888 + Zarlink + Xceive
;Mojave=11,       		// 888 + CX24010 + Zarlink
HKR,"DriverData","BoardType",0x00010001, 0x03, 0x00, 0x00, 0x00

;
; Driver Configuration Registry Entries
;
;; Wow64 filters
;HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"WinFast.cxtvrate.dll",,"rundll32 %10%\SysWOW64\WFEXEC.DLL,WinFastExec regsvr32 -s %10%\SysWOW64\cxtvrate.dll"
;HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"WinFast.cpnotify.ax",,"rundll32 %10%\SysWOW64\WFEXEC.DLL,WinFastExec regsvr32 -s %10%\SysWOW64\cpnotify.ax"
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"WinFast.encprxypage.ax",,"rundll32 %10%\SysWOW64\WFEXEC.DLL,WinFastExec regsvr32 -s %10%\SysWOW64\encprxypage.ax"



[CX23885.Xceive.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00


;-------------------------------------------------------------------
; Crossbar AddReg sections
;
;---Crossbar registry values---
;
; Note: For each pin on the crossbar, specify the following:
; (1) Pin type 
;     0 - TunerIn
;     1 - Composite 1
;     2 - SVideo 1
;     3 - Component
;     4 - Composite 2
;     5 - SVideo 2
;     6 - Audio from Tuner
;     7 - Audio from Line In
;     8 - Audio from Line In 2
; (2) InputMux (optional) - input mux to use for the selected pin
;     in 0xAA, 0xBB, 0xCC, 0x00 format
;     where AA is the input mux for Composite/S-Video Luma/Component Luma
;           BB is the input mux for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input mux for Component YPb
; (3) InputChannel (optional, but required if InputMux present) - Input channel 
;     to use for mux in 0xAA, 0xBB, 0xCC, 0xDD format
;     where AA is the input channel for Composite/S-Video Luma/Component Luma
;           BB is the input channel for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input channel for Component YPb 
;           DD = 1 if dual ADC2 mode required, zero if single mode
; (4) RelatedPinIndex 

;-------------------------------------------------------------------

[SonoraXBAR.AddReg]

;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin6 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN1 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear) : Conexant 
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Lume, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin7
;;HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
;;HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
;;HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
;;HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00
;Pin 2 - S-Video 1 (Rear) : Leadtek 
; Input Mux       : VIN3 for Luma, VIN4 for Chroma
; Input Channel   : Ch1 for  Lume, Ch2  for Chroma
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 3 - Component 1 (Rear) : Conexant
; Input Mux       : VIN8 for Luma, VIN6 for YPb, VIN7 for YPr
; Input Channel   : Ch1 for  Lume, Ch2  for YPb, Ch3  for YPr, Dual ADC
; Related PinIndex: Audio Line In 1 - Pin7
;;HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
;;HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x08,0x06,0x07,0x00
;;HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x02,0x03,0x01
;;HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00
;Pin 3 - Component 1 (Rear) : Leadtek
; Input Mux       : VIN7 for Luma, VIN6 for YPb, VIN8 for YPr
; Input Channel   : Ch1 for  Lume, Ch2  for YPb, Ch3  for YPr, Dual ADC
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x07,0x06,0x08,0x00
HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x02,0x03,0x01
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - Composite 2 (Front) 
; Input Mux       : VIN1 for Composite - same as Composite1 - switched with GPIO0 MUX
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 5 - S-Video 2 (Front)
; Input Mux       : VIN3 for Luma, VIN4 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin5","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 6 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 7 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 8 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin4
HKR,"DriverData\XBarPin8","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin8","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00


;-------------------------------------------------------------------
; Tuner AddReg sections
;-------------------------------------------------------------------

[Xceive.AddReg]
; XC4000
HKR,"DriverData","TunerType",0x00010001, 0x21, 0x00, 0x00, 0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

;-------------------------------------------------------------------
; AddReg sections for TS filter
;-------------------------------------------------------------------

[CXTS.AddReg]
HKLM,%MediaCategories%\%TSPinID%,Display,1, 00,00,00,00
HKLM,%MediaCategories%\%TSPinID%,Name,,%TSPinName%

;
; Interfaces installation
;

;
; Video
;
[CX23885.Sonora.Interfaces]
Needs=VID.Interfaces

[CX23885.Sonora.NT.Interfaces]
Needs=VID.Interfaces


[VID.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%KsNameFilter%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
;AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,
; Encoder interface
AddInterface=%GUID.Encoder%,%EncoderReferenceGuid%,ENCODER_Interface,
AddInterface=%GUID.Multiplexer%,%EncoderReferenceGuid%,ENCODER_Interface


[VID_Interface]
AddReg=VID_Interface.AddReg

[VID_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%VIDFriendlyName%

[TvAudio_Interface]
AddReg=TvAudio_Interface.AddReg

[TvAudio_Interface.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%TVAudioFriendlyName%

[CX88XBAR_Interface]
AddReg=CX88XBAR_Interface.AddReg

[CX88XBAR_Interface.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%XBARFriendlyName%

[CX88TUNE_Interface]
AddReg=CX88TUNE_Interface.AddReg

[CX88TUNE_Interface.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%TunerFriendlyName%

[AUD_Interface]
AddReg=AUD_Interface.AddReg

[AUD_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AudioFriendlyName%

[BDATUNE_Interface]
AddReg=BDATUNE_Interface.AddReg

[BDATUNE_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName%

[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%

[ENCODER_Interface]
AddReg=ENCODER_Interface.AddReg

[ENCODER_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%EncoderFriendlyName%
;Add an interface for Microsoft's video bit rate property set
HKR,Interfaces\{B43C4EEC-8C32-4791-9102-508ADA5EE8E7},,,
HKR,Interfaces\{b05dabd9-56e5-4fdc-afa4-8a47e91f1c9c},,,
HKR,Capabilities,,,
HKR,Capabilities,"{BB4FAA02-596C-4129-8FB3-74E75421FA02}", 0x00010001,1

;
; Services installation
;
[CX23885.Sonora.Services]
AddService = WFSONORA,2,VID.ServiceInstall

[CX23885.Sonora.NT.Services]
AddService = WFSONORA,2,VID.ServiceInstall


[VID.ServiceInstall]
DisplayName   = %CX23885.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\wfsonora.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
KsNameFilter                 = "{9B365890-165F-11D0-A195-0020AFD156E4}"
Proxy.CLSID                  = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
;;
CX23885.DeviceDesc           = "WinFast PxDVR3200 H (XC4000)"
VIDFriendlyName              = "WinFast PxDVR3200 H Video Capture"
TVAudioFriendlyName          = "WinFast PxDVR3200 H TvAudio"
XBARFriendlyName             = "WinFast PxDVR3200 H Crossbar"
TunerFriendlyName            = "WinFast PxDVR3200 H Tuner"
BDATuneFriendlyName          = "WinFast PxDVR3200 H BDA Tuner"
TSFriendlyName               = "WinFast PxDVR3200 H TS Capture"
AudioFriendlyName            = "WinFast PxDVR3200 H Audio Capture"
EncoderFriendlyName          = "WinFast PxDVR3200 H MPEG Encoder"
;;
MediaCategories              = "SYSTEM\CurrentControlSet\Control\MediaCategories"
GUID.PINNAME_ANALOG_AUDIO_IN = "{04394D28-52A7-4c46-AED0-65D62CC64DA6}"
;; Vista RC2
;;Pin.p2AnalogAudioIn          = "Analog Audio In"
Pin.p2AnalogAudioIn          = "Audio"
GUID.PINNAME_AUDIO_OUT       = "{9DA02733-7910-40f2-95DD-0441676C9A9B}"
PinName.AnalogAudioOut       = "Audio Out"
TVAudioReferenceGuid         = "{991182D5-71A2-4b5c-9817-F551FBBC8232}"
XBARReferenceGUID            = "{77F656DA-696D-407c-BA1C-50E4457C12E8}"
TunerReferenceGuid           = "{5618011C-A4DA-455b-A448-EC2AF3DCCB02}"
TSPinID                      = "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName                    = "TS Out"
BDATuneReferenceGuid         = "{E01E1072-3DF3-4c23-B99F-6A27A7CC7CD2}"
TSReferenceGuid              = "{5ea9c066-1dfe-41c5-a2de-bf766e83c98e}"
AudioReferenceGuid           = "{AB766B70-AFB3-4461-A4DE-22E9C516B7FE}"
EncoderReferenceGuid         = "{1C10193D-7DCA-4f55-99D8-B017AAD3921D}"
GUID.Encoder                 = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
GUID.Multiplexer             = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
Category_Encoders            = "WDM Streaming Encoder Devices"
Category_Multiplexers        = "WDM Streaming Multiplexer Devices"
Node.Encoder                 = "Encoder"
Node.Multiplexer             = "Multiplexer"
GUID.PINNAME_656_IN          = "{DFD530C7-36D9-47ff-B838-9A11D215B140}"
PinName.656_IN               = "656"
GUID.PINNAME_656_OUT         = "{E2EEB283-EB84-4910-BABE-037FFBB03249}"
PinName.656_OUT              = "656"
GUID.PINNAME_MPEG_OUT        = "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
PinName.MpegOut              = "MPEG"
GUID.IVAC_PROPERTIES         = "{87489F71-B890-4ba2-A88B-03E0B1A4EC1D}"
GUID.General_Properties      = "{F6E6FBD9-FE5D-419d-B994-57FB20AAED1D}"
GUID.Video_Properties        = "{5D64F5ED-1526-46f5-B510-AA93437FFA6E}"
GUID.Audio_Properties        = "{9D52CFF7-0DB7-4300-B936-844105E64E9E}"
GUID.MPEG_Properties         = "{A6ABB595-D3B7-4fdf-A418-F2C79E6E1C14}"
GUID.Diagnostic_Properties   = "{18759BBE-6A06-4118-9A57-E833AD670B81}"
GUID.Noise_Properties        = "{10E2DF32-3EC5-4551-BAE6-6D8F6B6C853A}"
MediaSets                    = "System\CurrentControlSet\Control\MediaSets"
ActiveMovieCategories        = "CLSID\{da4e3da0-d07d-11d0-bd50-00a0c911ce86}\Instance"
MediaInterfaces              = "System\CurrentControlSet\Control\MediaInterfaces"

