;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 2006-2013 Hauppauge Computer Works, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;   Abstract:
;
;       This is the CX23885/7/8 AVStream video/audio capture driver inf file
;      
;       PCI Express x1 Adapter
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider="Hauppauge"
DriverVer=11/07/2013,1.51.31310
CatalogFile.ntamd64=hcw85b64.cat
DriverPackageType=PlugAndPlay
DriverPackageDisplayName="WinTV (885/7/8)"

[Manufacturer]
"Hauppauge"=Hauppauge,NTamd64

[SourceDisksNames]
1=%p2.InstallDisk%,,,Driver85             ;32/64bit machine, Non-Bit-Specific Components
2=%p2.InstallDisk64%,,,"Driver85\64bit"   ;64bit machine, 64bit components
3=%p2.InstallDiskWOW%,,,"Driver85\WOW64"  ;64bit machine, 32bit components (WOW64)

[SourceDisksFiles]
hcw85enc.rom=1
;hcw85mlC.rom=1
hcw85mlD.rom=1
hcw85bda.sys=2
hcw85enc.ax=2
hcw85prop.ax=2
;;hcwCoIns hcw85CoInstaller.dll=2
hcwcp.ax=2
hcwecppp.ax=2
;;NotFor64 hcwxds.dll=1

[Hauppauge.NTamd64]
; Chesterfield3 OEM - 888/NXP18271/10048 DVB-T Hybrid (SW Encode) + DVBS tuner  
%CX885.M5300%=CX885.M5300_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53000070
%CX885.M5300%=CX885.M5300_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53F00070
%CX885.M5300%=CX885.M5300_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53F10070

; Chesterfield3 Retail - 888/NXP18271/10048 DVB-T Hybrid (SW Encode) + DVBS tuner  
%CX885.M5300%=CX885.M5300_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53080070

; Chesterfield3 OEM - 888/NXP18271/10048 DVB-T Hybrid (SW Encode) + DVBS tuner, No IR/WAke 
%CX885.M5340%=CX885.M5340_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53400070
%CX885.M5340%=CX885.M5340_50,PCI\VEN_14F1&DEV_8880&SUBSYS_53F20070


; Chesterfield4 OEM - 888/NXP18271/Si2165 DVB-T Hybrid (SW Encode) + DVBS2 tuner  
%CX885.MC100%=CX885.MC100_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1000070
%CX885.MC100%=CX885.MC100_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1F00070
;;%CX885.MC100%=CX885.MC100_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1F10070

; Chesterfield4 Retail - 888/NXP18271/Si2165 DVB-C/T Hybrid (SW Encode) + DVBS2 tuner  
%CX885.MC130%=CX885.MC130_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1300070
; Chesterfield4 OEM - 888/NXP18271/Si2165 DVB-C/T Hybrid (SW Encode) + DVBS2 tuner  
%CX885.MC130%=CX885.MC130_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1F80070

; Chesterfield4 OEM - 888/NXP18271/Si2165 DVB-C/T Hybrid (SW Encode) + DVBS2 tuner, Retail IR recv  
%CX885.MC130%=CX885.MC130_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1380070
; Chesterfield4 OEM - 888/NXP18271/Si2165 DVB-T Hybrid (SW Encode) + DVBS2 tuner, Retail IR recv  
;%CX885.MC130%=CX885.MC130_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1xx0070

; Chesterfield4 Retail - 888/NXP18271/Si2165 DVB-T Hybrid (SW Encode) + DVBS2 tuner  
%CX885.MC100%=CX885.MC100_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1080070

; Chesterfield4 OEM - 888/NXP18271/Si2165 DVB-T Hybrid (SW Encode) + DVBS2 tuner, No IR/WAke 
%CX885.MC140%=CX885.MC140_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1400070
;;%CX885.MC140%=CX885.MC140_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C1F20070

; Chesterfield4 - 888 + DVBS2 tuner, Retail IR; Sat Only 
%CX885.MC12A%=CX885.MC12A_50,PCI\VEN_14F1&DEV_8880&SUBSYS_C12A0070


; K4C4 Retail - 888/SI2157/3306 ATSC/QAM Hybrid (SW Encode)
%CX885.M2A18%=CX885.M2A18_50,PCI\VEN_14F1&DEV_8880&SUBSYS_2A180070
; K4C4 Retail - 888/SI2157/Si2168 DVB-T/T2/C Hybrid, FM (SW Encode)
%CX885.M2A28%=CX885.M2A28_50,PCI\VEN_14F1&DEV_8880&SUBSYS_2A280070
; K4C4 Retail - 888/SI2157/Si2168 DVB-T/T2/C + 3306 ATSC/QAM Hybrid (SW Encode)
%CX885.M2A38%=CX885.M2A38_50,PCI\VEN_14F1&DEV_8880&SUBSYS_2A380070


; Coram2 Retail - 888/NXP18271/3305 ATSC/QAM Hybrid tuner (SW Encode)
%CX885.M2211%=CX885.M2211_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22110070
%CX885.M2211%=CX885.M2211_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22190070

; Coram2 OEM - 888/NXP18271/3305 ATSC/QAM Hybrid tuner (SW Encode, A/B switch)
%CX885.M2215%=CX885.M2215_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22150070
%CX885.M2215%=CX885.M2215_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F20070
; Coram2 Retail - 888/NXP18271/3305 ATSC/QAM Hybrid tuner (SW Encode, A/B switch)
%CX885.M2215%=CX885.M2215_50,PCI\VEN_14F1&DEV_8880&SUBSYS_221D0070

; Coram2 OEM - 888/NXP18271/228 ATSC/QAM Hybrid tuner (SW Encode)
%CX885.M2251%=CX885.M2251_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22510070
; Coram2 Retail - 888/NXP18271/228 ATSC/QAM Hybrid tuner (SW Encode)
%CX885.M2251%=CX885.M2251_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22590070
%CX885.M2251%=CX885.M2251_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F10070

; Kingston2 OEM - 888/NXP18271/10048 DVB Hybrid tuner, FM (SW Encode)
%CX885.M2291%=CX885.M2291_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22910070
; Kingston2 Retail - 888/NXP18271/10048 DVB Hybrid tuner, FM (SW Encode)
%CX885.M2291%=CX885.M2291_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22990070
%CX885.M2291%=CX885.M2291_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F00070
; Kingston2 - PCTV 311ix
%CX885.M22F4%=CX885.M2291_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F40070
%CX885.M22F4%=CX885.M2291_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F42013

; Kingston2 OEM - 888/NXP18271/10048 DVB Hybrid tuner, FM (SW Encode, A/B switch)
%CX885.M2295%=CX885.M2295_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22950070
%CX885.M2295%=CX885.M2295_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F30070
; Kingston2 Retail - 888/NXP18271/10048 DVB Hybrid tuner, FM (SW Encode, A/B switch)
%CX885.M2295%=CX885.M2295_50,PCI\VEN_14F1&DEV_8880&SUBSYS_229D0070
; Kingston2 - PCTV 311ix
%CX885.M22F4%=CX885.M2295_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F50070
%CX885.M22F4%=CX885.M2295_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22F52013

; Kingston2 OEM - 888/NXP18271/8295/10048 DVB Hybrid tuner (SW Encode)
%CX885.M22D1%=CX885.M22D1_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22D10070
; Kingston2 OEM - 888/NXP18271/8295/10048 DVB Hybrid tuner (SW Encode, No FP header)
%CX885.M22D3%=CX885.M22D3_50,PCI\VEN_14F1&DEV_8880&SUBSYS_22D30070

; Kingston - Zarlink353, Xc3028, 417 MPEG2 Encoder
%CX885.M7100%=CX885.M7100,PCI\VEN_14F1&DEV_8852&SUBSYS_71000070
; Kingston - Zarlink353, Xc3028, 417 MPEG2 Encoder, No FM
%CX885.M7101%=CX885.M7101,PCI\VEN_14F1&DEV_8852&SUBSYS_71010070
; Kingston Lite - Zarlink353, Xc3028 (SW Encode)
%CX885.M7110%=CX885.M7110,PCI\VEN_14F1&DEV_8852&SUBSYS_71100070
; Kingston PVR - Xc3028, 417 MPEG2 Encoder
%CX885.M7120%=CX885.M7120,PCI\VEN_14F1&DEV_8852&SUBSYS_71200070
; Kingston GO - Xc3028 (SW Encode)
%CX885.M7130%=CX885.M7130,PCI\VEN_14F1&DEV_8852&SUBSYS_71300070
; Kingston VCB - No tuner (Analog baseband only)
%CX885.M7133%=CX885.M7133,PCI\VEN_14F1&DEV_8852&SUBSYS_71330070

; Kingston (aka Dover-e) - NXP8275A/8290 DVB Hybrid tuner, 417 MPEG2 Encoder
%CX885.M7108%=CX885.M7108,PCI\VEN_14F1&DEV_8852&SUBSYS_71080070
; Kingston Lite (aka Oxford-e) - NXP8275A/8290 DVB Hybrid tuner (SW Encode)
%CX885.M7118%=CX885.M7118,PCI\VEN_14F1&DEV_8852&SUBSYS_71180070
; Kingston PVR (aka Roslyn-e) - NXP8275A/8290 tuner (HW Encode, Analog only)
%CX885.M7128%=CX885.M7128,PCI\VEN_14F1&DEV_8852&SUBSYS_71280070
; Kingston GO (aka Pluto-e) - NXP8275A/8290 tuner (SW Encode, Analog only)
%CX885.M7138%=CX885.M7138,PCI\VEN_14F1&DEV_8852&SUBSYS_71380070

; Kingston (aka Dover-e) - NXP8275A/8295 DVB Hybrid tuner, 417 MPEG2 Encoder
%CX885.M7148%=CX885.M7148,PCI\VEN_14F1&DEV_8852&SUBSYS_71480070
; Kingston Lite (aka Oxford-e) - NXP8275A/8295 DVB Hybrid tuner (SW Encode)
%CX885.M7158%=CX885.M7158,PCI\VEN_14F1&DEV_8852&SUBSYS_71580070
; Kingston PVR (aka Roslyn-e) - NXP8275A/8295 tuner (HW Encode, Analog only)
%CX885.M7168%=CX885.M7168,PCI\VEN_14F1&DEV_8852&SUBSYS_71680070
; Kingston GO (aka Pluto-e) - NXP8275A/8290 tuner (SW Encode, Analog only)
%CX885.M7178%=CX885.M7178,PCI\VEN_14F1&DEV_8852&SUBSYS_71780070

; Kingston (aka Dover-e) - NXP18271/8295/10046 DVB Hybrid tuner, 417 MPEG2 Encoder
%CX885.M7141%=CX885.M7141,PCI\VEN_14F1&DEV_8852&SUBSYS_71410070
; Kingston Lite (aka Oxford-e) - NXP18271/8295/10046 DVB Hybrid tuner (SW Encode)
%CX885.M7151%=CX885.M7151,PCI\VEN_14F1&DEV_8852&SUBSYS_71510070
; Kingston-05 Lite (aka Oxford-e) - NXP18271/8295 tuner (SW Encode)
%CX885.M7173%=CX885.M7173,PCI\VEN_14F1&DEV_8852&SUBSYS_71730070
; Kingston-05 Lite (aka Oxford-e) - NXP18271/8295/10048 DVB Hybrid tuner (SW Encode)
%CX885.M71D1%=CX885.M71D1,PCI\VEN_14F1&DEV_8852&SUBSYS_71D10070
; Kingston-05 Lite 887 (aka Oxford-e) - NXP18271/8295/10048 DVB Hybrid tuner (SW Encode)
%CX885.M71D1%=CX885.M71D1_25,PCI\VEN_14F1&DEV_8880&SUBSYS_71D10070
; Kingston-05 Lite (aka Oxford-e) - NXP18271/8295/10048 DVB Hybrid tuner (SW Encode, No FP header)
%CX885.M71D3%=CX885.M71D3,PCI\VEN_14F1&DEV_8852&SUBSYS_71D30070
; Kingston-05 Lite 887 (aka Oxford-e) - NXP18271/8295/10048 DVB Hybrid tuner (SW Encode, No FP header)
%CX885.M71D3%=CX885.M71D3_25,PCI\VEN_14F1&DEV_8880&SUBSYS_71D30070


; Brentwood - 8275A+8295+417 MPEG2 Encoder, + MT2161/CX24227  ATSC Combo
%CX885.M7600%=CX885.M7600,PCI\VEN_14F1&DEV_8852&SUBSYS_76000070
; Brentwood Lite - 8275A+8295+(SW encode), + MT2161/CX24227  ATSC Combo
%CX885.M7610%=CX885.M7610,PCI\VEN_14F1&DEV_8852&SUBSYS_76100070


; Melville - CX24277, Xc3028 (ATSC/NTSC Hybrid, SW Encode)
%CX885.M7710%=CX885.M771x,PCI\VEN_14F1&DEV_8852&SUBSYS_77100070
%CX885.M7717%=CX885.M771x,PCI\VEN_14F1&DEV_8852&SUBSYS_77170070
; Melville-Q - CX24277, Xc5000 (ATSC/QAM/NTSC Hybrid, SW Encode)
%CX885.M7790%=CX885.M779x,PCI\VEN_14F1&DEV_8852&SUBSYS_77900070
%CX885.M7797%=CX885.M779x,PCI\VEN_14F1&DEV_8852&SUBSYS_77970070


; Medford - 18271/8295/417 MPEG2 Encoder, MT2131/CX24227  NTSC/ATSC/QAM Combo
%CX885.M7800%=CX885.M7800,PCI\VEN_14F1&DEV_8880&SUBSYS_78000070
; Medford - 18271/8295/417 MPEG2 Encoder, MT2131/CX24227  NTSC/ATSC/QAM Combo
%CX885.M7801%=CX885.M7801,PCI\VEN_14F1&DEV_8880&SUBSYS_78010070
; Medford - 18271/8295/417 MPEG2 Encoder, MT2131/CX24227  NTSC/ATSC/QAM Combo/No FM
%CX885.M7809%=CX885.M7809,PCI\VEN_14F1&DEV_8880&SUBSYS_78090070
; Medford Lite - 18271/8295 \, MT2131/CX24227  NTSC/ATSC/QAM Combo (SW Encode)
%CX885.M7810%=CX885.M771x,PCI\VEN_14F1&DEV_8880&SUBSYS_78100070
; Medford Lite - 18271/8295 \, MT2131/CX24227  NTSC/ATSC/QAM Combo (SW Encode)
%CX885.M7811%=CX885.M7811,PCI\VEN_14F1&DEV_8880&SUBSYS_78110070


; Coram - 887, MT2131/TDA9885/CX24227 NTSC/ATSC/QAM Hybrid tuner (SW Encode)
%CX885.M7911%=CX885.M7911_25,PCI\VEN_14F1&DEV_8880&SUBSYS_79110070
; Coram - 885, MT2131/TDA9885/CX24227 NTSC/ATSC/QAM Hybrid tuner (SW Encode)
%CX885.M7911%=CX885.M7911,PCI\VEN_14F1&DEV_8852&SUBSYS_79110070


; Whitman - Dib7000pc, Xc3028L (DVBT/PAL Hybrid, SW Encode)
%CX885.M8010%=CX885.M801x,PCI\VEN_14F1&DEV_8852&SUBSYS_80100070
%CX885.M8017%=CX885.M801x,PCI\VEN_14F1&DEV_8852&SUBSYS_80170070

%CX885.M8050%=CX885.M805x,PCI\VEN_14F1&DEV_8852&SUBSYS_80500070
%CX885.M8056%=CX885.M805x,PCI\VEN_14F1&DEV_8852&SUBSYS_80560070
%CX885.M8057%=CX885.M805x,PCI\VEN_14F1&DEV_8852&SUBSYS_80570070


; Whitney - 885, NXP18271/8295/10048 DVB Hybrid tuner, 417 MPEG2 Encoder
%CX885.M8101%=CX885.M8101,PCI\VEN_14F1&DEV_8852&SUBSYS_81010070
; Whitney - 887, NXP18271/8295/10048 DVB Hybrid tuner, 417 MPEG2 Encoder
%CX885.M8101%=CX885.M8101_25,PCI\VEN_14F1&DEV_8880&SUBSYS_81010070


; Medford2 - 18271/8295/417 MPEG2 Encoder, 18271/CX24228  NTSC/ATSC/QAM Combo
%CX885.M8501%=CX885.M8501,PCI\VEN_14F1&DEV_8880&SUBSYS_85010070
; Medford2 - 18271/417 MPEG2 Encoder, 18271/CX24228  NTSC/ATSC/QAM Combo
%CX885.M8541%=CX885.M8541,PCI\VEN_14F1&DEV_8880&SUBSYS_85410070
; Medford2Lite - 18271/CX24228  NTSC/ATSC/QAM Combo, SW encode
%CX885.M8551%=CX885.M8551,PCI\VEN_14F1&DEV_8880&SUBSYS_85510070
; Medford2Hyb - 18271/CX24228  NTSC/ATSC/QAM Hybrid
%CX885.M8571%=CX885.M8571,PCI\VEN_14F1&DEV_8880&SUBSYS_85710070



;Production test - EEprom programming only
;%CX23885.Blank%=CX885.M7138,PCI\VEN_14F1&DEV_8852
;%CX23887.Blank%=CX885.M71D1_25,PCI\VEN_14F1&DEV_8880&REV_02
;%CX23888.Blank%=CX885.M8571,PCI\VEN_14F1&DEV_8880&REV_03
;%CX23888.Blank%=CX885.M8571,PCI\VEN_14F1&DEV_8880&REV_04
;%CX23887.Blank%=CX885.M71D1_25,PCI\VEN_14F1&DEV_8880&REV_0E
;%CX23887.Blank%=CX885.M71D1_25,PCI\VEN_14F1&DEV_8880&REV_0F

; Sonora Ref board - Zarlink353, Xc3028 EVK/417 MPEG2 Encoder
;%CX23885.Sonora%=CX885.M7100,PCI\VEN_14F1&DEV_8852&SUBSYS_003714F1



[CX885.M5300_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M5300.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M5300_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M5300.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M5340_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M5340.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M5340_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M5340.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL



[CX885.MC100_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC100.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.MC100_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC100.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.MC12A_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CXTS.AddReg,MC12A.AddReg,LNB.AddReg,Xtal50.Addreg,CX885.CapOnly.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.MC12A_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CXTS.AddReg,MC12A.AddReg,LNB.AddReg,Xtal50.Addreg,CX885.CapOnly.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.MC130_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC130.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.MC130_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC130.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.MC140_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC140.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.MC140_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,MC140.AddReg,LNB.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL



[CX885.M2211_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2211.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2211_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2211.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M2215_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2215.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2215_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2215.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M2251_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2251.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2251_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2251.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL



[CX885.M2291_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2291.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2291_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2291.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2295_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2295.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2295_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M2295.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M22D1_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M22D1.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M22D1_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M22D1.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M22D3_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M22D3.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M22D3_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M22D3.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL



[CX885.M2A18_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Si2157.AddReg,CXTS.AddReg,M2A18.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2A18_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Si2157.AddReg,CXTS.AddReg,M2A18.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M2A28_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Si2157.AddReg,CXTS.AddReg,M2A28.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2A28_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Si2157.AddReg,CXTS.AddReg,M2A28.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M2A38_50]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Si2157.AddReg,CXTS.AddReg,M2A38.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M2A38_50.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Si2157.AddReg,CXTS.AddReg,M2A38.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL




[CX885.M7100]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7100.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7100.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7100.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7101]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7101.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7101.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7101.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7110]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7110.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7110.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7110.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7120]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7120.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7120.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7120.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7130]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7130.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7130.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M7130.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7108]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,CXTS.AddReg,M7108.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7108.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,CXTS.AddReg,M7108.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7118]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,CXTS.AddReg,M7118.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7118.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,CXTS.AddReg,M7118.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7128]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,M7128.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7128.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290DVB.AddReg,M7128.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7133]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_VCB_NoFP_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,M7133.AddReg,CX885.wave.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7133.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_VCB_NoFP_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,M7133.AddReg,CX885.wave.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7138]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290.AddReg,M7138.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7138.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8290.AddReg,M7138.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7141]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7141.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7141.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7141.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7148]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295DVB.AddReg,CXTS.AddReg,M7148.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7148.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295DVB.AddReg,CXTS.AddReg,M7148.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7151]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7151.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7151.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7151.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7158]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295DVB.AddReg,CXTS.AddReg,M7158.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7158.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295DVB.AddReg,CXTS.AddReg,M7158.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7168]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295.AddReg,M7168.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7168.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295.AddReg,M7168.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7173]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7173.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7173.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7173.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7178]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295.AddReg,M7178.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7178.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp8295.AddReg,M7178.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M71D1]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D1.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M71D1.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D1.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M71D1_25]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D1.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M71D1_25.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D1.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M71D3]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D3.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M71D3.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D3.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M71D3_25]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D3.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M71D3_25.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP_NoYPrPb.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M71D3.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7600]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtNTSC.AddReg,Nxp8295.AddReg,CXTS.AddReg,M7600.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7600.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtNTSC.AddReg,Nxp8295.AddReg,CXTS.AddReg,M7600.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7610]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtNTSC.AddReg,Nxp8295.AddReg,CXTS.AddReg,M7610.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7610.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtNTSC.AddReg,Nxp8295.AddReg,CXTS.AddReg,M7610.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M771x]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtNTSC.AddReg,Xceive.AddReg,CXTS.AddReg,M7717.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

;;hcwCoIns [CX885.M771x.CoInstallers] 
;;hcwCoIns AddReg=hcwCoInstallers.AddReg
;;hcwCoIns CopyFiles=hcwCoInstallers.CopyFiles

[CX885.M771x.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtNTSC.AddReg,Xceive.AddReg,CXTS.AddReg,M7717.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

;;hcwCoIns [CX885.M771x.NT.CoInstallers] 
;;hcwCoIns AddReg=hcwCoInstallers.AddReg
;;hcwCoIns CopyFiles=hcwCoInstallers.CopyFiles

[CX885.M779x]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtNTSC.AddReg,Xceive.AddReg,CXTS.AddReg,M7797.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M779x.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtNTSC.AddReg,Xceive.AddReg,CXTS.AddReg,M7797.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7800]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7800.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7800.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7800.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7801]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7801.AddReg,Xtal25.Addreg,CX885.wave.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7801.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7801.AddReg,Xtal25.Addreg,CX885.wave.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7809]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7809.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7809.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7809.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7811]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7811.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7811.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M7811.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M7911]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,MT2131.AddReg,CXTS.AddReg,M7911.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7911.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,MT2131.AddReg,CXTS.AddReg,M7911.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7911_25]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,MT2131.AddReg,CXTS.AddReg,M7911.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M7911_25.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,MT2131.AddReg,CXTS.AddReg,M7911.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M801x]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M801x.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M801x.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M801x.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M805x.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M805x.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M805x]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoFP.AddReg,CX885.FmtPAL.AddReg,Xceive.AddReg,CXTS.AddReg,M805x.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8101]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8101.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8101.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8101.AddReg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8101_25]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8101.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8101_25.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_All.AddReg,CX885.FmtPAL.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8101.AddReg,Xtal25.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8501]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8501.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8501.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8501.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8541]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8541.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8541.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8541.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8551]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8551.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8551.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8551.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL


[CX885.M8571]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration, WDMAUDIO.Registration, BDA.Registration,bda.Installation
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8571.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL

[CX885.M8571.NT]
Include=    ks.inf, kscaptur.inf, wdmaudio.inf, bda.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, WDMAUDIO.Registration, BDA.Registration,bda.Installation.NT
AddReg=     CX885.AddReg,CX885XBAR.AddReg,CX885XBAR_NoYPrPb.AddReg,CX885.FmtNTSC.AddReg,Nxp18271.AddReg,CXTS.AddReg,M8571.AddReg,Xtal50.Addreg
DelReg=     Mxxxx.DelReg
CopyFiles=  CX885.CopyDrivers,DSFilters.CopyFiles
RegisterDlls=DSFilters.RegDLL



[DestinationDirs]
CX885.CopyDrivers=10,system32\drivers
DSFilters.CopyFiles=11
;;hcwCoIns hcwCoInstallers.CopyFiles=11

[CX885.CopyDrivers]
HCW85BDA.sys
hcw85enc.rom
;; Merlin Rev. C audio firmware
;hcw85mlC.rom
;; Merlin Rev. D audio firmware
hcw85mlD.rom

[DSFilters.CopyFiles]
hcw85enc.ax
hcw85prop.ax
hcwcp.ax
hcwecppp.ax
;;NotFor64 hcwxds.dll

[DSFilters.RegDLL]
11,,hcw85enc.ax,1
11,,hcw85prop.ax,1
11,,hcwcp.ax,1
11,,hcwecppp.ax,1
;;NotFor64 11,,hcwxds.dll,1

;;hcwCoIns [hcwCoInstallers.CopyFiles]
;;hcwCoIns hcw85CoInstaller.dll

;;hcwCoIns [hcwCoInstallers.AddReg]
;;hcwCoIns HKR,,CoInstallers32,0x00010000,"hcw85CoInstaller,CoInstallerEntry"

[CX885.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,HCW85BDA.sys
HKR,,OkToHibernate,3,01
; Disable driver page out
HKR,,PageOutWhenUnopened,3,0
;HKR,,PageOutWhenUnopened,3,01
HKR,,DontSuspendIfStreamsAreRunning,3,01
HKLM,%MediaCategories%\%GUID.PINNAME_ANALOG_AUDIO_IN%,Name,,%Pin.p2AnalogAudioIn%
HKLM,%MediaCategories%\%GUID.PINNAME_AUDIO_OUT%,Name,,%PinName.AnalogAudioOut%
; Can do this here or in the driver; useful for ExpressCard devices
;HKR,,SurpriseRemovalOK,0x00010001,1
HKLM,%Services%\HCW85BDA\Parameters,UseRegisterAdapterObjectEx,0x00010001, 0x01, 0x00, 0x00, 0x00

;Copy protection method enforced by driver
HKR,"DriverData","CpMethod",0x00010001, 0xFE, 0x00, 0x00, 0x00

;Set ASPM mode
HKR,"DriverData","SetASPMState",0x00010001, 0x00, 0x00, 0x00, 0x00

;
;Register the name of the 656 and MPEG pins
;
HKLM,%MediaCategories%\%GUID.PINNAME_656_OUT%,Name,,%PinName.656_OUT%
HKLM,%MediaCategories%\%GUID.PINNAME_656_IN%,Name,,%PinName.656_IN%
HKLM,%MediaCategories%\%GUID.PINNAME_MPEG_OUT%,Name,,%PinName.MpegOut%

;
;Add the property pages
;
HKCR,CLSID\%GUID.GenEnc_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.GenEnc_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.GenEnc_Properties%,,,

HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Video_Properties%,,,

HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Audio_Properties%,,,

HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.MPEG_Properties%,,,

HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Diagnostic_Properties%,,,

HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,,,hcw85enc.ax
HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Noise_Properties%,,,

;Register the encoder and multiplexer classes with Direct X
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,CLSID,,%GUID.Encoder%
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,FriendlyName,,%Category_Encoders%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,CLSID,,%GUID.Multiplexer%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,FriendlyName,,%Category_Multiplexers%

;Register the names of the encoder and multiplexer nodes
HKLM,%MediaCategories%\%GUID.Encoder%,Name,,%Node.Encoder%
HKLM,%MediaCategories%\%GUID.Encoder%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%GUID.Multiplexer%,Name,,%Node.Multiplexer%
HKLM,%MediaCategories%\%GUID.Multiplexer%,Display,1,00,00,00,00




;SliceCC
HKR,"DriverData","EnableSliceCC",0x00010001, 0x01, 0x00, 0x00, 0x00


; these registry keys for 3D comb filter enable
; use3DComb entry allows the use of the 3D Comb feature, currently connected to the color enable
; property of the capture filter
HKR,"DriverData","Use3DComb",0x00010001, 0x01,0x00,0x00,0x00

; this entry sets the initial state of the 3D comb enable when use3DComb is specified
HKR,"DriverData","Enable3DComb",0x00010001, 0x01,0x00,0x00,0x00

;Enable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1E, 0x00, 0x00, 0x00

; these registry keys for TS filter
; DebugTS entry forces creation of TS capture filter without a demod
;HKR,"DriverData","DebugTS",0x00010001, 0x01,0x00,0x00,0x00
; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsTSStream",0x00010001,0x01,0x00,0x00,0x00

; this registry keys for the FixNMI option which takes care of the BSODs in the 
; ICH6/7 chipsets
HKR,"DriverData","FixNMIBit",0x00010001, 0x00,0x00,0x00,0x00

;IR Support (default to EEprom based)
;;;HKR,"DriverData","EnableIR",0x00010001, 0x01, 0x00, 0x00, 0x00
;NEC standard (not used by driver)
;;HKR,"DriverData","IRStandard",0x00010001, 0x01, 0x00, 0x00, 0x00

;Add the property pages
HKCR,CLSID\%GUID.Corona_Properties%\InprocServer32,,,hcw85prop.ax
HKCR,CLSID\%GUID.Corona_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.CORONA_VERSION_PROPERTIES%\PropertyPages\%GUID.Corona_Properties%,,,

; GPIO Pin values
;;HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
;;HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

;Demod Comm mode : 0x00 = Serial, 0x01 = Parallel
HKR,"DriverData","DemodTransferMode",0x00010001, 0x00, 0x00, 0x00, 0x00


;HKR,"DriverData","IsMCE",0x00010001, 0x00,0x00,0x00,0x00

; Static Temporal filter, level=4
HKR,"DriverData","StaticTemporalLevel",0x00010001, 0x04, 0x00, 0x00, 0x00
HKR,"DriverData","IsStaticTemporal",0x00010001, 0x01, 0x00, 0x00, 0x00

; Back Panel = 0x00, Front Panel = 0x01
HKR,"DriverData","comp_select_panel", 0x00010001, 0x00, 0x00, 0x00, 0x00

; Use DriverTunes strategy by default
HKR,"DriverData","TunerUsePllTuningStrategy", 0x00010001, 0x00, 0x00, 0x00, 0x00
; Enable AutoAFC for all boards???
;HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


; save our driver version for reference
HKLM,Software\Hauppauge\WDM\Version,,0x4000,"1.46.28154"

HKLM,Software\Hauppauge\hcwTVWnd,"VCapFilter",0x4000,"%VIDFriendlyName%"


[CX885.wave.AddReg]
;Wave in audio device registration
HKR,,AssociatedFilters,,"wdmaud,redbook"
HKR,Drivers,SubClasses,,"wave,mixer"
HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\wave\wdmaud.drv,Description,,%WaveFriendlyName%

HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Description,,%WaveFriendlyName%

HKR,"DriverData","CreateAudioFilter",0x00010001, 0x01, 0x00, 0x00, 0x00

;
; Driver Configuration Registry Entries
;

[CX885.FmtPAL.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x10,0x00,0x00,0x00

[CX885.FmtNTSC.AddReg]
HKR,"DriverData","VideoStandard",0x00010001, 0x01,0x00,0x00,0x00

[CX885.NoAnalog.AddReg]
HKR,"DriverData","CreateAnalogFilters",0x00010001, 0x00,0x00,0x00,0x00

[CX885.CapOnly.AddReg]
HKR,"DriverData","CreateAnalogFilters",0x00010001, 0x01,0x00,0x00,0x00


;-------------------------------------------------------------------
; Crossbar AddReg sections
;
;---Crossbar registry values---
;
; Note: For each pin on the crossbar, specify the following:
; (1) Pin type 
;     0 - TunerIn
;     1 - Composite 1
;     2 - SVideo 1
;     3 - Component
;     4 - Composite 2
;     5 - SVideo 2
;     6 - Audio from Tuner
;     7 - Audio from Line In
;     8 - Audio from Line In 2
; (2) InputMux (optional) - input mux to use for the selected pin
;     in 0xAA, 0xBB, 0xCC, 0x00 format
;     where AA is the input mux for Composite/S-Video Luma/Component Luma
;           BB is the input mux for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input mux for Component YPb
; (3) InputChannel (optional, but required if InputMux present) - Input channel 
;     to use for mux in 0xAA, 0xBB, 0xCC, 0xDD format
;     where AA is the input channel for Composite/S-Video Luma/Component Luma
;           BB is the input channel for Tuner Audio/S-Video Chroma/Component YPr
;           CC is the input channel for Component YPb 
;           DD = 1 if dual ADC2 mode required, zero if single mode
; (4) RelatedPinIndex 

;-------------------------------------------------------------------

[CX885XBAR_All.AddReg]
HKR,"DriverData","XbarType",0x00010001, 0x00,0x00,0x00,0x00
;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

[CX885XBAR_NoYPrPb.AddReg]
HKR,"DriverData","XbarType",0x00010001, 0x01,0x00,0x00,0x00
;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

[CX885XBAR_NoFP.AddReg]
HKR,"DriverData","XbarType",0x00010001, 0x02,0x00,0x00,0x00
;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

[CX885XBAR_NoFP_NoYPrPb.AddReg]
HKR,"DriverData","XbarType",0x00010001, 0x03,0x00,0x00,0x00
;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00

[CX885XBAR_VCB_NoFP_NoYPrPb.AddReg]
HKR,"DriverData","XbarType",0x00010001, 0x04,0x00,0x00,0x00
;Composite input is the default
HKR,"DriverData","VideoInputPin",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","ForceAudioWithVideoPin",0x00010001, 0x01,0x00,0x00,0x00


[CX885XBAR.AddReg]
;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin6 
HKR,"DriverData\XBarPin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBarPin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBarPin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin0","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN6 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin1","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBarPin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBarPin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBarPin2","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 3 - Component 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN6 for YPb, VIN7 for YPr
; Input Channel   : Ch1 for  Lume, Ch2  for YPb, Ch3  for YPr, Dual ADC
; Related PinIndex: Audio Line In 1 - Pin7
HKR,"DriverData\XBarPin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBarPin3","InputMux",0x00010001, 0x08,0x06,0x07,0x00
HKR,"DriverData\XBarPin3","InputChannel",0x00010001, 0x01,0x02,0x03,0x01
HKR,"DriverData\XBarPin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - Composite 2 (Front) 
; Input Mux       : VIN1 for Composite 
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin4","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBarPin4","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 5 - S-Video 2 (Front)
; Input Mux       : VIN3 for Luma, VIN4 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin8
HKR,"DriverData\XBarPin5","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBarPin5","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBarPin5","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBarPin5","RelatedPinIndex",0x00010001, 0x08,0x00,0x00,0x00

;Pin 6 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBarPin6","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBarPin6","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 7 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBarPin7","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBarPin7","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 8 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin4
HKR,"DriverData\XBarPin8","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBarPin8","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 9 - Audio SPDIF in 
;;HKR,"DriverData\XBarPin9","PinType",0x00010001, 0x09,0x00,0x00,0x00
;;HKR,"DriverData\XBarPin9","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00


;[CX885XBAR_NoYPrPb.AddReg]
;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin5 
HKR,"DriverData\XBar1Pin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBar1Pin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBar1Pin0","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN6 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBar1Pin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin1","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin6
HKR,"DriverData\XBar1Pin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBar1Pin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBar1Pin2","RelatedPinIndex",0x00010001, 0x06,0x00,0x00,0x00

;Pin 3 - Composite 2 (Front) 
; Input Mux       : VIN1 for Composite 
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBar1Pin3","PinType",0x00010001, 0x04,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin3","InputMux",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin3","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin3","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 4 - S-Video 2 (Front)
; Input Mux       : VIN3 for Luma, VIN4 for Chroma
; Input Channel   : Ch1 for  Luma, Ch2  for Chroma
; Related PinIndex: Audio Line In 2 - Pin7
HKR,"DriverData\XBar1Pin4","PinType",0x00010001, 0x05,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin4","InputMux",0x00010001, 0x03,0x04,0x00,0x00
HKR,"DriverData\XBar1Pin4","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBar1Pin4","RelatedPinIndex",0x00010001, 0x07,0x00,0x00,0x00

;Pin 5 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBar1Pin5","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin5","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 6 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBar1Pin6","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin6","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00

;Pin 7 - Audio Line In 2 (Front)
; Related PinIndex: Composite 2 - Pin3
HKR,"DriverData\XBar1Pin7","PinType",0x00010001, 0x08,0x00,0x00,0x00
HKR,"DriverData\XBar1Pin7","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00


;[CX885XBAR_NoFP.AddReg]
;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin4 
HKR,"DriverData\XBar2Pin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBar2Pin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBar2Pin0","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN6 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin5
HKR,"DriverData\XBar2Pin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin1","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin5
HKR,"DriverData\XBar2Pin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBar2Pin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBar2Pin2","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 3 - Component 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN6 for YPb, VIN7 for YPr
; Input Channel   : Ch1 for  Lume, Ch2  for YPb, Ch3  for YPr, Dual ADC
; Related PinIndex: Audio Line In 1 - Pin5
HKR,"DriverData\XBar2Pin3","PinType",0x00010001, 0x03,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin3","InputMux",0x00010001, 0x08,0x06,0x07,0x00
HKR,"DriverData\XBar2Pin3","InputChannel",0x00010001, 0x01,0x02,0x03,0x01
HKR,"DriverData\XBar2Pin3","RelatedPinIndex",0x00010001, 0x05,0x00,0x00,0x00

;Pin 4 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBar2Pin4","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin4","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 5 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBar2Pin5","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBar2Pin5","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00


;[CX885XBAR_NoFP_NoYPrPb.AddReg]
;Pin 0 - Tuner In
; Input MUX       : VIN2 for video, VIN5 for audio
; Input Channel   : Ch1 for video,  Ch2  for audio
; Related PinIndex: Tuner Audio - Pin3 
HKR,"DriverData\XBar3Pin0","PinType",0x00010001, 0x00,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin0","InputMux",0x00010001, 0x02,0x05,0x00,0x00
HKR,"DriverData\XBar3Pin0","InputChannel",0x00010001, 0x01,0x02,0x00,0x00
HKR,"DriverData\XBar3Pin0","RelatedPinIndex",0x00010001, 0x03,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN6 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBar3Pin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin1","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 2 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin4
HKR,"DriverData\XBar3Pin2","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin2","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBar3Pin2","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBar3Pin2","RelatedPinIndex",0x00010001, 0x04,0x00,0x00,0x00

;Pin 3 - Tuner Audio
; Related PinIndex: Tuner In - Pin0
HKR,"DriverData\XBar3Pin3","PinType",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin3","RelatedPinIndex",0x00010001, 0x00,0x00,0x00,0x00

;Pin 4 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBar3Pin4","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBar3Pin4","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00


;[CX885XBAR_VCB_NoFP_NoYPrPb.AddReg]
;Pin 0 - S-Video 1 (Rear)
; Input Mux       : VIN8 for Luma, VIN7 for Chroma
; Input Channel   : Ch1 for  Luma, Ch3  for Chroma
; Related PinIndex: Audio Line In 1 - Pin2
HKR,"DriverData\XBar4Pin0","PinType",0x00010001, 0x02,0x00,0x00,0x00
HKR,"DriverData\XBar4Pin0","InputMux",0x00010001, 0x08,0x07,0x00,0x00
HKR,"DriverData\XBar4Pin0","InputChannel",0x00010001, 0x01,0x03,0x00,0x00
HKR,"DriverData\XBar4Pin0","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00

;Pin 1 - Composite 1 (Rear)
; Input Mux       : VIN6 for Composite
; Input Channel   : Ch1 for Composite
; Related PinIndex: Audio Line In 1 - Pin2
HKR,"DriverData\XBar4Pin1","PinType",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar4Pin1","InputMux",0x00010001, 0x06,0x00,0x00,0x00
HKR,"DriverData\XBar4Pin1","InputChannel",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData\XBar4Pin1","RelatedPinIndex",0x00010001, 0x02,0x00,0x00,0x00

;Pin 2 - Audio Line In 1 (Rear)
; Related PinIndex: Composite 1 - Pin1
HKR,"DriverData\XBar4Pin2","PinType",0x00010001, 0x07,0x00,0x00,0x00
HKR,"DriverData\XBar4Pin2","RelatedPinIndex",0x00010001, 0x01,0x00,0x00,0x00




;-------------------------------------------------------------------
; Tuner AddReg sections
;-------------------------------------------------------------------

[Xceive.AddReg]


[Nxp8290.AddReg]


[Nxp8290DVB.AddReg]


[Nxp8295.AddReg]


[Nxp8295DVB.AddReg]


[Nxp18271.AddReg]
HKR,"Parameters","TDA18271_DCToDCSetting",  0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_DCToDCSetting",0x00010001, 0x00, 0x00, 0x00, 0x00


[MT2131.AddReg]


[Si2157.AddReg]



;-------------------------------------------------------------------
; AddReg sections for TS filter
;-------------------------------------------------------------------

[CXTS.AddReg]
HKLM,%MediaCategories%\%TSPinID%,Display,1, 00,00,00,00
HKLM,%MediaCategories%\%TSPinID%,Name,,%TSPinName%

;
; Interfaces installation
;

;
; Video
;
[CX885.M5300_50.Interfaces]
Needs=TriMode.Interfaces
[CX885.M5300_50.NT.Interfaces]
Needs=TriMode.Interfaces

[CX885.M5340_50.Interfaces]
Needs=TriMode.Interfaces
[CX885.M5340_50.NT.Interfaces]
Needs=TriMode.Interfaces

[CX885.MC100_50.Interfaces]
Needs=TriMode.Interfaces
[CX885.MC100_50.NT.Interfaces]
Needs=TriMode.Interfaces

[CX885.MC12A_50.Interfaces]
Needs=Sat.Interfaces
[CX885.MC12A_50.NT.Interfaces]
Needs=Sat.Interfaces

[CX885.MC130_50.Interfaces]
Needs=QuadMode.Interfaces
[CX885.MC130_50.NT.Interfaces]
Needs=QuadMode.Interfaces

[CX885.MC140_50.Interfaces]
Needs=TriMode.Interfaces
[CX885.MC140_50.NT.Interfaces]
Needs=TriMode.Interfaces

[CX885.M2211_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2211_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M2215_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2215_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M2251_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2251_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M2291_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2291_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M2295_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2295_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M22D1_50.Interfaces]
Needs=VID.Interfaces
[CX885.M22D1_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M22D3_50.Interfaces]
Needs=VID.Interfaces
[CX885.M22D3_50.NT.Interfaces]
Needs=VID.Interfaces


[CX885.M2A18_50.Interfaces]
Needs=VID.Interfaces
[CX885.M2A18_50.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M2A28_50.Interfaces]
Needs=QuadMode.Interfaces
[CX885.M2A28_50.NT.Interfaces]
Needs=QuadMode.Interfaces

[CX885.M2A38_50.Interfaces]
Needs=QuadMode.Interfaces
[CX885.M2A38_50.NT.Interfaces]
Needs=QuadMode.Interfaces


[CX885.M7100.Interfaces]
Needs=VID.Interfaces
[CX885.M7100.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7101.Interfaces]
Needs=VID.Interfaces
[CX885.M7101.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7110.Interfaces]
Needs=VID.Interfaces
[CX885.M7110.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7120.Interfaces]
Needs=VID.Interfaces
[CX885.M7120.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7130.Interfaces]
Needs=VID.Interfaces
[CX885.M7130.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7108.Interfaces]
Needs=VID.Interfaces
[CX885.M7108.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7118.Interfaces]
Needs=VID.Interfaces
[CX885.M7118.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7128.Interfaces]
Needs=VID.Interfaces
[CX885.M7128.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7133.Interfaces]
Needs=VID.Interfaces,Wave.Interfaces
[CX885.M7133.NT.Interfaces]
Needs=VID.Interfaces,Wave.Interfaces

[CX885.M7138.Interfaces]
Needs=VID.Interfaces
[CX885.M7138.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7141.Interfaces]
Needs=VID.Interfaces
[CX885.M7141.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7148.Interfaces]
Needs=VID.Interfaces
[CX885.M7148.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7151.Interfaces]
Needs=VID.Interfaces
[CX885.M7151.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7158.Interfaces]
Needs=VID.Interfaces
[CX885.M7158.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7168.Interfaces]
Needs=VID.Interfaces
[CX885.M7168.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7173.Interfaces]
Needs=VID.Interfaces
[CX885.M7173.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7178.Interfaces]
Needs=VID.Interfaces
[CX885.M7178.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M71D1.Interfaces]
Needs=VID.Interfaces
[CX885.M71D1.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M71D1_25.Interfaces]
Needs=VID.Interfaces
[CX885.M71D1_25.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M71D3.Interfaces]
Needs=VID.Interfaces
[CX885.M71D3.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M71D3_25.Interfaces]
Needs=VID.Interfaces
[CX885.M71D3_25.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7600.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces
[CX885.M7600.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces

[CX885.M7610.Interfaces]
Needs=VIDCombo.Interfaces
[CX885.M7610.NT.Interfaces]
Needs=VIDCombo.Interfaces

[CX885.M771x.Interfaces]
Needs=VIDCombo.Interfaces
[CX885.M771x.NT.Interfaces]
Needs=VIDCombo.Interfaces

[CX885.M779x.Interfaces]
Needs=VIDCombo.Interfaces
[CX885.M779x.NT.Interfaces]
Needs=VIDCombo.Interfaces

[CX885.M7800.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces
[CX885.M7800.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces

[CX885.M7801.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces,Wave.Interfaces
[CX885.M7801.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces,Wave.Interfaces

[CX885.M7809.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces
[CX885.M7809.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces

[CX885.M7811.Interfaces]
Needs=VIDCombo.Interfaces
[CX885.M7811.NT.Interfaces]
Needs=VIDCombo.Interfaces

[CX885.M7911.Interfaces]
Needs=VID.Interfaces
[CX885.M7911.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M7911_25.Interfaces]
Needs=VID.Interfaces
[CX885.M7911_25.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M801x.Interfaces]
Needs=VID.Interfaces
[CX885.M801x.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M805x.Interfaces]
Needs=VID.Interfaces
[CX885.M805x.NT.Interfaces]
Needs=VID.Interfaces

[CX885.M8101.Interfaces]
Needs=VID.Interfaces,Encoder.Interfaces
[CX885.M8101.NT.Interfaces]
Needs=VID.Interfaces,Encoder.Interfaces

[CX885.M8101_25.Interfaces]
Needs=VID.Interfaces,Encoder.Interfaces
[CX885.M8101_25.NT.Interfaces]
Needs=VID.Interfaces,Encoder.Interfaces

[CX885.M8501.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces
[CX885.M8501.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces

[CX885.M8541.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces
[CX885.M8541.NT.Interfaces]
Needs=VIDCombo.Interfaces,Encoder.Interfaces

[CX885.M8551.Interfaces]
Needs=VIDCombo.Interfaces
[CX885.M8551.NT.Interfaces]
Needs=VIDCombo.Interfaces

[CX885.M8571.Interfaces]
Needs=VID.Interfaces
[CX885.M8571.NT.Interfaces]
Needs=VID.Interfaces



[VID.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%VcapReferenceGUID%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
; Debug interface for TS testing
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,

[VIDCombo.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%VcapReferenceGUID%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDACombo_Interface,
; Debug interface for TS testing
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,

[TriMode.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%VcapReferenceGUID%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,
;SAT related
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%AltBDATuneReferenceGuid%,AltBDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%AltTSReferenceGuid%,AltTS_Interface,

[QuadMode.Interfaces]
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%VcapReferenceGUID%,VID_Interface,
AddInterface={a799a802-a46d-11d0-a18c-00a02401dcd4},%TVAudioReferenceGuid%,TvAudio_Interface,
AddInterface={a799a801-a46d-11d0-a18c-00a02401dcd4},%XBARReferenceGUID%,CX88XBAR_Interface,
AddInterface={a799a800-a46d-11d0-a18c-00a02401dcd4},%TunerReferenceGuid%,CX88TUNE_Interface,
AddInterface={6994AD04-93EF-11D0-A3CC-00A0C9223196},%AudioReferenceGuid%,AUD_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid%,BDATUNE_Interface,
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%BDATuneReferenceGuid2%,BDATUNE_Interface2,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSReferenceGuid%,TS_Interface,
;SAT related
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%AltBDATuneReferenceGuid%,AltBDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%AltTSReferenceGuid%,AltTS_Interface,

[Sat.Interfaces]
; SAT-only related
AddInterface={71985F48-1CA1-11d3-9CC8-00C04F7971E0},%AltBDATuneReferenceGuid%,AltBDATUNE_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%AltTSReferenceGuid%,AltTS_Interface,
AddInterface={65e8773d-8f56-11d0-a3b9-00a0c9223196},%VcapReferenceGUID%,VID_Interface,

[Encoder.Interfaces]
; Encoder interfaces
AddInterface=%GUID.Encoder%,%EncoderReferenceGuid%,ENCODER_Interface,
AddInterface=%GUID.Multiplexer%,%EncoderReferenceGuid%,ENCODER_Interface,

[Wave.Interfaces]
; Wave Audio capture device
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,AUD_Interface,
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,AUD_Interface,
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,AUD_Interface_Topology,
;;AddInterface=%KSCATEGORY_TOPOLOGY%,%KSNAME_Topology%,AUD_Interface_Topology,

AddInterface=%KSCATEGORY_CAPTURE%,%AudioReferenceGuid%,AUD_Interface,
AddInterface=%KSCATEGORY_AUDIO%,%AudioReferenceGuid%,AUD_Interface,
AddInterface=%KSCATEGORY_AUDIO_CAP%,%AudioReferenceGuid%,AUD_Interface,
;;AddInterface=%KSCATEGORY_WDMAUD%,%AudioReferenceGuid%,AUD_Interface,


[VID_Interface]
AddReg=VID_Interface.AddReg

[VID_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%VIDFriendlyName%

[TvAudio_Interface]
AddReg=TvAudio_Interface.AddReg

[TvAudio_Interface.AddReg]
HKR,,CLSID,,{71F96462-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%TVAudioFriendlyName%

[CX88XBAR_Interface]
AddReg=CX88XBAR_Interface.AddReg

[CX88XBAR_Interface.AddReg]
HKR,,CLSID,,{71F96460-78F3-11d0-A18C-00A0C9118956}
HKR,,FriendlyName,,%XBARFriendlyName%

[CX88TUNE_Interface]
AddReg=CX88TUNE_Interface.AddReg

[CX88TUNE_Interface.AddReg]
HKR,,CLSID,,{266EEE40-6C63-11cf-8A03-00AA006ECB65}
HKR,,FriendlyName,,%TunerFriendlyName%
;Vista tunerInstanceID entry, see CXTUNE_Interface.AddReg
HKR,,TunerInstanceID,0x00010001,10


[AUD_Interface]
AddReg=AUD_Interface.AddReg

[AUD_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AudioFriendlyName%

[AUD_Interface_Topology]
AddReg=AUD_Interface_Topology.AddReg, OEMSettingsOverride.AddReg

[AUD_Interface_Topology.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TopoFriendlyName%


[OEMSettingsOverride.AddReg]


[BDATUNE_Interface]
AddReg=BDATUNE_Interface.AddReg

[BDATUNE_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName%
;Vista tunerInstanceID entry, see CXTUNE_Interface.AddReg
;Use this to indicate a Hybrid Card
HKR,,TunerInstanceID,0x00010001,10

[BDATUNE_Interface2]
AddReg=BDATUNE_Interface2.AddReg

[BDATUNE_Interface2.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName2%
;Vista tunerInstanceID entry, see CXTUNE_Interface.AddReg
;Use this to indicate a Hybrid Card
HKR,,TunerInstanceID,0x00010001,10

[BDACombo_Interface]
AddReg=BDACombo_Interface.AddReg

[BDACombo_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%BDATuneFriendlyName%
;Vista tunerInstanceID entry, see CXTUNE_Interface.AddReg
;Use this to indicate a Combo(Dual tuner) Card
HKR,,TunerInstanceID,0x00010001,11

[AltBDATUNE_Interface]
AddReg=AltBDATUNE_Interface.AddReg

[AltBDATUNE_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AltBDATuneFriendlyName%
;Vista tunerInstanceID entry, see CXTUNE_Interface.AddReg
;Use this to indicate Sat. is a distinct tuner
HKR,,TunerInstanceID,0x00010001,12


[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%


[AltTS_Interface]
AddReg=AltTS_Interface.AddReg

[AltTS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%AltTSFriendlyName%


[ENCODER_Interface]
AddReg=ENCODER_Interface.AddReg

[ENCODER_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%EncoderFriendlyName%
;Add an interface for Microsoft's video bit rate property set
HKR,Interfaces\{B43C4EEC-8C32-4791-9102-508ADA5EE8E7},,,
HKR,Interfaces\{b05dabd9-56e5-4fdc-afa4-8a47e91f1c9c},,,
HKR,Capabilities,,,
HKR,Capabilities,"{BB4FAA02-596C-4129-8FB3-74E75421FA02}", 0x00010001,1


;
; Services installation
;
[CX885.M5300_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M5300_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M5340_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M5340_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.MC100_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.MC100_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.MC12A_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.MC12A_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.MC130_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.MC130_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.MC140_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.MC140_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2211_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2211_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2215_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2215_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2251_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2251_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2291_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2291_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2295_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2295_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M22D1_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M22D1_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M22D3_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M22D3_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall


[CX885.M2A18_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2A18_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2A28_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2A28_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M2A38_50.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M2A38_50.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall


[CX885.M7100.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7100.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7101.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7101.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7110.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7110.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7120.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7120.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7130.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7130.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7108.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7108.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7118.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7118.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7128.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7128.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7133.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7133.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7138.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7138.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7141.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7141.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7148.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7148.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7151.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7151.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7158.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7158.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7168.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7168.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7173.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7173.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7178.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7178.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M71D1.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M71D1.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M71D1_25.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M71D1_25.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M71D3.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M71D3.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M71D3_25.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M71D3_25.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7600.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7600.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7610.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7610.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M771x.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M771x.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M779x.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M779x.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7800.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7800.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7801.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7801.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7809.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7809.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7811.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7811.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7911.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7911.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M7911_25.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M7911_25.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M801x.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M801x.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M805x.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M805x.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8101.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8101.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8101_25.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8101_25.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8501.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8501.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8541.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8541.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8551.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8551.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall

[CX885.M8571.Services]
AddService = HCW85BDA,2,VID.ServiceInstall
[CX885.M8571.NT.Services]
AddService = HCW85BDA,2,VID.ServiceInstall




[VID.ServiceInstall]
DisplayName   = %CX23885.DeviceDesc%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %10%\system32\drivers\HCW85BDA.sys

;;;;;;;;;;;;;;;;;;;;;
;
[Mxxxx.DelReg]
HKR,"DriverData"
HKR,"Parameters"
HKR,"I2C Devices"
HKR,"ENUM"

[Xtal25.Addreg]
HKR,"DriverData","XtalFreq",0x00010001, 0x19,0x00,0x00,0x00

[Xtal50.Addreg]
HKR,"DriverData","XtalFreq",0x00010001, 0x32,0x00,0x00,0x00

;; Overrides for 888 based boards (should put these elsewhere)
;HKR,"DriverData","HcwHue",0x00010001, 0
;HKR,"DriverData","HcwSaturation",0x00010001, 128
;HKR,"DriverData","HcwBrightness",0x00010001, 3
;HKR,"DriverData","HcwContrast",0x00010001, 125
HKR,"DriverData","HcwSharpness",0x00010001, 3

[LNB.AddReg]
; 2 = Use 13/18V instead of 14/19V
; 4 = don't power down LNB when not in use
HKLM,%Services%\HCW85BDA\Parameters,"LNBVoltage_Ctrl",0x00010001, 0x02,0x00,0x00,0x00

[M5300.AddReg]
;;;Chesterfield3 (888 DIF, CI, CIR, Wake from Standby, FM via Sat input)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield3",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x03, 0x00, 0x00, 0x00


HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+CX23888+TDA10048(205)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcd, 0x00, 0x00, 0x00

; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x01, 0x00, 0x00, 0x00

; power control adjustment for HVR-3300
HKR,"DriverData","PowerControl",0x00010001, 0x10, 0x00, 0x00, 0x00



[M5340.AddReg]
;;;Chesterfield3 (888 DIF, no CI, no IR, no Wake, No FM via Sat input)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield3",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x03, 0x00, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+CX23888+TDA10048(205)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcd, 0x00, 0x00, 0x00

; PAL/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x62, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
;HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x00, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00


; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x00, 0x00, 0x00, 0x00

; power control adjustment for HVR-3300
HKR,"DriverData","PowerControl",0x00010001, 0x10, 0x00, 0x00, 0x00



[MC100.AddReg]
;;;Chesterfield4 (888 DIF, Si2165, CI, CIR, Wake from Standby, FM)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield4_DVBT",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

; Fixme - need Si2165 value
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x02, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+Si2165(210)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xD2, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x01, 0x00, 0x00, 0x00


[MC12A.AddReg]
;;;Chesterfield4 (888 DIF, DVB-S/s2 only, CIR)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield4_DVBS2",0x00010001, 0x01,0x00,0x00,0x00
;HKR,"DriverData","TunerType",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to 0
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x01, 0x00, 0x00, 0x00


[MC130.AddReg]
;;;Chesterfield4 (888 DIF, Si2165, CI, CIR, Wake from Standby, FM via Sat input)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield4_DVBC",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

HKR,"DriverData","BDA_Demod_Tuner_type", 0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","BDA_Demod_Tuner_type2",0x00010001, 0x01, 0x00, 0x00, 0x40
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x02, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+Si2165(210)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xD2, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x01, 0x00, 0x00, 0x00


[MC140.AddReg]
;;;Chesterfield4 (888 DIF, Si2165, No IR/WAke)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Chesterfield4_DVBT_IR",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

; Fixme - need Si2165 value
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x02, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+Si2165(210)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xD2, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00

HKR,"DriverData","HasCIInterface",0x00010001, 0x01, 0x00, 0x00, 0x00



[M2211.AddReg]
;;;Coram2 (888 DIF, 3305)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Coram2-03",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Single Multituner, 888 DIF
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x03, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x03, 0x00, 0x00, 0x10

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner  type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00

;; NTSC/ATSC
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; All-TV/ATSC (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00


[M2215.AddReg]
;;;Coram2 (888 DIF,3305, A/B Switch)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Coram2-04",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Single Multituner, 888 DIF
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x03, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x03, 0x00, 0x00, 0x10

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner  type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
;; NTSC/FM/ATSC
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xB1, 0x00, 0x00, 0x00
;; All-TV/FM/ATSC (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x31, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00


[M2251.AddReg]
;;;Coram2 (888 DIF, 228)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Coram2-05",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Single Multituner, 888 DIF, 228 demod
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x01, 0x00, 0x80
HKR,"Parameters","TDA18271_IFLevel_ATSC",0x00010001, 0x05, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DCABLE",0x00010001, 0x05, 0x00, 0x00, 0x00
; need this for 228 demod
HKR,"DriverData","TS2_GEN_CTL_TS",0x00010001, 0xC,0x00,0x00,0x00

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner  type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00

;; NTSC/ATSC
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; All-TV/ATSC (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; use agressive power controls by default??
HKR,"DriverData","PowerControl",0x00010001, 0x00, 0x00, 0x00, 0x00



[M2291.AddReg]
;;;Kingston2 (888 DIF)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston2-03",0x00010001, 0x01,0x00,0x00,0x00

HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+CX23888+TDA10048(205)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcd, 0x00, 0x00, 0x00

; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/DVB-T (testing only); may break MCE scanning
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x22, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00


[M2295.AddReg]
;;;Kingston2 (888 DIF, A/B Switch)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston2-03",0x00010001, 0x01,0x00,0x00,0x00

HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
;HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+CX23888+TDA10048(205)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcd, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00



[M22D1.AddReg]
;;;Kingston2
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston2-03",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x08, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00

HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+CX23888+TDA10048(205)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcd, 0x00, 0x00, 0x00

;; PAL/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x62, 0x00, 0x00, 0x00
;; All-TV/DVB-T (testing only); may break MCE scanning
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x22, 0x00, 0x00, 0x00

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
;; Use GPIO10 as VAux Control
;HKR,"DriverData","VauxGPIO",0x00010001, 0x0A, 0x00, 0x00, 0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00


[M22D3.AddReg]
;;;Kingston2
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston2NoFP",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x08, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
;; PAL/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x62, 0x00, 0x00, 0x00
;; All-TV/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
;; Use GPIO10 as VAux Control
;HKR,"DriverData","VauxGPIO",0x00010001, 0x0A, 0x00, 0x00, 0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00




[M2A18.AddReg]
;;;K4C4 (888 DIF, 3306)
HKR,"DriverData","BoardType",0x00010001, 0x1C,0x00,0x00,0x00
HKR,"DriverData","Is_Coram4-01",0x00010001, 0x01,0x00,0x00,0x00

HKR,"DriverData","TunerType",0x00010001, 0x81, 0x04, 0x00, 0x80
; BDA_Demod_Tuner_Type
; LG3306_Si2158 Multituner
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x81, 0x04, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;set tuner type to Si2157+LG3306A(214)(0xd6)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xd6, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","Si2158_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
;; NTSC/FM/ATSC
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; All-TV/FM/ATSC (testing only); may break MCE scanning
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x31, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; need this for 3306A
HKR,"DriverData","TS2_GEN_CTL_TS",0x00010001, 0xC,0x00,0x00,0x00


[M2A28.AddReg]
;;;K4C4 (888 DIF, Si2168, CIR)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston4-01",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

HKR,"DriverData","BDA_Demod_Tuner_type", 0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x02, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;set MultiTuner type to Si2157+Si2168(210) BUGBUG
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xD2, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","Si2158_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00


[M2A38.AddReg]
;;;K4C4 (888 DIF, Si2168, LG3306, CIR)
HKR,"DriverData","BoardType",0x00010001, 0x1F,0x00,0x00,0x00
HKR,"DriverData","Is_K4C4-01",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00

HKR,"DriverData","BDA_Demod_Tuner_type", 0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","BDA_Demod_Tuner_type2", 0x00010001, 0x01, 0x00, 0x00, 0x10
HKR,"Parameters","MultiTuner_Demod_Type",0x00010001, 0x02, 0x00, 0x00, 0x00

HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x09, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","AltBDADemodResetGPIO", 0x00010001, 0x08, 0x00, 0x00, 0x00
;Enable Alt TS capture and BDA filter registration
HKR,"DriverData","AltBDATunerModel",0x00010001, 0x04, 0x01, 0x00, 0x00

HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00

;;set MultiTuner type to Si2157+Si2168+LG3306(210) BUGBUG
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xD2, 0x00, 0x00, 0x00

HKR,"Parameters","TDA18271_IFLevel_DVBC",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_IFLevel_DVBT",0x00010001, 0x07, 0x00, 0x00, 0x00
HKR,"Parameters","18271_Digital_TOP_Level",0x00010001, 0x48, 0x00, 0x00, 0x00
HKR,"Parameters","Si2165_ForceAutoBW_DVBC",0x00010001, 0x08, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","Si2158_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
; PAL/FM/DVB-T
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
;; All-TV/FM/DVB-T (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00

HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00

; Next line enables the software TS packetizer
;HKR,"DriverData","dwIsAltTSStream",0x00010001,0x01,0x00,0x00,0x00
;HKR,"DriverData","dwAltTP_PACKET_SIZE",0x00010001,0xBC,0x00,0x00,0x00



[M7100.AddReg]
;;;Kingston
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1C, 0x00, 0x00, 0x00


[M7101.AddReg]
;;;Kingston, No FM
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1C, 0x00, 0x00, 0x00


[M7110.AddReg]
;;;Kingston	Lite
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston_lite",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x1C, 0x00, 0x00, 0x00


[M7120.AddReg]
;;;Kingston	PVR
HKR,"DriverData","BoardType",0x00010001, 0x12,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston_PVR",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00


[M7130.AddReg]
;;;Kingston	GO
HKR,"DriverData","BoardType",0x00010001, 0x15,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston_GO",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0x01, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00


[M7108.AddReg]
;;;Kingston (aka Dover-e)
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Dover-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00


[M7118.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Oxford-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00


[M7128.AddReg]
;;;Kingston PVR (aka Roslyn-e)
HKR,"DriverData","BoardType",0x00010001, 0x12,0x00,0x00,0x00
HKR,"DriverData","Is_Roslyn-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00


[M7133.AddReg]
;;;Kingston VCB
HKR,"DriverData","BoardType",0x00010001, 0x15,0x00,0x00,0x00
HKR,"DriverData","Is_VCB-e",0x00010001, 0x01,0x00,0x00,0x00
;HKR,"DriverData","TunerType",0x00010001, 0x00, 0x00, 0x00, 0x00
;HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
;per JS(UK), solves issues with downstream ACM Codec filter 
HKR,"DriverData","drop_audio_discontinuities",0x00010001, 0x00,0x00,0x00,0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00


[M7138.AddReg]
;;;Kingston Go (aka Pluto-e)
HKR,"DriverData","BoardType",0x00010001, 0x15,0x00,0x00,0x00
HKR,"DriverData","Is_Pluto-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00


[M7141.AddReg]
;;;Kingston (aka Dover-e)
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston04",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295+10046(204)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcc, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00


[M7148.AddReg]
;;;Kingston (aka Dover-e)
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Dover-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA8275A+TDA8295+10046(200)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc8, 0x00, 0x00, 0x00
;;invert TV/FM selection logic
HKR,"I2C Devices","Device 0, Data7",0x00010001, 0xa0, 0x00, 0x00, 0x00


[M7151.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston04_Lite",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295+10046(204)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcc, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00


[M7158.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Oxford-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA8275A+TDA8295+10046(200)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc8, 0x00, 0x00, 0x00
;;invert TV/FM selection logic
HKR,"I2C Devices","Device 0, Data7",0x00010001, 0xa0, 0x00, 0x00, 0x00


[M7168.AddReg]
;;;Kingston PVR (aka Roslyn-e)
HKR,"DriverData","BoardType",0x00010001, 0x12,0x00,0x00,0x00
HKR,"DriverData","Is_Roslyn-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA8275A+TDA8295(201)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc9, 0x00, 0x00, 0x00


[M7173.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston05_Lite",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Allow FM via TV RF input
;HKR,"Parameters","TDA18271C1_UseFMInput",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x60, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;Change default AGC timing to 31.25KHz
HKR,"Parameters","TDA18271C1_EXTENDED_BYTE_12",0x00010001, 0x03, 0x00, 0x00, 0x00
;BUGBUG 990ms is TOO LONG; fix this
HKR,"Parameters","TDA18271C1_StaticAGCDelay",0x00010001, 0xDE, 0x03, 0x00, 0x00


[M7178.AddReg]
;;;Kingston Go (aka Pluto-e)
HKR,"DriverData","BoardType",0x00010001, 0x15,0x00,0x00,0x00
HKR,"DriverData","Is_Pluto-e",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;Disable TS capture and BDA filter registration
HKR,"DriverData","Enable_BDA",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set MultiTuner type to TDA8275A+TDA8295(201)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc9, 0x00, 0x00, 0x00


[M71D1.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston05_Lite",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Allow FM via TV RF input
HKR,"Parameters","TDA18271C1_UseFMInput",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x72, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;Change default AGC timing to 31.25KHz
HKR,"Parameters","TDA18271C1_EXTENDED_BYTE_12",0x00010001, 0x03, 0x00, 0x00, 0x00
;BUGBUG 990ms is TOO LONG; fix this
HKR,"Parameters","TDA18271C1_StaticAGCDelay",0x00010001, 0xDE, 0x03, 0x00, 0x00


[M71D3.AddReg]
;;;Kingston Lite (aka Oxford-e)
HKR,"DriverData","BoardType",0x00010001, 0x11,0x00,0x00,0x00
HKR,"DriverData","Is_Kingston05_LiteNoFP",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Allow FM via TV RF input
;HKR,"Parameters","TDA18271C1_UseFMInput",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x62, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;Change default AGC timing to 31.25KHz
HKR,"Parameters","TDA18271C1_EXTENDED_BYTE_12",0x00010001, 0x03, 0x00, 0x00, 0x00
;BUGBUG 990ms is TOO LONG; fix this
HKR,"Parameters","TDA18271C1_StaticAGCDelay",0x00010001, 0xDE, 0x03, 0x00, 0x00


[M7600.AddReg]
;;;Brentwood
HKR,"DriverData","BoardType",0x00010001, 0x13,0x00,0x00,0x00
HKR,"DriverData","Is_Brentwood",0x00010001, 0x01,0x00,0x00,0x00
;Orig boards had tuner at addr C0, new ones at C2
;HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x10
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking, for testing
HKR,"Parameters","TDA8275A_Blanking",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA8275A+TDA8295(201)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc9, 0x00, 0x00, 0x00
;; Prototype -01 boards used address C2
;;HKR,"I2C Devices","Device 0, Data2",0x00010001, 0xc2, 0x00, 0x00, 0x00


[M7610.AddReg]
;;;Brentwood Lite
HKR,"DriverData","BoardType",0x00010001, 0x14,0x00,0x00,0x00
HKR,"DriverData","Is_Brentwood_lite",0x00010001, 0x01,0x00,0x00,0x00
;Orig boards had tuner at addr C0, new ones at C2
;HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x10
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking, for testing
HKR,"Parameters","TDA8275A_Blanking",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA8275A+TDA8295(201)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xc9, 0x00, 0x00, 0x00


[M7717.AddReg]
;;;Melville (XC3028 tuner)
HKR,"DriverData","BoardType",0x00010001, 0x16,0x00,0x00,0x00
HKR,"DriverData","Is_Melville",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x32, 0x00, 0x00, 0x00

HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7797.AddReg]
;;;Melville (XC5000 tuner)
HKR,"DriverData","BoardType",0x00010001, 0x16,0x00,0x00,0x00
HKR,"DriverData","Is_Melville-Q",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x11, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x40, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC2, 0x00, 0x00, 0x00
HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x32, 0x00, 0x00, 0x00

HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7800.AddReg]
;;;Medford
HKR,"DriverData","BoardType",0x00010001, 0x18,0x00,0x00,0x00
HKR,"DriverData","Is_Medford",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_DIG_IF_Level",0x00010001, 0x3, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_XTALOut_Mode",0x00010001, 0x1, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x31, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7801.AddReg]
;;;Medford
HKR,"DriverData","BoardType",0x00010001, 0x18,0x00,0x00,0x00
HKR,"DriverData","Is_Medford_25M",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x19,0x00,0x00,0x00
HKR,"DriverData","blaster_reset_gpio_bit", 0x00010001, 0x2f, 0x00, 0x00, 0x00
HKR,"DriverData","blaster_data_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_DIG_IF_Level",0x00010001, 0x3, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_XTALOut_Mode",0x00010001, 0x1, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x31, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7809.AddReg]
;;;Medford, No FM
HKR,"DriverData","BoardType",0x00010001, 0x18,0x00,0x00,0x00
HKR,"DriverData","Is_Medford_25M_NoFM",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x19,0x00,0x00,0x00
HKR,"DriverData","blaster_reset_gpio_bit", 0x00010001, 0x2f, 0x00, 0x00, 0x00
HKR,"DriverData","blaster_data_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_DIG_IF_Level",0x00010001, 0x3, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_XTALOut_Mode",0x00010001, 0x1, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7811.AddReg]
;;;Medford Lite
HKR,"DriverData","BoardType",0x00010001, 0x19,0x00,0x00,0x00
HKR,"DriverData","Is_Medford_lite",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x0E, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x19,0x00,0x00,0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_DIG_IF_Level",0x00010001, 0x3, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271C1_XTALOut_Mode",0x00010001, 0x1, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x31, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M7911.AddReg]
;;;Coram
HKR,"DriverData","BoardType",0x00010001, 0x17,0x00,0x00,0x00
HKR,"DriverData","Is_Coram",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x10, 0x00, 0x10
HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_demod_reset_gpio_bit",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","MT2131_227_tuner_reset_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00


[M801x.AddReg]
;;;Whitman
HKR,"DriverData","BoardType",0x00010001, 0x1a,0x00,0x00,0x00
HKR,"DriverData","Is_Whitman",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x10, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x1A, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC8, 0x00, 0x00, 0x00
;HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x12, 0x00, 0x00, 0x00

HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00

;Mask NTSC_M, NTSC_M_J, PAL_M, PAL_N and PAL_N_COMBO standards
HKR,"DriverData","TunerStandardsMask",0x00010001, 0xfc, 0xf9, 0xef, 0xff


[M805x.AddReg]
;;;Whitman-D
HKR,"DriverData","BoardType",0x00010001, 0x1a,0x00,0x00,0x00
HKR,"DriverData","Is_Whitman-D",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x12, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

HKR,"DriverData","TunerType",0x00010001, 0x41, 0x00, 0x00, 0x00
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","TunerI2CAddress",0x00010001, 0xC8, 0x00, 0x00, 0x00
;HKR,"DriverData","Tuner2IFAddress",0x00010001, 0x86, 0x00, 0x00, 0x00
HKR,"DriverData","DemodI2CAddress",0x00010001, 0x12, 0x00, 0x00, 0x00

HKR,"DriverData","EnableIR",0x00010001, 0x00, 0x00, 0x00, 0x00

;Mask NTSC_M, NTSC_M_J, PAL_M, PAL_N and PAL_N_COMBO standards
;;HKR,"DriverData","TunerStandardsMask",0x00010001, 0xfc, 0xf9, 0xef, 0xff
;Debug, allow all standards
HKR,"DriverData","TunerStandardsMask",0x00010001, 0xff, 0xff, 0xff, 0xff



[M8101.AddReg]
;;;Whitney (aka Dover-e)
HKR,"DriverData","BoardType",0x00010001, 0x10,0x00,0x00,0x00
HKR,"DriverData","Is_Whitney",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","TunerType",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","TunerCountryCode",0x00010001, 0x31,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x01, 0x00, 0x00, 0x80
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x02, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_PRESENT",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_FLASH_EEPROM",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA10048_EEPROM_AUTOUPDATE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Allow FM via TV RF input
;HKR,"Parameters","TDA18271C1_UseFMInput",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set MultiTuner type to TDA18271+TDA8295+10048(203)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xcb, 0x00, 0x00, 0x00
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x62, 0x00, 0x00, 0x00
; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x32, 0x00, 0x00, 0x00
;Change default AGC timing to 31.25KHz
HKR,"Parameters","TDA18271C1_EXTENDED_BYTE_12",0x00010001, 0x03, 0x00, 0x00, 0x00
;BUGBUG 990ms is TOO LONG; fix this
;HKR,"Parameters","TDA18271C1_StaticAGCDelay",0x00010001, 0xDE, 0x03, 0x00, 0x00


[M8501.AddReg]
;;;Medford2	(8295)
HKR,"DriverData","BoardType",0x00010001, 0x1B,0x00,0x00,0x00
HKR,"DriverData","Is_Medford2_50",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Dual Multituner
HKR,"DriverData","TunerType",0x00010001, 0x02, 0x01, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10

HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0x2F, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x32,0x00,0x00,0x00

;;;This depends on the port expander being used
;HKR,"DriverData","VauxGPIO",0x00010001, 0x30,0x00,0x00,0x00
HKR,"DriverData","VauxGPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0x32,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_AUTOMUTE_VIDEO",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set tuner count to 2
HKR,"I2C Devices","Number of I2C Devices",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set tuner 1 type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
;;set tuner 2 type to TDA18271+CX24228(207)
HKR,"I2C Devices","Device 1, Data1",0x00010001, 0xcf, 0x00, 0x00, 0x00

;; Disable FM
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0x98, 0xab, 0x02, 0x00

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00
; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00



[M8541.AddReg]
;;;Medford2	(888 DIF)
HKR,"DriverData","BoardType",0x00010001, 0x1B,0x00,0x00,0x00
HKR,"DriverData","Is_Medford2_50",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Dual Multituner, 888 DIF
HKR,"DriverData","TunerType",0x00010001, 0x82, 0x01, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10

HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x32,0x00,0x00,0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set tuner count to 2
HKR,"I2C Devices","Number of I2C Devices",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set tuner 1 type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
;;;set tuner 1 type to TDA18271+CX23888(206)  (using 888 DIF)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xce, 0x00, 0x00, 0x00

;;set tuner 2 type to TDA18271+CX24228(207)
HKR,"I2C Devices","Device 1, Data1",0x00010001, 0xcf, 0x00, 0x00, 0x00

;; FM is on TV input
HKR,"Parameters","TDA18271_UseFMInput",0x00010001, 0x03, 0x00, 0x00, 0x00
;; Enable TV,FM,ATSC
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xB1, 0x00, 0x00, 0x00
;; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0x32,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00



[M8551.AddReg]
;;;Medford2Lite	(888 DIF)
HKR,"DriverData","BoardType",0x00010001, 0x1D,0x00,0x00,0x00
HKR,"DriverData","Is_Medford2_Lite",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Dual Multituner, 888 DIF
HKR,"DriverData","TunerType",0x00010001, 0x82, 0x01, 0x00, 0x80

HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10

HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x32,0x00,0x00,0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set tuner count to 2
HKR,"I2C Devices","Number of I2C Devices",0x00010001, 0x02, 0x00, 0x00, 0x00
;;set tuner 1 type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
;;;set tuner 1 type to TDA18271+CX23888(206)  (using 888 DIF)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xce, 0x00, 0x00, 0x00

;;set tuner 2 type to TDA18271+CX24228(207)
HKR,"I2C Devices","Device 1, Data1",0x00010001, 0xcf, 0x00, 0x00, 0x00

;; Disable FM
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80
; verify Video present during AFC test
;HKR,"DriverData","AFCVideoRetrys", 0x00010001, 0x05, 0x00, 0x00, 0x00


;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00



[M8571.AddReg]
;;;Medford2Hyb	(888 DIF)
HKR,"DriverData","BoardType",0x00010001, 0x1E,0x00,0x00,0x00
HKR,"DriverData","Is_Medford2_Hybrid",0x00010001, 0x01,0x00,0x00,0x00

;;Following enables Single Multituner, 888 DIF
HKR,"DriverData","TunerType",0x00010001, 0x81, 0x01, 0x00, 0x80


HKR,"DriverData","TunerCountryCode",0x00010001, 0x01,0x00,0x00,0x00
HKR,"DriverData","BDA_Demod_Tuner_type",0x00010001, 0x02, 0x00, 0x00, 0x10

HKR,"DriverData","demod_reset_gpio_bit", 0x00010001, 0x2E, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_reset_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","demod_sleep_gpio_bit", 0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","tuner_sif_fm_gpio_bit",0x00010001, 0xff, 0x00, 0x00, 0x00
HKR,"DriverData","XtalFreq",0x00010001, 0x32,0x00,0x00,0x00

HKR,"DriverData","IsDIFBoard",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"DriverData","Use888VSYNC",0x00010001, 0x01, 0x00, 0x00, 0x00
;Enable AGC Adjustment for DIF and Tuner
HKR,"DriverData","enable_tuner_agc_adjustment",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_Disable16Mhz",0x00010001, 0x01, 0x00, 0x00, 0x00
HKR,"Parameters","TDA18271_XTALOut_Mode",0x00010001, 0x00, 0x00, 0x00, 0x00

;;disable any blanking
HKR,"Parameters","TDA18271_BlankVideo",0x00010001, 0x00, 0x00, 0x00, 0x00

;;set tuner 1 type to TDA18271+TDA8295(202)
HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xca, 0x00, 0x00, 0x00
HKR,"Parameters","TDA8295_NoHW",0x00010001, 0x01, 0x00, 0x00, 0x00
;;;set tuner 1 type to TDA18271+CX23888(206)  (using 888 DIF)
;HKR,"I2C Devices","Device 0, Data1",0x00010001, 0xce, 0x00, 0x00, 0x00

;; Disable FM
HKR,"I2C Devices","Device 0, Data6",0x00010001, 0xA1, 0x00, 0x00, 0x00
;; Enable all formats (testing only); may break MCE scanning
;HKR,"I2C Devices","Device 0, Data6",0x00010001, 0x21, 0x00, 0x00, 0x00
;; Enable AutoAFC, no retry if out of range
HKR,"DriverData","TunerUseAutoAFC", 0x00010001, 0xf8, 0x24, 0x01, 0x80

;Load the CIR driver
HKR,"ENUM\Device1",pnpid,,"HCW85CIR3"
;CIR Support
HKR,"DriverData","EnableCIR",0x00010001, 0x01, 0x00, 0x00, 0x00
; What IR Mask is used for CIR? 0 = IR_MSK(D0), 1 = UART_MSK(C0a), 2 = TIMER_MSK(C0)
HKR,"DriverData","IRInterruptMask",0x00010001, 0x00, 0x00, 0x00, 0x00

; VAux switching is NOT controlled by Hardware
HKR,"DriverData","VAUX_CTRL_BY_HARDWARE",0x00010001, 0x00, 0x00, 0x00, 0x00
; Use GPIO0 as VAux Control
HKR,"DriverData","VauxGPIO",0x00010001, 0x00, 0x00, 0x00, 0x00
HKR,"DriverData","Reset417GPIO",0x00010001, 0xff,0x00,0x00,0x00
HKR,"DriverData","PortMuxState",0x00010001, 0x00,0x00,0x00,0x00

; DeviceToWakeFrom: possible values :
; Prefered values : 4 or 5
;    PowerSystemUnspecified = 0
;    PowerSystemWorking     = 1
;    PowerSystemSleeping1   = 2
;    PowerSystemSleeping2   = 3
;    PowerSystemSleeping3   = 4
;    PowerSystemHibernate   = 5
;    PowerSystemShutdown    = 6
;    PowerSystemMaximum     = 7
HKR,"DriverData","DeviceToWakeFrom",0x00010001, 0x04, 0x00, 0x00, 0x00

;;EnableGreyVideoAtChannelChange : 0x00 = Disable, 0x01 = Enable
;HKR,"DriverData","EnableGreyVideoAtChannelChange",0x00010001, 0x00, 0x00, 0x00, 0x00




;;;;;;;;;;;;;;;;;;;;;

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------


[Strings]
CX885.M5300                  = "Hauppauge WinTV HVR-3300 (Model 53xxx, Hybrid DVB-T/S, IR)"
CX885.M5340                  = "Hauppauge WinTV HVR-3300 (Model 53xxx, Hybrid DVB-T/S)"
CX885.MC100                  = "Hauppauge WinTV HVR-4400 (Model 121xxx, Hybrid DVB-T/S2, IR)"
CX885.MC130                  = "Hauppauge WinTV HVR-5500 (Model 121xxx, Hybrid DVB-T/C/S2, IR)"
CX885.MC140                  = "Hauppauge WinTV HVR-4400 (Model 121xxx, Hybrid DVB-T/S2)"
CX885.MC12A                  = "Hauppauge WinTV Starburst (Model 121x00, DVB-S2, IR)"
CX885.M2211                  = "Hauppauge WinTV HVR-1250 (Model 22xxx, Hybrid ATSC/QAM)"
CX885.M2215                  = "Hauppauge WinTV HVR-1250 (Model 22xxx, Hybrid ATSC/QAM, RF Switch)"
CX885.M2251                  = "Hauppauge WinTV HVR-1255 (Model 22xxx, Hybrid ATSC/QAM)"
CX885.M2291                  = "Hauppauge WinTV HVR-1200 (Model 22xxx, Hybrid DVB-T)"
CX885.M22F4                  = "PCTV 311ix (Hybrid DVB-T)"
CX885.M2295                  = "Hauppauge WinTV HVR-1211 (Model 22xxx, Hybrid DVB-T, RF Switch)"
CX885.M22D1                  = "Hauppauge WinTV HVR-12?? (Model 22xxx, Hybrid DVB-T, 8295)"
CX885.M22D3                  = "Hauppauge WinTV HVR-12?? (Model 22xxx, Hybrid DVB-T, 8295, No FP)"
CX885.M2A18                  = "Hauppauge WinTV HVR-1265 (Model 161xxx, Hybrid ATSC/QAM, IR)"
CX885.M2A28                  = "Hauppauge WinTV HVR-1205 (Model 161xxx, Hybrid DVB-T/T2/C, IR)"
CX885.M2A38                  = "Hauppauge WinTV HVR-1275 (Model 161xxx, Hybrid DVB-T/T2/C, ATSC/QAM, IR)"
CX885.M7100                  = "Hauppauge WinTV 885 (Model 71xxx PVR/DVB-T Hybrid, Xc3028)"
CX885.M7101                  = "Hauppauge WinTV 885 (Model 71xxx PVR/DVB-T Hybrid, Xc3028, No FM)"
CX885.M7110                  = "Hauppauge WinTV 885 (Model 71xxx Analog/DVB-T Hybrid, Xc3028)"
CX885.M7120                  = "Hauppauge WinTV 885 (Model 71xxx PVR, Xc3028)"
CX885.M7130                  = "Hauppauge WinTV 885 (Model 71xxx Analog, Xc3028)"
CX885.M7108                  = "Hauppauge WinTV 885 (Model 71xxx PVR/DVB-T Hybrid, 8275a/8290)"
CX885.M7118                  = "Hauppauge WinTV 885 (Model 71xxx Analog/DVB-T Hybrid, 8275a/8290)"
CX885.M7128                  = "Hauppauge WinTV 885 (Model 71xxx PVR, 8275a/8290)"
CX885.M7133                  = "Hauppauge ImpactVCB-e (Model 711xx)"
CX885.M7138                  = "Hauppauge WinTV 885 (Model 71xxx Analog, 8275a/8290)"
CX885.M7141                  = "Hauppauge WinTV HVR-1700 Engr Sample (OBSOLETE)"
CX885.M7148                  = "Hauppauge WinTV 885 (Model 71xxx PVR/DVB-T Hybrid, 8275a/8295)"
CX885.M7151                  = "Hauppauge WinTV HVR-1200 (Model 71xxx, Hybrid DVB-T)"
CX885.M7158                  = "Hauppauge WinTV 885 (Model 71xxx Analog/DVB-T Hybrid, 8275a/8295)"
CX885.M7168                  = "Hauppauge WinTV 885 (Model 71xxx PVR, 8275a/8295)"
CX885.M7173                  = "Hauppauge WinTV HVR-1200 (Model 71xxx, Multi-PAL)"
CX885.M7178                  = "Hauppauge WinTV 885 (Model 71xxx Analog, 8275a/8295)"
CX885.M71D1                  = "Hauppauge WinTV HVR-1200 (Model 71xxx, Hybrid DVB-T)"
CX885.M71D3                  = "Hauppauge WinTV HVR-1200 (Model 71xxx, Hybrid DVB-T, No FP)"
CX885.M7600                  = "Hauppauge WinTV HVR-1800lp (Model 76xxx, Combo)"
CX885.M7610                  = "Hauppauge WinTV 885 (Model 76xxx Analog/ATSC Combo, 8275a/8295)"
CX885.M7710                  = "Hauppauge WinTV HVR-1500 (Model 77xxx, Hybrid ATSC)"
CX885.M7717                  = "HP Digital/Analog TV Tuner"
CX885.M7790                  = "Hauppauge WinTV HVR-1500 (Model 77xxx, Hybrid ATSC/QAM)"
CX885.M7797                  = "HP Digital/Analog TV Tuner"
CX885.M7800                  = "Hauppauge WinTV HVR-1800 Engr Sample (OBSOLETE)"
CX885.M7801                  = "Hauppauge WinTV HVR-1800 (Model 78xxx, Combo ATSC/QAM)"
CX885.M7809                  = "Hauppauge WinTV HVR-1800 (Model 78xxx, Combo ATSC/QAM, No FM)"
CX885.M7810                  = "Hauppauge WinTV HVR-1800sw Engr Sample (OBSOLETE)"
CX885.M7811                  = "Hauppauge WinTV HVR-1800sw (Model 78xxx, Combo ATSC/QAM)"
CX885.M7911                  = "Hauppauge WinTV HVR-1250 (Model 79xxx, Hybrid ATSC/QAM)"
CX885.M8010                  = "Hauppauge WinTV HVR-1400 (Model 80xxx, Hybrid DVB-T)"
CX885.M8017                  = "HVR-1400 OEM Digital/Analog TV Tuner"
CX885.M8050                  = "Hauppauge WinTV HVR-1400 (Model 80xxx, Hybrid DVB-T)"
CX885.M8056                  = "Hauppauge WinTV HVR-1400 (Model 80xxx, Hybrid DVB-T, OEM)"
CX885.M8057                  = "HVR-1400 OEM2 Digital/Analog TV Tuner"
CX885.M8101                  = "Hauppauge WinTV HVR-1700 (Model 81xxx, Hybrid DVB-T)"
CX885.M8501                  = "Hauppauge WinTV HVR-1850 (Model 85xxx, Combo ATSC/QAM)"
CX885.M8541                  = "Hauppauge WinTV HVR-1850 (Model 85xxx, Combo ATSC/QAM, 888 DIF)"
CX885.M8551                  = "Hauppauge WinTV HVR-1290 (Model 85xxx, Combo ATSC/QAM, SW Encode)"
CX885.M8571                  = "Hauppauge WinTV HVR-12?? (Model 85xxx, Hybrid ATSC/QAM, SW Encode)"

CX23885.DeviceDesc           = "Hauppauge WinTV 885 Video Capture"
CX23885.Sonora               = "Hauppauge WinTV 885 Video Capture (proto)"
CX23885.Blank                = "Hauppauge WinTV 885 (CX23885 Blank EEprom)"
CX23887.Blank                = "Hauppauge WinTV 885 (CX23887 Blank EEprom)"
CX23888.Blank                = "Hauppauge WinTV 885 (CX23888 Blank EEprom)"
VIDFriendlyName              = "Hauppauge WinTV 885 Video Capture"
TVAudioFriendlyName          = "Hauppauge WinTV 885 TvAudio"
XBARFriendlyName             = "Hauppauge WinTV 885 Crossbar"
TunerFriendlyName            = "Hauppauge WinTV 885 Tuner"
AudioFriendlyName            = "Hauppauge WinTV 885 Audio Capture"
BDATuneFriendlyName          = "Hauppauge WinTV 885 BDA Tuner/Demod"
BDATuneFriendlyName2         = "Hauppauge WinTV 885 DVBC Tuner/Demod"
EncoderFriendlyName          = "Hauppauge WinTV 885 MPEG Encoder"
TSFriendlyName               = "Hauppauge WinTV 885 TS Capture"

AltBDATuneFriendlyName       = "Hauppauge WinTV 885 Alt BDA Tuner/Demod"
AltTSFriendlyName            = "Hauppauge WinTV 885 Alt TS Capture"

p2.InstallDisk               = "Hauppauge CX23885 Drivers Install Disk"
p2.InstallDisk64             = "Hauppauge CX23885 Drivers Install Disk (64Bit Components)"
p2.InstallDiskWOW            = "Hauppauge CX23885 Drivers Install Disk (WOW64 Components)"

VcapReferenceGUID            = "{9F0E8B75-C677-11db-BEB4-00A0C9F21FC7}"
Proxy.CLSID                  = "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
MediaCategories              = "SYSTEM\CurrentControlSet\Control\MediaCategories"
GUID.PINNAME_ANALOG_AUDIO_IN = "{04394D28-52A7-4c46-AED0-65D62CC64DA6}"
Pin.p2AnalogAudioIn          = "Analog Audio In"
GUID.PINNAME_AUDIO_OUT       = "{9DA02733-7910-40f2-95DD-0441676C9A9B}"
PinName.AnalogAudioOut       = "Audio Out"
TVAudioReferenceGuid         = "{9F0E8B76-C677-11db-BEB4-00A0C9F21FC7}"
XBARReferenceGUID            = "{9F0E8B71-C677-11db-BEB4-00A0C9F21FC7}"
TunerReferenceGuid           = "{9F0E8B77-C677-11db-BEB4-00A0C9F21FC7}"
TSPinID                      = "{5237C937-0A21-4f7e-B338-DE0D0793D03F}"
TSPinName                    = "TS Out"
BDATuneReferenceGuid         = "{9F0E8B70-C677-11db-BEB4-00A0C9F21FC7}"
BDATuneReferenceGuid2        = "{9F0E8B80-C677-11db-BEB4-00A0C9F21FC7}"
TSReferenceGuid              = "{9F0E8B73-C677-11db-BEB4-00A0C9F21FC7}"
AudioReferenceGuid           = "{9F0E8B74-C677-11db-BEB4-00A0C9F21FC7}"

AltBDATuneReferenceGuid      = "{B8917E6F-D893-431b-A41C-33C7DC91BA98}"
AltTSReferenceGuid           = "{B5CFCD56-6B0C-408d-9A38-A3FE1DC7CED0}"

EncoderReferenceGuid         = "{9F0E8B72-C677-11db-BEB4-00A0C9F21FC7}"
GUID.Encoder                 = "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
GUID.Multiplexer             = "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"
Category_Encoders            = "WDM Streaming Encoder Devices"
Category_Multiplexers        = "WDM Streaming Multiplexer Devices"
Node.Encoder                 = "Encoder"
Node.Multiplexer             = "Multiplexer"


GUID.PINNAME_656_IN          = "{DFD530C7-36D9-47ff-B838-9A11D215B140}"
PinName.656_IN               = "656"
GUID.PINNAME_656_OUT         = "{E2EEB283-EB84-4910-BABE-037FFBB03249}"
PinName.656_OUT              = "656"
GUID.PINNAME_MPEG_OUT        = "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
PinName.MpegOut              = "MPEG"

;GUID.IVAC_PROPERTIES        = "{87489F71-B890-4ba2-A88B-03E0B1A4EC1D}"
; we implement the true legacy version of the IVAC API
GUID.IVAC_PROPERTIES         = "{d2185a40-0398-11d3-a53e-00a0c9ef506a}"

GUID.GenEnc_Properties       = "{F6E6FBD9-FE5D-419d-B994-57FB20AAED1D}"
GUID.Video_Properties        = "{5D64F5ED-1526-46f5-B510-AA93437FFA6E}"
GUID.Audio_Properties        = "{9D52CFF7-0DB7-4300-B936-844105E64E9E}"
GUID.MPEG_Properties         = "{A6ABB595-D3B7-4fdf-A418-F2C79E6E1C14}"
GUID.Diagnostic_Properties   = "{18759BBE-6A06-4118-9A57-E833AD670B81}"
GUID.Noise_Properties        = "{10E2DF32-3EC5-4551-BAE6-6D8F6B6C853A}"

GUID.Corona_Properties       = "{063108C1-C019-4d4a-8145-7C7A8AA1E700}"
GUID.CORONA_VERSION_PROPERTIES  = "{461C2E4C-FC98-44c4-A735-21A9FA837A02}"

MediaSets                    = "System\CurrentControlSet\Control\MediaSets"
ActiveMovieCategories        = "CLSID\{da4e3da0-d07d-11d0-bd50-00a0c911ce86}\Instance"

MediaInterfaces              = "System\CurrentControlSet\Control\MediaInterfaces"
Services                     = "System\CurrentControlSet\Services"

WaveFriendlyName             = "WinTV 885 Audio"
TopoFriendlyName             = "WinTV 885 Audio"
KSNAME_Wave                  = "Wave"
KSNAME_Topology              = "Topology"
KSCATEGORY_CAPTURE           = "{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_AUDIO             = "{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_TOPOLOGY          = "{DDA54A40-1E4C-11D1-A050-405705C10000}"
KSCATEGORY_WDMAUD            = "{3E227E76-690D-11D2-8161-0000F8775BF1}"
KSCATEGORY_AUDIO_CAP         = "{33D9A762-90C8-11D0-BD43-00A0C911CE86}"

KSNODETYPE_OUTPUT_UNDEFINED                = "{DFF21CE0-F70F-11D0-B917-00A0C9223196}"
PKEY_AudioEndpoint_ControlPanelProvider    = "{1DA5D803-D492-4EDD-8C23-E0C0FFEE7F0E},1"
PKEY_AudioEndpoint_Association             = "{1DA5D803-D492-4EDD-8C23-E0C0FFEE7F0E},2"
PKEY_AudioDevice_NeverSetAsDefaultEndpoint = "{F3E80BEF-1723-4FF2-BCC4-7F83DC5E46D4},3"
PKEY_AudioDevice_EnableEndpointByDefault   = "{F3E80BEF-1723-4FF2-BCC4-7F83DC5E46D4},4"
PKEY_AudioEngine_OEMFormat                 = "{E4870E26-3CC5-4CD2-BA46-CA0A9A70ED04},3"
PKEY_ItemNameDisplay                       = "{B725F130-47EF-101A-A5F1-02608C9EEBAC},10"

;AudioEndpoint_Association
KSNODETYPE_TV_TUNER_AUDIO     = "{DFF220EC-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_INPUT_UNDEFINED    = "{DFF21BE0-F70F-11D0-B917-00A0C9223196}"
KSNODETYPE_EXTERNAL_UNDEFINED = "{DFF21FE0-F70F-11D0-B917-00A0C9223196}"
