;------------------------------------------------------------------------
;
;   Copyright and Disclaimer:
;
;       ---------------------------------------------------------------
;       This software is provided "as is" without warranty of any kind,
;       either expressed or implied, including but not limited to the
;       implied warranties of merchantability and/or fitness for a
;       particular purpose.
;
;       Copyright (c) 1999-2009 Hauppauge Computer Works, Inc.
;       All Rights Reserved.
;       ---------------------------------------------------------------
;
;   Abstract:
;       This is the 23416 MPEG encoder/TS Capture driver for CX2388x platform.
;
;------------------------------------------------------------------------

[Version]
signature="$CHICAGO$"
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Hauppauge%
DriverVer=08/04/2009,2.124.27191.1
CatalogFile.ntx86=hcw88tse.cat

[Manufacturer]
%Hauppauge%=Hauppauge

[DestinationDirs]
CX88TSE.CopyDrivers=10,system32\drivers

[SourceDisksNames]
1=%p2.InstallDisk%,,,Driver88				;32/64bit machine, Non-Bit-Specific Components
2=%p2.InstallDisk64%,,,"Driver88\64bit"		;64bit machine, 64bit components
3=%p2.InstallDiskWOW%,,,"Driver88\WOW64"		;64bit machine, 32bit components (WOW64)

[SourceDisksFiles]
hcw88tse.sys=1
hcw88prx.ax=1


[CX88TSE.CopyDrivers]
hcw88tse.sys
hcw88prx.ax



[Hauppauge]
;HCW hardware IDs
; Roslyn Analog w/HW MPEG Encoder
%ROSLYN.DeviceDesc%=ROSLYN,      PCI\VEN_14F1&DEV_8802&SUBSYS_28000070
%ROSLYN.DeviceDesc%=ROSLYN,      PCI\VEN_14F1&DEV_8802&SUBSYS_28010070
%ROSLYN.DeviceDesc%=ROSLYN,      PCI\VEN_14F1&DEV_8802&SUBSYS_28030070
%ROSLYN.DeviceDesc%=ROSLYN,      PCI\VEN_14F1&DEV_8802&SUBSYS_28050070

;Dover DVB-T/Analog Hybrid w/HW MPEG Encoder
%DOVER.DeviceDesc%=DOVER,        PCI\VEN_14F1&DEV_8802&SUBSYS_96000070
%DOVER.DeviceDesc%=DOVER,        PCI\VEN_14F1&DEV_8802&SUBSYS_96010070
%DOVER.DeviceDesc%=DOVER,        PCI\VEN_14F1&DEV_8802&SUBSYS_96020070

;TriMode DVB-S/DVB-T/Analog Hybrid
%TRIMODE.DeviceDesc%=hcwDVBST,   PCI\VEN_14F1&DEV_8802&SUBSYS_14000070
%TRIMODE.DeviceDesc%=hcwDVBST,   PCI\VEN_14F1&DEV_8802&SUBSYS_14010070
%TRIMODE.DeviceDesc%=hcwDVBST,   PCI\VEN_14F1&DEV_8802&SUBSYS_14020070
%TRIMODE.DeviceDesc%=hcwDVBST,   PCI\VEN_14F1&DEV_8802&SUBSYS_14040070

;TriMode2 DVB-S2/DVB-T/Analog Hybrid
%TRIMODE2.DeviceDesc%=hcwDVBST,  PCI\VEN_14F1&DEV_8802&SUBSYS_69000070
%TRIMODE2.DeviceDesc%=hcwDVBST,  PCI\VEN_14F1&DEV_8802&SUBSYS_69010070
%TRIMODE2.DeviceDesc%=hcwDVBST,  PCI\VEN_14F1&DEV_8802&SUBSYS_69020070
%TRIMODE2.DeviceDesc%=hcwDVBST,  PCI\VEN_14F1&DEV_8802&SUBSYS_69040070

;TriMode2 DVB-S2 Only
%TRIMODE2.DeviceDesc%=hcwDVBS,   PCI\VEN_14F1&DEV_8802&SUBSYS_69050070
%TRIMODE2.DeviceDesc%=hcwDVBS,   PCI\VEN_14F1&DEV_8802&SUBSYS_69060070

;Oxford	DVB-T/Analog Hybrid
%OXFORD.DeviceDesc%=hcwDVBT,     PCI\VEN_14F1&DEV_8802&SUBSYS_94000070
%OXFORD.DeviceDesc%=hcwDVBT,     PCI\VEN_14F1&DEV_8802&SUBSYS_94010070
%OXFORD.DeviceDesc%=hcwDVBT,     PCI\VEN_14F1&DEV_8802&SUBSYS_94020070

;Oxford-lp DVB-T/Analog Hybrid
%OXFORDHH.DeviceDesc%=hcwDVBT,   PCI\VEN_14F1&DEV_8802&SUBSYS_98000070
%OXFORDHH.DeviceDesc%=hcwDVBT,   PCI\VEN_14F1&DEV_8802&SUBSYS_98020070
%OXFORDHH.DeviceDesc%=hcwDVBT,   PCI\VEN_14F1&DEV_8802&SUBSYS_98100070
%OXFORDHH.DeviceDesc%=hcwDVBT,   PCI\VEN_14F1&DEV_8802&SUBSYS_98120070

;Chelsea DVB-T
%CHELSEA.DeviceDesc%=hcwDVBT,    PCI\VEN_14F1&DEV_8802&SUBSYS_90000070
%CHELSEA.DeviceDesc%=hcwDVBT,    PCI\VEN_14F1&DEV_8802&SUBSYS_90010070
%CHELSEA.DeviceDesc%=hcwDVBT,    PCI\VEN_14F1&DEV_8802&SUBSYS_90020070
%CHELSEA.DeviceDesc%=hcwDVBT,    PCI\VEN_14F1&DEV_8802&SUBSYS_90030070

;Bremen	DVB-S
%BREMEN.DeviceDesc%=hcwDVBS,     PCI\VEN_14F1&DEV_8802&SUBSYS_92000070
%BREMEN.DeviceDesc%=hcwDVBS,     PCI\VEN_14F1&DEV_8802&SUBSYS_92010070
%BREMEN.DeviceDesc%=hcwDVBS,     PCI\VEN_14F1&DEV_8802&SUBSYS_92020070

;%CX88x.null%=NullSection,        PCI\VEN_14F1&DEV_8802


[NullSection]

[NullSection.Services]
AddService = , 2  ; null service install



[ROSLYN]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration
AddReg=     HCW88TSE.AddReg,ROSLYN.AddReg
CopyFiles=  CX88TSE.CopyDrivers

[ROSLYN.NT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT
;AddReg=     CX88ENC.AddReg,ROSLYN.AddReg
AddReg=     HCW88TSE.AddReg,ROSLYN.AddReg
CopyFiles=  CX88TSE.CopyDrivers


[ROSLYN.AddReg]
; Macrovision
HKR,"DriverData","EncoderMVDRM",0x00010001,   0x00,0x00,0x00,0x00
HKR,"DriverData","DeferFWLoad",0x00010001,   0x01,0x00,0x00,0x00

;Register the name of the 656, and I2S pins
HKLM,%MediaCategories%\%GUID.PINNAME_656_IN%,Name,,%PinName.656_IN%
HKLM,%MediaCategories%\%GUID.PINNAME_I2S_IN%,Name,,%PinName.I2S_IN%

;Name of the MPEG output pin.
HKLM,%MediaCategories%\%TPPinID%,Display,1, 00,00,00,00
HKLM,%MediaCategories%\%TPPinID%,Name,,%TPpinName%

;Add the property pages

HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,

HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Video_Properties%,,,

HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Audio_Properties%,,,

HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.MPEG_Properties%,,,

HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Diagnostic_Properties%,,,

HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Noise_Properties%,,,

;Register the encoder and multiplexer classes with Direct X
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,CLSID,,%GUID.Encoder%
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,FriendlyName,,%Category_Encoders%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,CLSID,,%GUID.Multiplexer%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,FriendlyName,,%Category_Multiplexers%

;Register the names of the encoder and multiplexer nodes
HKLM,%MediaCategories%\%GUID.Encoder%,Name,,%Node.Encoder%
HKLM,%MediaCategories%\%GUID.Encoder%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%GUID.Multiplexer%,Name,,%Node.Multiplexer%
HKLM,%MediaCategories%\%GUID.Multiplexer%,Display,1,00,00,00,00


;
; Interfaces installation
;

[ROSLYN.Interfaces]
AddInterface=%GUID.Encoder%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface=%GUID.Multiplexer%,%EncFilterReferenceGUID%,DOVER_Interface,

[ROSLYN.NT.Interfaces]
AddInterface=%GUID.Encoder%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface=%GUID.Multiplexer%,%EncFilterReferenceGUID%,DOVER_Interface,


[ROSLYN_Interface]
AddReg=ROSLYN_Interface.AddReg

[ROSLYN_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%MPEGEncFriendlyName%
;Add interfaces for Microsoft's video bit rate property set
; CLSID_IVideoEncoderProxy = {B43C4EEC-8C32-4791-9102-508ADA5EE8E7} 
;  Causes KsProxy to expose the IVideoEncoder interface 
HKR,Interfaces\{B43C4EEC-8C32-4791-9102-508ADA5EE8E7},,,
; CLSID_IVideoEncoderCodecAPIProxy = {B05DABD9-56E5-4FDC-AFA4-8A47E91F1C9C} 
;  Causes KsProxy to expose both the IVideoEncoder and ICodecAPI interfaces
HKR,Interfaces\{b05dabd9-56e5-4fdc-afa4-8a47e91f1c9c},,,
; Dynamic Bitrate support
HKR,Capabilities,,,
HKR,Capabilities,"{BB4FAA02-596C-4129-8FB3-74E75421FA02}", 0x00010001,1
;;Encoder property page extension
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"hcw88prx.ax",,"RunDll32 %10%\system32\drivers\hcw88prx.ax,DllRegisterServer"

;
; Services installation
;

[ROSLYN.Services]
;AddService = HCW88ENC,2,HCW88ENC.ServiceInstall
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall

[ROSLYN.NT.Services]
;AddService = HCW88ENC,2,HCW88ENC.ServiceInstall
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall


;
; Driver Configuration Registry Entries
;
[CX88ENC.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,hcw88enc.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01

[HCW88ENC.ServiceInstall]
DisplayName   = %ROSLYN.DeviceDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\hcw88enc.sys





[hcwDVBT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration
AddReg=     HCW88TSE.AddReg,hcwDVBT.AddReg
CopyFiles=  CX88TSE.CopyDrivers

[hcwDVBT.NT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT
AddReg=     HCW88TSE.AddReg,hcwDVBT.AddReg
CopyFiles=  CX88TSE.CopyDrivers

;
; Interfaces installation
;

[hcwDVBT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

[hcwDVBT.NT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

;
; Services installation
;

[hcwDVBT.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall

[hcwDVBT.NT.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall




[hcwDVBS]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration
AddReg=     HCW88TSE.AddReg,hcwDVBS.AddReg
CopyFiles=  CX88TSE.CopyDrivers

[hcwDVBS.NT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT
AddReg=     HCW88TSE.AddReg,hcwDVBS.AddReg
CopyFiles=  CX88TSE.CopyDrivers

;
; Interfaces installation
;

[hcwDVBS.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

[hcwDVBS.NT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

;
; Services installation
;

[hcwDVBS.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall

[hcwDVBS.NT.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall



[hcwDVBST]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration
AddReg=     HCW88TSE.AddReg,hcwDVBT.AddReg,hcwDVBS.AddReg
CopyFiles=  CX88TSE.CopyDrivers

[hcwDVBST.NT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT
AddReg=     HCW88TSE.AddReg,hcwDVBT.AddReg,hcwDVBS.AddReg
CopyFiles=  CX88TSE.CopyDrivers

;
; Interfaces installation
;

[hcwDVBST.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

[hcwDVBST.NT.Interfaces]
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

;
; Services installation
;

[hcwDVBST.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall

[hcwDVBST.NT.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall




[DOVER]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration
AddReg=     HCW88TSE.AddReg,DOVER.AddReg,hcwDVBT.AddReg
CopyFiles=  CX88TSE.CopyDrivers

[DOVER.NT]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration, KSCAPTUR.Registration.NT
AddReg=     HCW88TSE.AddReg,DOVER.AddReg,hcwDVBT.AddReg
CopyFiles=  CX88TSE.CopyDrivers


[DOVER.AddReg]
; Macrovision
HKR,"DriverData","EncoderMVDRM",0x00010001,   0x00,0x00,0x00,0x00
HKR,"DriverData","DeferFWLoad",0x00010001,   0x01,0x00,0x00,0x00

;Register the name of the 656, and I2S pins
HKLM,%MediaCategories%\%GUID.PINNAME_656_IN%,Name,,%PinName.656_IN%
HKLM,%MediaCategories%\%GUID.PINNAME_I2S_IN%,Name,,%PinName.I2S_IN%

;Name of the MPEG output pin.
HKLM,%MediaCategories%\%TPPinID%,Display,1, 00,00,00,00
HKLM,%MediaCategories%\%TPPinID%,Name,,%TPpinName%

;Add the property pages

HKCR,CLSID\%GUID.General_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.General_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.General_Properties%,,,

HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Video_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Video_Properties%,,,

HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Audio_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Audio_Properties%,,,

HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.MPEG_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.MPEG_Properties%,,,

HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Diagnostic_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Diagnostic_Properties%,,,

HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,,,hcw88prx.ax
HKCR,CLSID\%GUID.Noise_Properties%\InprocServer32,ThreadingModel,,Both
HKLM,%MediaSets%\%GUID.IVAC_PROPERTIES%\PropertyPages\%GUID.Noise_Properties%,,,

;Register the encoder and multiplexer classes with Direct X
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,CLSID,,%GUID.Encoder%
HKCR,%ActiveMovieCategories%\%GUID.Encoder%,FriendlyName,,%Category_Encoders%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,CLSID,,%GUID.Multiplexer%
HKCR,%ActiveMovieCategories%\%GUID.Multiplexer%,FriendlyName,,%Category_Multiplexers%

;Register the names of the encoder and multiplexer nodes
HKLM,%MediaCategories%\%GUID.Encoder%,Name,,%Node.Encoder%
HKLM,%MediaCategories%\%GUID.Encoder%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%GUID.Multiplexer%,Name,,%Node.Multiplexer%
HKLM,%MediaCategories%\%GUID.Multiplexer%,Display,1,00,00,00,00


;
; Interfaces installation
;

[DOVER.Interfaces]
AddInterface=%GUID.Encoder%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface=%GUID.Multiplexer%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,

[DOVER.NT.Interfaces]
AddInterface=%GUID.Encoder%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface=%GUID.Multiplexer%,%EncFilterReferenceGUID%,DOVER_Interface,
AddInterface={FD0A5AF4-B41D-11d2-9C95-00C04F7971E0},%TSFilterReferenceGUID%,TS_Interface,


[DOVER_Interface]
AddReg=DOVER_Interface.AddReg

[DOVER_Interface.AddReg]
HKR,,CLSID,,{17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%MPEGEncFriendlyName%
;Add interfaces for Microsoft's video bit rate property set
; CLSID_IVideoEncoderProxy = {B43C4EEC-8C32-4791-9102-508ADA5EE8E7} 
;  Causes KsProxy to expose the IVideoEncoder interface 
HKR,Interfaces\{B43C4EEC-8C32-4791-9102-508ADA5EE8E7},,,
; CLSID_IVideoEncoderCodecAPIProxy = {B05DABD9-56E5-4FDC-AFA4-8A47E91F1C9C} 
;  Causes KsProxy to expose both the IVideoEncoder and ICodecAPI interfaces
HKR,Interfaces\{b05dabd9-56e5-4fdc-afa4-8a47e91f1c9c},,,
; Dynamic Bitrate support
HKR,Capabilities,,,
HKR,Capabilities,"{BB4FAA02-596C-4129-8FB3-74E75421FA02}", 0x00010001,1
;;Encoder property page extension
HKLM,Software\Microsoft\Windows\CurrentVersion\RunOnce,"hcw88prx.ax",,"RunDll32 %10%\system32\drivers\hcw88prx.ax,DllRegisterServer"

;
; Services installation
;

[DOVER.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall

[DOVER.NT.Services]
AddService = HCW88TSE,2,HCW88TSE.ServiceInstall



;
; Driver Configuration Registry Entries
;
[HCW88TSE.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,hcw88tse.sys
HKR,,OkToHibernate,3,01
HKR,,PageOutWhenUnopened,3,00
HKR,,DontSuspendIfStreamsAreRunning,3,01

[HCW88TSE.ServiceInstall]
DisplayName   = %HCW88TSE.ServiceDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\hcw88tse.sys



[hcwDVBT.AddReg]
;
; DVBT TS Configuration Registry Entries
;
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00
;HKR,"DriverData","dwTS_HW_SOP_CNTRL",0x00010001,  0xFF,0xFF,0xFF,0xFF
;HKR,"DriverData","dwDataSRBFrames",0x00010001,    0x0a,0x00,0x00,0x00

; DirectShow Filter output pin names
;;HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Display,1, 00,00,00,00
;;HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Name,,%PSpinName%


[hcwDVBS.AddReg]
;
; DVBS TS Configuration Registry Entries
;
HKR,"DriverData","dwTS_GEN_CNTRL",0x00010001,     0x04,0x00,0x00,0x00
HKR,"DriverData","dwIsTSStream",0x00010001,       0x00,0x00,0x00,0x00
HKR,"DriverData","dwTP_PACKET_SIZE",0x00010001,   0xBC,0x00,0x00,0x00

; DirectShow Filter output pin names
;HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Display,1, 00,00,00,00
;HKLM,System\CurrentControlSet\Control\MediaCategories\%PSPinID%,Name,,%PSpinName%



[TS_Interface]
AddReg=TS_Interface.AddReg

[TS_Interface.AddReg]
HKR,,CLSID,,%Proxy.CLSID%       ; {17CCA71B-ECD7-11D0-B908-00A0C9223196}
HKR,,FriendlyName,,%TSFriendlyName%



;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------

[Strings]
Hauppauge="Hauppauge"
p2.InstallDisk     = "Hauppauge WinTV 88x Drivers Install Disk"
p2.InstallDisk64   = "Hauppauge WinTV 88x Drivers Install Disk (64Bit Components)"
p2.InstallDiskWOW  = "Hauppauge WinTV 88x Drivers Install Disk (WOW64 Components)"

CX88x.null            =    "Hauppauge WinTV 88x (unused function)"

MPEGEncFriendlyName   =    "Hauppauge WinTV 88x MPEG Encoder"

TSFriendlyName        =    "Hauppauge WinTV 88x TS Capture"

HCW88TSE.ServiceDesc  =    "Hauppauge WinTV 88x MPEG/TS Capture"

CHELSEA.DeviceDesc    =    "Hauppauge WinTV 88x TS Capture (90xxx)"

BREMEN.DeviceDesc     =    "Hauppauge WinTV 88x TS Capture (92xxx)"

TRIMODE.DeviceDesc    =    "Hauppauge WinTV 88x TS Capture (14xxx)"

TRIMODE2.DeviceDesc   =    "Hauppauge WinTV 88x TS Capture (69xxx)"

OXFORD.DeviceDesc     =    "Hauppauge WinTV 88x TS Capture (94xxx)"
OXFORDHH.DeviceDesc   =    "Hauppauge WinTV 88x TS Capture (98xxx)"

ROSLYN.DeviceDesc     =    "Hauppauge WinTV 88x MPEG Encoder (28xxx)"

DOVER.DeviceDesc      =    "Hauppauge WinTV 88x MPEG Encoder (96xxx)"

MediaCategories          =    "SYSTEM\CurrentControlSet\Control\MediaCategories"
MediaSets                =    "System\CurrentControlSet\Control\MediaSets"
ActiveMovieCategories    =    "CLSID\{da4e3da0-d07d-11d0-bd50-00a0c911ce86}\Instance"

TPPinID                  =    "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
TPPinName                =    "MPEG Out"

GUID.PINNAME_656_IN      =    "{DFD530C7-36D9-47ff-B838-9A11D215B140}"
PinName.656_IN           =    "656"

GUID.PINNAME_I2S_IN      =    "{DF77FE27-FA59-47d7-BFC4-955DE7A32794}"
PinName.I2S_IN           =    "I2S"

GUID.IVAC_PROPERTIES     =    "{d2185a40-0398-11d3-a53e-00a0c9ef506a}"

EncFilterReferenceGUID   =    "{1C10193D-7DCA-4f55-99D8-00A0C9F21FC7}"
GUID.Encoder             =    "{19689BF6-C384-48fd-AD51-90E58C79F70B}"
GUID.Multiplexer         =    "{7A5DE1D3-01A1-452c-B481-4FA2B96271E8}"

Category_Encoders        =    "WDM Streaming Encoder Devices"
Category_Multiplexers    =    "WDM Streaming Multiplexer Devices"
Node.Encoder             =    "Encoder"
Node.Multiplexer         =    "Multiplexer"

GUID.General_Properties  =    "{1CC63210-AB37-4d6e-9D72-79C02C381CBC}"
GUID.Video_Properties    =    "{1CC63211-AB37-4d6e-9D72-79C02C381CBC}"
GUID.Audio_Properties    =    "{1CC63212-AB37-4d6e-9D72-79C02C381CBC}"
GUID.MPEG_Properties     =    "{1CC63213-AB37-4d6e-9D72-79C02C381CBC}"
GUID.Diagnostic_Properties =  "{1CC63214-AB37-4d6e-9D72-79C02C381CBC}"
GUID.Noise_Properties    =    "{1CC63215-AB37-4d6e-9D72-79C02C381CBC}"


;TS capture related
TSFilterReferenceGUID    =    "{5EA9C066-1DFE-41c5-A2DE-00A0C9F21FC7}"
Proxy.CLSID              =    "{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

;;PSPinID                =    "{1649D2C1-435E-11d3-A94B-00A0C9D8B34E}"
;;PSPinName              =    "MPEG-2 PS"

