; Windows Vista Virtual Serial Port Setup File
; Copyright (c) 2010 Qualcomm Incorporated
; Manufacturer: Qualcomm Incorporated
;

[Version]
signature  = "$WINDOWS NT$"
Class      = Ports
Provider   = %ACER%
ClassGuid  = {4D36E978-E325-11CE-BFC1-08002BE10318}
DriverVer  = 11/10/2011,1.0.0.0
Catalogfile.NTx86 = qcusbser32.cat
Catalogfile.NTamd64  = qcusbser64.cat

[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%ACER% = AcerSerialPort, NTx86, NTamd64

[SourceDisksNames]
 1000 = %AcerSrcDisk%,,,\i386
 1001 = %AcerSrcDisk%,,,\amd64

[SourceDisksFiles.x86]
qcusbser.sys = 1000
  
[SourceDisksFiles.amd64]
qcusbser.sys = 1001



[AcerSerialPort.NTx86]

%AcerDevice33800%  = AcerportInstall00, USB\VID_0502&PID_3380&MI_00
%AcerDevice33802%  = AcerportInstall00, USB\VID_0502&PID_3380&MI_02
%AcerDevice33810%  = AcerportInstall00, USB\VID_0502&PID_3381&MI_00
%AcerDevice33813%  = AcerportInstall00, USB\VID_0502&PID_3381&MI_03
%AcerDevice33822%  = AcerportInstall00, USB\VID_0502&PID_3382&MI_02
%AcerDevice33824%  = AcerportInstall00, USB\VID_0502&PID_3382&MI_04
%AcerDevice339F1%  = AcerportInstall00, USB\VID_0502&PID_339F&MI_01
%AcerDevice339F3%  = AcerportInstall00, USB\VID_0502&PID_339F&MI_03
%AcerDevice33A02%  = AcerportInstall00, USB\VID_0502&PID_33A0&MI_02
%AcerDevice33A04%  = AcerportInstall00, USB\VID_0502&PID_33A0&MI_04
%AcerDevice33A11%  = AcerportInstall00, USB\VID_0502&PID_33A1&MI_01
%AcerDevice33A13%  = AcerportInstall00, USB\VID_0502&PID_33A1&MI_03
%AcerDevice33A22%  = AcerportInstall00, USB\VID_0502&PID_33A2&MI_02
%AcerDevice33A24%  = AcerportInstall00, USB\VID_0502&PID_33A2&MI_04
%AcerDevice33A32%  = AcerportInstall00, USB\VID_0502&PID_33A3&MI_02
%AcerDevice33A34%  = AcerportInstall00, USB\VID_0502&PID_33A3&MI_04
%AcerDevice33A43%  = AcerportInstall00, USB\VID_0502&PID_33A4&MI_03
%AcerDevice33A45%  = AcerportInstall00, USB\VID_0502&PID_33A4&MI_05
%AcerDevice337E0%  = AcerportInstall00, USB\VID_0502&PID_337E
[AcerSerialPort.NTamd64]

%AcerDevice33800%  = AcerportInstall00, USB\VID_0502&PID_3380&MI_00
%AcerDevice33802%  = AcerportInstall00, USB\VID_0502&PID_3380&MI_02
%AcerDevice33810%  = AcerportInstall00, USB\VID_0502&PID_3381&MI_00
%AcerDevice33813%  = AcerportInstall00, USB\VID_0502&PID_3381&MI_03
%AcerDevice33822%  = AcerportInstall00, USB\VID_0502&PID_3382&MI_02
%AcerDevice33824%  = AcerportInstall00, USB\VID_0502&PID_3382&MI_04
%AcerDevice339F1%  = AcerportInstall00, USB\VID_0502&PID_339F&MI_01
%AcerDevice339F3%  = AcerportInstall00, USB\VID_0502&PID_339F&MI_03
%AcerDevice33A02%  = AcerportInstall00, USB\VID_0502&PID_33A0&MI_02
%AcerDevice33A04%  = AcerportInstall00, USB\VID_0502&PID_33A0&MI_04
%AcerDevice33A11%  = AcerportInstall00, USB\VID_0502&PID_33A1&MI_01
%AcerDevice33A13%  = AcerportInstall00, USB\VID_0502&PID_33A1&MI_03
%AcerDevice33A22%  = AcerportInstall00, USB\VID_0502&PID_33A2&MI_02
%AcerDevice33A24%  = AcerportInstall00, USB\VID_0502&PID_33A2&MI_04
%AcerDevice33A32%  = AcerportInstall00, USB\VID_0502&PID_33A3&MI_02
%AcerDevice33A34%  = AcerportInstall00, USB\VID_0502&PID_33A3&MI_04
%AcerDevice33A43%  = AcerportInstall00, USB\VID_0502&PID_33A4&MI_03
%AcerDevice33A45%  = AcerportInstall00, USB\VID_0502&PID_33A4&MI_05
%AcerDevice337E0%  = AcerportInstall00, USB\VID_0502&PID_337E
[AcerportInstall00.NT]
CopyFiles=QCUsbDriverFiles
AddReg = All00, AddReg

[QCUsbDriverFiles]
qcusbser.sys

[DestinationDirs]
DefaultDestDir = 12

[AcerportInstall00.NT.Services]
AddService=qcusbser,  0x00000002, ACER_USBSerialService

[ACER_USBSerialService]
DisplayName   = %ACUSBSER%
ServiceType   = 1
StartType     = 3
ErrorControl  = 1
ServiceBinary = %12%\qcusbser.sys

[All00]
HKR,,NTMPDriver,,qcusbser.sys

[AddReg]
HKR,,PortSubClass,1,01
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[Strings]
ACUSBSER = "Qualcomm USB Device for Legacy Serial Communication"
AcerSrcDisk = "Acer USB Driver Disk"
ACER = "Acer"
AcerDevice33800 = "Acer HS-USB Diagnostics 3380"
AcerDevice33802 = "Acer HS-USB NMEA 3380"
AcerDevice33810 = "Acer HS-USB Diagnostics 3381"
AcerDevice33813  = "Acer HS-USB NMEA 3381"
AcerDevice33822  = "Acer HS-USB Diagnostics 3382"
AcerDevice33824  = "Acer HS-USB NMEA 3382"
AcerDevice339F1  = "Acer HS-USB Diagnostics 339F"
AcerDevice339F3  = "Acer HS-USB NMEA 339F"
AcerDevice33A02  = "Acer HS-USB Diagnostics 33A0"
AcerDevice33A04  = "Acer HS-USB NMEA 33A0"
AcerDevice33A11  = "Acer HS-USB Diagnostics 33A1"
AcerDevice33A13  = "Acer HS-USB NMEA 33A1"
AcerDevice33A22  = "Acer HS-USB Diagnostics 33A2"
AcerDevice33A24  = "Acer HS-USB NMEA 33A2"
AcerDevice33A32  = "Acer HS-USB Diagnostics 33A3"
AcerDevice33A34  = "Acer HS-USB NMEA 33A3"
AcerDevice33A43  = "Acer HS-USB Diagnostics 33A4"
AcerDevice33A45  = "Acer HS-USB NMEA 33A4"
AcerDevice337E0 = "Acer HS-USB Diagnostics 337E"

