;/*++
;
; Copyright (c) 2012  by KYOCERA Corporation
;
;--*/

[Version]
Signature = "$WINDOWS NT$"
Class     = AndroidUsbDeviceClass
ClassGuid = {3F966BD9-FA04-4ec5-991C-D326973B5128}
Provider  = %KYOCERA%
DriverVer=06/20/2012,2.0.0.0
CatalogFile=kc02us_adb.cat

; ================= Device section =====================
;
; This section seems to be required for WinUsb driver installation.
; If this section is removed the installer will report an error
; "Required section not found in INF file".
;
[ClassInstall32]
Addreg = AndroidWinUsbClassReg

[AndroidWinUsbClassReg]
HKR,,,0,%ClassName%
HKR,,Icon,,-1

[Manufacturer]
%MfgName%=Kyocera, NTx86, NTamd64

[Kyocera.NTx86]
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_051B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0524&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0546&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0548&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0556&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0557&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0558&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0559&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0572&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0573&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_057f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0580&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0590&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0594&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0595&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0596&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0597&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0598&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0599&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ab&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05AF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dc&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dd&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e4&MI_02

[Kyocera.NTamd64]
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_051B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0524&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_052C&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0546&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0548&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0556&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0557&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_056F&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0558&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0559&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055A&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_055B&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0572&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0573&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_057f&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0580&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058D&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058E&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_058f&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0590&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0594&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0595&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0596&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0597&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0598&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_0599&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059D&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_059E&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A8&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05A9&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05aa&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05ab&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05AF&MI_04
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05B0&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dc&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05dd&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05df&MI_02
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e0&MI_01
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e3&MI_03
%CompositeAdbInterface%     = USB_Install, USB\VID_0482&PID_05e4&MI_02

[USB_Install]
Include = winusb.inf
Needs   = WINUSB.NT

[USB_Install.Services]
Include     = winusb.inf
AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService = WINUSB, WinUSB_Install

[WinUSB_Install]
KmdfLibraryVersion = 1.9

[USB_Install.HW]
AddReg  = Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"

[USB_Install.CoInstallers]
AddReg    = CoInstallers_AddReg
CopyFiles = CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll  = 1
WdfCoInstaller01009.dll = 1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll  = 2
WdfCoInstaller01009.dll = 2

[Strings]
KYOCERA                     = "KYOCERA Corporation"
MfgName                     = "KYOCERA Corporation"
SingleAdbInterface          = "Android ADB Interface"
CompositeAdbInterface       = "Android Composite ADB Interface"
SingleBootLoaderInterface   = "Android Bootloader Interface"
WinUSB_SvcDesc              = "Android USB Driver"
DISK_NAME                   = "Android WinUsb installation disk"
ClassName                   = "Android Phone"

