; Windows Modem Setup File
; Copyright (c) 1993-2007 Sierra Wireless Inc.
; Manufacturer: Sierra Wireless Inc.
;****************************************************************************
;ACGPRSModem
;Ver 2.0.0.30
;Windows 2K/XP
;****************************************************************************

[Version]
Signature    = "$CHICAGO$"
Class        = Modem
ClassGUID    = {4D36E96D-E325-11CE-BFC1-08002BE10318}
Provider     = %SWI%
DriverVer    = 03/22/2007,2.0.0.30
CatalogFile  = mdmacgprs.cat

[Manufacturer]
%SWI% = SWI, NTamd64

[SWI]
%ACGPRS% = ModemCardGPRS, MF\AirCardGPRS_DEV0
%ACEDGE% = ModemCardEDGE, MF\AirCardEDGE_DEV0
%PC7000% = ModemCardGPRS, MF\PC7000_DEV0
%PC7200% = ModemCardEDGE, MF\PC7200_DEV0
%AC850%  = ModemCard3G,   MF\AirCard850_DEV0
%AC860%  = ModemCard3G,   MF\AirCard860_DEV0

[SWI.NTamd64]
%ACGPRS% = ModemCardGPRS, MF\AirCardGPRS_DEV0
%ACEDGE% = ModemCardEDGE, MF\AirCardEDGE_DEV0
%PC7000% = ModemCardGPRS, MF\PC7000_DEV0
%PC7200% = ModemCardEDGE, MF\PC7200_DEV0
%AC850%  = ModemCard3G,   MF\AirCard850_DEV0
%AC860%  = ModemCard3G,   MF\AirCard860_DEV0

[Strings]
SWI="Sierra Wireless Inc"  
ACGPRS="Sierra Wireless AirCard GPRS Modem"
ACEDGE="Sierra Wireless AirCard EDGE Modem"
PC7000="PC7000 GPRS Modem"
PC7200="PC7200 EDGE Modem"
AC850 ="Sierra Wireless AirCard 3G Modem"
AC860 ="Sierra Wireless AirCard 3G Modem"

[ModemCardGPRS]
AddReg=ALL, GenReg, PCMCIA, GenericAddReg, AddRegGPRS
DriverVer = 03/22/2007,2.0.0.30

[ModemCardEDGE]
AddReg=ALL, GenReg, PCMCIA, GenericAddReg, AddRegEDGE
DriverVer = 03/22/2007,2.0.0.30

[ModemCard3G]
AddReg=ALL, GenReg, PCMCIA, GenericAddReg, AddReg3G
DriverVer = 03/22/2007,2.0.0.30

[All]
HKR,,FriendlyDriver,,Unimodem.vxd
HKR,,DevLoader,,*VCOMM
HKR,,ConfigDialog,,modemui.dll
HKR,,PortSubClass,1,02
HKR,,EnumPropPages,,"modemui.dll,EnumPropPages"


[GenReg]
HKR,, Properties, 1, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 00,00,00,00, 10,00,00,00, 00,C2,01,00, 00,C2,01,00

[PCMCIA]
HKR,,PortDriver,,Serial.vxd
HKR,,Contention,,*vcd
HKR,,DeviceType, 1, 03

[GenericAddReg]
HKR, Init, 1,, "AT<cr>"
HKR, Init, 2,, "AT&F&D2&C1S0=0<cr>"
HKR, Init, 3,, "ATE0V1<cr>"
HKR, Monitor, 1,, "ATS0=0<cr>"
HKR, Monitor, 2,, "None"
HKR, Answer, 1,, "ATA<cr>"
HKR, Hangup, 1,, "ATH<cr>"
HKR,, Reset,, "ATZ<cr>"
HKR, Settings, Prefix,, "AT"
HKR, Settings, Terminator,, "<cr>"
HKR, Settings, DialPrefix,, "D"
HKR, Settings, DialSuffix,, ""
HKR, Settings, Pulse,, "P"
HKR, Settings, Tone,, "T"

HKR, Settings, FlowControl_Off,,  "+IFC=0,0"
HKR, Settings, FlowControl_Soft,, "+IFC=1,1"
HKR, Settings, FlowControl_Hard,, "+IFC=2,2"


HKR, Responses, "0<cr>",       1, 00, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "1<cr>",       1, 02, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "2<cr>",       1, 08, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "3<cr>",       1, 04, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "4<cr>",       1, 03, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "6<cr>",       1, 05, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "7<cr>",       1, 06, 00, 00,00,00,00, 00,00,00,00 
HKR, Responses, "8<cr>",       1, 07, 00, 00,00,00,00, 00,00,00,00 

HKR, Responses, "<cr><lf>OK<cr><lf>",          1, 00, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>ERROR<cr><lf>",       1, 03, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO CARRIER<cr><lf>",  1, 04, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO DIALTONE<cr><lf>", 1, 05, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>BUSY<cr><lf>",        1, 06, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>NO ANSWER<cr><lf>",   1, 07, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RING<cr><lf>",        1, 08, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>RINGING<cr><lf>",     1, 01, 00, 00,00,00,00, 00,00,00,00
HKR, Responses, "<cr><lf>DIALING<cr><lf>",     1, 01, 00, 00,00,00,00, 00,00,00,00

[AddRegGPRS]
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 40,9C,00,00, 00,00,00,00

[AddRegEDGE]
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 60,5B,03,00, 00,00,00,00

[AddReg3G]
HKR, Responses, "<cr><lf>CONNECT<cr><lf>",     1, 02, 00, 40,77,1B,00, 00,00,00,00




