;-------------------------------------------------------------------------------
; net9500-x86-n630f.inf
;
; SMSC LAN9500 USB to Ethernet Adapter installation script for x86.
;
; Copyright (c) SMSC.  All rights reserved.

[version]
Signature   = "$Windows NT$"
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Class       = Net
Provider    = %V_SMSC%
DriverPackageDisplayName = %LAN9500.PackageDesc.ntx86%
CatalogFile = lan9500-x86-n630f.cat
DriverVer   = 04/14/2015,2.7.1.0

[ControlFlags]
ExcludeFromSelect = USB\VID_0424&PID_9500   ; LAN9500 with default LEDs.
ExcludeFromSelect = USB\VID_0424&PID_9505   ; LAN9505 with default LEDs.
ExcludeFromSelect = USB\VID_0424&PID_9E00   ; LAN9500A with default LEDs.
ExcludeFromSelect = USB\VID_0424&PID_9E01   ; LAN9505A with default LEDs.
ExcludeFromSelect = USB\VID_0424&PID_EC00   ; LAN9512/LAN9514 with default LEDs.
ExcludeFromSelect = USB\VID_0424&PID_9900   ; LAN9500 with separate (SW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9901   ; LAN9505 with separate (SW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9902   ; LAN9500A with separate (SW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9903   ; LAN9505A with separate (SW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9904   ; LAN9512/LAN9514 with separate (SW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9905   ; LAN9500A with separate (HW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9906   ; LAN9505A with separate (HW driven) Link/Act LEDs
ExcludeFromSelect = USB\VID_0424&PID_9E08   ; Auto Thera
ExcludeFromSelect = USB\VID_0424&PID_9E09   ; 
ExcludeFromSelect = USB\VID_0424&PID_9530   ; 
ExcludeFromSelect = USB\VID_0424&PID_9535   ; 
ExcludeFromSelect = USB\VID_0424&PID_9730   ; 
ExcludeFromSelect = USB\VID_0424&PID_9735   ; 

[Manufacturer]
%V_SMSC%=SMSC,ntx86

[SMSC.ntx86]
%LAN9500.DeviceDesc%    = LAN9500.ndi.ntx86, USB\VID_0424&PID_9500
%LAN9505.DeviceDesc%    = LAN9500.ndi.ntx86, USB\VID_0424&PID_9505
%LAN9E00.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9E00
%LAN9E01.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9E01
%LANEC00.DeviceDesc%    = LAN9500.ndi.ntx86, USB\VID_0424&PID_EC00          
%LAN9900.DeviceDesc%    = LAN9500-SAL10.ndi.ntx86, USB\VID_0424&PID_9900
%LAN9901.DeviceDesc%    = LAN9500-SAL10.ndi.ntx86, USB\VID_0424&PID_9901
%LAN9902.DeviceDesc%    = LAN9500A-SAL10.ndi.ntx86, USB\VID_0424&PID_9902
%LAN9903.DeviceDesc%    = LAN9500A-SAL10.ndi.ntx86, USB\VID_0424&PID_9903
%LAN9904.DeviceDesc%    = LAN9500-SAL10.ndi.ntx86, USB\VID_0424&PID_9904
%LAN9905.DeviceDesc%    = LAN9500A-HAL.ndi.ntx86, USB\VID_0424&PID_9905
%LAN9906.DeviceDesc%    = LAN9500A-HAL.ndi.ntx86, USB\VID_0424&PID_9906
%LAN9E08.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9E08
%LAN9E09.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9E09
%LAN9530.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9530
%LAN9535.DeviceDesc%    = LAN9500A.ndi.ntx86, USB\VID_0424&PID_9535
%LAN9730.DeviceDesc%    = LAN9730.ndi.ntx86, USB\VID_0424&PID_9730
%LAN9735.DeviceDesc%    = LAN9730.ndi.ntx86, USB\VID_0424&PID_9735

;-------------------------------------------------------------------------------
; SMSC LAN9500 USB 2.0 to Ethernet 10/100 Adapter
;
[LAN9500.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps, DelReg.SelectiveSuspend
AddReg          = LAN9500.ndi.reg, LAN9500.params.reg, LAN9500Gen1st.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9500.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-------------------------------------------------------------------------------
; SMSC LAN9500A USB 2.0 to Ethernet 10/100 Adapter
;
[LAN9500A.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps
AddReg          = LAN9500.ndi.reg, LAN9500.params.reg, LAN9500A.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9500A.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-------------------------------------------------------------------------------
; SMSC LAN9500 USB 2.0 to Ethernet 10/100 Adapter (SAL10)
;
[LAN9500-SAL10.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps, DelReg.SelectiveSuspend
AddReg          = LAN9500-SAL10.ndi.reg, LAN9500.params.reg, LAN9500Gen1st.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9500-SAL10.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-------------------------------------------------------------------------------
; SMSC LAN9500A USB 2.0 to Ethernet 10/100 Adapter (SAL10)
;
[LAN9500A-SAL10.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps
AddReg          = LAN9500-SAL10.ndi.reg, LAN9500.params.reg, LAN9500A.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9500A-SAL10.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-------------------------------------------------------------------------------
; SMSC LAN9500 USB 2.0 to Ethernet 10/100 Adapter (HAL)
;
[LAN9500A-HAL.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps
AddReg          = LAN9500A-HAL.ndi.reg, LAN9500.params.reg, LAN9500A.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9500A-HAL.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-------------------------------------------------------------------------------
; SMSC LAN9730 USB 2.0 to Ethernet 10/100 Adapter
;
[LAN9730.ndi.ntx86]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84                  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
DelReg          = DelReg.UnusedCaps
AddReg          = LAN9500.ndi.reg, LAN9500.params.reg, LAN9730.params.reg
CopyFiles       = LAN9500.CopyFiles.ntx86

[LAN9730.ndi.ntx86.Services]
AddService      = LAN9500, 2, LAN9500.Service.ntx86, LAN9500.EventLog.ntx86

;-----------------------------------------------------------------------------
; Miniport Common
;
[LAN9500.ndi.reg]
HKR,    ,                         BusNumber,           0, "0" 
HKR, Ndi,                         Service,             0, "LAN9500"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042495000100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042495000200, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042495050100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042495050200, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\04249E000100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\04249E010100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\0424EC000100, DisableOnSoftRemove, 1, 01, 00

[LAN9500-SAL10.ndi.reg]
HKR,    ,                         BusNumber,           0, "0" 
HKR,    ,                         LinkLedOnGpio,       0, "10" 
HKR, Ndi,                         Service,             0, "LAN9500"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499000100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499000200, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499010100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499010200, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499020100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499030100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499040100, DisableOnSoftRemove, 1, 01, 00

[LAN9500A-HAL.ndi.reg]
HKR,    ,                         BusNumber,           0, "0" 
HKR,    ,                         LinkActLedCfg,       0, "1" 
HKR, Ndi,                         Service,             0, "LAN9500"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499050100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042499060100, DisableOnSoftRemove, 1, 01, 00

[LAN9500.params.reg]

HKR,Ndi\Params\*SpeedDuplex,ParamDesc,      ,%SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,type,           ,enum
HKR,Ndi\Params\*SpeedDuplex,default,        ,0
HKR,Ndi\Params\*SpeedDuplex\enum,0,         ,%SpeedDuplex_AutoNeg%
HKR,Ndi\Params\*SpeedDuplex\enum,1,         ,%SpeedDuplex_10HD%
HKR,Ndi\Params\*SpeedDuplex\enum,2,         ,%SpeedDuplex_10FD%
HKR,Ndi\Params\*SpeedDuplex\enum,3,         ,%SpeedDuplex_100HD%
HKR,Ndi\Params\*SpeedDuplex\enum,4,         ,%SpeedDuplex_100FD%

HKR,Ndi\Params\*FlowControl,ParamDesc,       ,%FlowControl%
HKR,Ndi\Params\*FlowControl,type,            ,"enum"
HKR,Ndi\Params\*FlowControl,default,         ,"3"
HKR,Ndi\Params\*FlowControl\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*FlowControl\enum,"1",       ,%Tx_Enabled%
HKR,Ndi\Params\*FlowControl\enum,"2",       ,%Rx_Enabled%
HKR,Ndi\Params\*FlowControl\enum,"3",       ,%Rx_And_Tx_Enabled%

HKR,Ndi\Params\NetworkAddress,ParamDesc,    ,%NetAddr%
HKR,Ndi\Params\NetworkAddress,type,         ,edit
HKR,Ndi\Params\NetworkAddress,LimitText,    ,17
HKR,Ndi\Params\NetworkAddress,UpperCase,    ,1
HKR,Ndi\Params\NetworkAddress,default,      ,""
HKR,Ndi\Params\NetworkAddress,optional,     ,1

HKR,Ndi\Params\*PriorityVLANTag,ParamDesc,  ,%PriorityAndVlan%
HKR,Ndi\Params\*PriorityVLANTag,type,       ,"enum"
HKR,Ndi\Params\*PriorityVLANTag,default,    ,"3"
HKR,Ndi\Params\*PriorityVLANTag\enum,"0",   ,%PVDisabled%
HKR,Ndi\Params\*PriorityVLANTag\enum,"3",   ,%PVEnabled%

HKR,Ndi\Params\VlanID,ParamDesc,            ,%VlanID%
HKR,Ndi\Params\VlanID,type,                 ,"word"
HKR,Ndi\Params\VlanID,default,              ,"0"
HKR,Ndi\Params\VlanID,min,                  ,"0"
HKR,Ndi\Params\VlanID,max,                  ,"4095"
HKR,Ndi\Params\VlanID,step,                 ,"1"
HKR,Ndi\Params\VlanID,base,                 ,"10"

HKR,Ndi\Params\USBBandwidthMode,ParamDesc,  ,%USBBwMode%
HKR,Ndi\Params\USBBandwidthMode,type,       ,"enum"
HKR,Ndi\Params\USBBandwidthMode,default,    ,"2"
HKR,Ndi\Params\USBBandwidthMode\enum,"0",   ,%USBBwMaxTput%
HKR,Ndi\Params\USBBandwidthMode\enum,"1",   ,%USBBwFriendly%
HKR,Ndi\Params\USBBandwidthMode\enum,"2",   ,%USBBwAutomatic%

HKR,Ndi\Params\AutoMdix,ParamDesc,          ,%AutoMdix%
HKR,Ndi\Params\AutoMdix,type,               ,"enum"
HKR,Ndi\Params\AutoMdix,default,            ,"3"
HKR,Ndi\Params\AutoMdix\enum,"3",           ,%AMDIXHwStrap%
HKR,Ndi\Params\AutoMdix\enum,"2",           ,%AMDIXOn%
HKR,Ndi\Params\AutoMdix\enum,"1",           ,%AMDIXOff-Swap%
HKR,Ndi\Params\AutoMdix\enum,"0",           ,%AMDIXOff-Normal%

HKR,Ndi\Params\*WakeOnPattern,ParamDesc,    ,%WakePattern%
HKR,Ndi\Params\*WakeOnPattern,type,         ,enum
HKR,Ndi\Params\*WakeOnPattern,default,      ,1
HKR,Ndi\Params\*WakeOnPattern\enum,0,       ,%WakeDisable%
HKR,Ndi\Params\*WakeOnPattern\enum,1,       ,%WakeEnable%

HKR,Ndi\Params\*WakeOnMagicPacket,ParamDesc,,%WakeMagicPkt%
HKR,Ndi\Params\*WakeOnMagicPacket,type,     ,enum
HKR,Ndi\Params\*WakeOnMagicPacket,default,  ,1
HKR,Ndi\Params\*WakeOnMagicPacket\enum,0,   ,%WakeDisable%
HKR,Ndi\Params\*WakeOnMagicPacket\enum,1,   ,%WakeEnable%

HKR,,DrvCmdMode, 0, "2"

[LAN9500Gen1st.params.reg]

HKR,,AutoMdixMode, 0, "0" 

[LAN9500A.params.reg]

HKR,,AutoMdixMode, 0, "2" 

HKR,Ndi\Params\SleepPhyOnLinkDown,ParamDesc,     ,%EDPD%
HKR,Ndi\Params\SleepPhyOnLinkDown,type,          ,"enum"
HKR,Ndi\Params\SleepPhyOnLinkDown,default,       ,"0"
HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"0",      ,%EDPDOFF%
HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"1",      ,%EDPDON%

HKR,Ndi\Params\*SelectiveSuspend,ParamDesc, ,%SSuspend%
HKR,Ndi\Params\*SelectiveSuspend,type,      ,enum
HKR,Ndi\Params\*SelectiveSuspend,default,   ,1
HKR,Ndi\Params\*SelectiveSuspend\enum,0,    ,%SSDisable%
HKR,Ndi\Params\*SelectiveSuspend\enum,1,    ,%SSEnable%

HKR,Ndi\Params\*SSIdleTimeout,ParamDesc,    ,%SSIdleTimeout%
HKR,Ndi\Params\*SSIdleTimeout,default,      ,"10"
HKR,Ndi\Params\*SSIdleTimeout,type,         ,"int"
HKR,Ndi\Params\*SSIdleTimeout,min,          ,"1"
HKR,Ndi\Params\*SSIdleTimeout,max,          ,"10"
HKR,Ndi\Params\*SSIdleTimeout,step,         ,"1"
HKR,Ndi\Params\*SSIdleTimeout,base,         ,"10"

HKR,,EDPDConfig, 0, "B000" 

HKR,,LinkWakeModes, 0, "80000040" 

[LAN9730.params.reg]

HKR,,AutoMdixMode, 0, "2" 

HKR,Ndi\Params\SleepPhyOnLinkDown,ParamDesc,     ,%EDPD%
HKR,Ndi\Params\SleepPhyOnLinkDown,type,          ,"enum"
HKR,Ndi\Params\SleepPhyOnLinkDown,default,       ,"0"
HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"0",      ,%EDPDOFF%
HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"1",      ,%EDPDON%

HKR,Ndi\Params\*SelectiveSuspend,ParamDesc, ,%SSuspend%
HKR,Ndi\Params\*SelectiveSuspend,type,      ,enum
HKR,Ndi\Params\*SelectiveSuspend,default,   ,1
HKR,Ndi\Params\*SelectiveSuspend\enum,0,    ,%SSDisable%
HKR,Ndi\Params\*SelectiveSuspend\enum,1,    ,%SSEnable%

HKR,Ndi\Params\*SSIdleTimeout,ParamDesc,    ,%SSIdleTimeout%
HKR,Ndi\Params\*SSIdleTimeout,default,      ,"10"
HKR,Ndi\Params\*SSIdleTimeout,type,         ,"int"
HKR,Ndi\Params\*SSIdleTimeout,min,          ,"1"
HKR,Ndi\Params\*SSIdleTimeout,max,          ,"10"
HKR,Ndi\Params\*SSIdleTimeout,step,         ,"1"
HKR,Ndi\Params\*SSIdleTimeout,base,         ,"10"

HKR,,EDPDConfig, 0, "B000" 

HKR,,LinkWakeModes, 0, "80000040" 

[DelReg.UnusedCaps]
HKR,Ndi\Params\NetDetach
HKR,Ndi\Params\MediaType
HKR,Ndi\Params\FlowControl
HKR,Ndi\Params\PriorityVLANTag

[DelReg.SelectiveSuspend]
HKR,Ndi\Params\*SelectiveSuspend
HKR,Ndi\Params\*SSIdleTimeout

;-----------------------------------------------------------------------------
; Driver and Service Section
;
[LAN9500.CopyFiles.ntx86]
lan9500-x86-n630f.sys,,,2

[LAN9500.Service.ntx86]
DisplayName     = %LAN9500.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\lan9500-x86-n630f.sys
LoadOrderGroup  = NDIS

[LAN9500.EventLog.ntx86]
AddReg = LAN9500.AddEventLog.Reg.ntx86

[LAN9500.AddEventLog.Reg.ntx86]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\lan9500-x86-n630f.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; WDF Coinstaller installation section
;
[LAN9500.ndi.ntx86.CoInstallers]
AddReg=LAN9500.CoInstaller.AddReg
CopyFiles=LAN9500.CoInstaller.CopyFiles

[LAN9500A.ndi.ntx86.CoInstallers]
AddReg=LAN9500.CoInstaller.AddReg
CopyFiles=LAN9500.CoInstaller.CopyFiles

[LAN9500-SAL10.ndi.ntx86.CoInstallers]
AddReg=LAN9500.CoInstaller.AddReg
CopyFiles=LAN9500.CoInstaller.CopyFiles

[LAN9500A-SAL10.ndi.ntx86.CoInstallers]
AddReg=LAN9500.CoInstaller.AddReg
CopyFiles=LAN9500.CoInstaller.CopyFiles

[LAN9500A-HAL.ndi.ntx86.CoInstallers]
AddReg=LAN9500.CoInstaller.AddReg
CopyFiles=LAN9500.CoInstaller.CopyFiles

[LAN9500.CoInstaller.AddReg]
HKR,,CoInstallers32,0x00010000, "WdfCoInstaller01011.dll,WdfCoInstaller"

[LAN9500.CoInstaller.CopyFiles]
WdfCoInstaller01011.dll

[LAN9500.ndi.ntx86.Wdf]
KmdfService = LAN9500, LAN9500.wdfsect

[LAN9500A.ndi.ntx86.Wdf]
KmdfService = LAN9500, LAN9500.wdfsect

[LAN9500-SAL10.ndi.ntx86.Wdf]
KmdfService = LAN9500, LAN9500.wdfsect

[LAN9500A-SAL10.ndi.ntx86.Wdf]
KmdfService = LAN9500, LAN9500.wdfsect

[LAN9500A-HAL.ndi.ntx86.Wdf]
KmdfService = LAN9500, LAN9500.wdfsect

[LAN9500.wdfsect]
KmdfLibraryVersion = 1.11

;-----------------------------------------------------------------------------
; Files
;
[SourceDisksNames]
1 = %SMSC_DISK_NAME%,,,""

[SourceDisksFiles]
lan9500-x86-n630f.sys                       = 1,,
WdfCoInstaller01011.dll = 1

;-----------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
LAN9500.CopyFiles.ntx86 = 12
LAN9500.CoInstaller.CopyFiles = 11

;-----------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
V_SMSC="SMSC"
LAN9500.DeviceDesc          = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter"
LAN9505.DeviceDesc          = "LAN9505 USB 2.0 to Ethernet 10/100 Adapter"
LAN9E00.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter"
LAN9E01.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter"
LANEC00.DeviceDesc          = "LAN9512/LAN9514 USB 2.0 to Ethernet 10/100 Adapter"
LAN9900.DeviceDesc          = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9901.DeviceDesc          = "LAN9505 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9902.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9903.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9904.DeviceDesc          = "LAN9512/LAN9514 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9905.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter (HAL)"
LAN9906.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter (HAL)"
LAN9E08.DeviceDesc          = "LAN89530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9E09.DeviceDesc          = "LAN89530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9730.DeviceDesc          = "LAN9730 USB 2.0 to Ethernet 10/100 Adapter"
LAN9735.DeviceDesc          = "LAN9730 USB 2.0 to Ethernet 10/100 Adapter"
LAN9530.DeviceDesc          = "LAN9530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9535.DeviceDesc          = "LAN9530 USB 2.0 to Ethernet 10/100 Adapter"


LAN9500.PackageDesc.ntx86   = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter x86 Driver"
LAN9500.Service.DispName    = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter Service"
SMSC_DISK_NAME="LAN9500 USB to Ethernet Driver Files"

;Parameters and values
FlowControl     = "Flow Control"
Disabled            = "Disabled"
Tx_Enabled          = "Tx Enabled"
Rx_Enabled          = "Rx Enabled"
Rx_And_Tx_Enabled   = "Rx & Tx Enabled"

SpeedDuplex         = "Speed & Duplex"
SpeedDuplex_AutoNeg = "Auto Negotiation"
SpeedDuplex_10HD    = "10 Mbps Half Duplex"
SpeedDuplex_10FD    = "10 Mbps Full Duplex"
SpeedDuplex_100HD   = "100 Mbps Half Duplex"
SpeedDuplex_100FD   = "100 Mbps Full Duplex"

NetAddr         = "Network Address"

PriorityAndVlan = "Priority & VLAN"
PVDisabled      = "Priority & VLAN Disabled"
PVEnabled       = "Priority & VLAN Enabled"
VlanID          = "VLAN ID"

USBBwMode       = "USB Bandwidth Usage Mode"
USBBwMaxTput    = "Maximum Throughput"
USBBwFriendly   = "Sharing Friendly"
USBBwAutomatic  = "Automatic"

EDPD            = "Energy Detect Power Down"
EDPDOFF         = "Disabled"
EDPDON          = "Enabled"

AutoMdix        = "Auto Mdix"
AMDIXOn         = "ON"
AMDIXOff-Swap   = "OFF / Crossed"
AMDIXOff-Normal = "OFF / Straight"
AMDIXHwStrap    = "HW Controlled"

AutoMdixMode    = "Auto Mdix Mode"
AMDIXModeAuto   = "Automatic ON/OFF"
AMDIXModeOn8023 = "ON with 802.3 timing"
AMDIXModeOnXtnd = "ON with Extended timing"

SSuspend        = "Selective Suspend"
SSEnable        = "Enabled"
SSDisable       = "Disabled"

SSIdleTimeout   = "Selective Suspend Idle Timeout"

WakePattern     = "Wake on pattern match"
WakeMagicPkt    = "Wake on magic packet"
WakeDisable     = "Disabled"
WakeEnable      = "Enabled"

[Strings.0011] ; Japanese
V_SMSC="SMSC"
LAN9500.DeviceDesc          = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter"
LAN9505.DeviceDesc          = "LAN9505 USB 2.0 to Ethernet 10/100 Adapter"
LAN9E00.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter"
LAN9E01.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter"
LANEC00.DeviceDesc          = "LAN9512/LAN9514 USB 2.0 to Ethernet 10/100 Adapter"
LAN9900.DeviceDesc          = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9901.DeviceDesc          = "LAN9505 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9902.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9903.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9904.DeviceDesc          = "LAN9512/LAN9514 USB 2.0 to Ethernet 10/100 Adapter (SAL10)"
LAN9905.DeviceDesc          = "LAN9500A USB 2.0 to Ethernet 10/100 Adapter (HAL)"
LAN9906.DeviceDesc          = "LAN9505A USB 2.0 to Ethernet 10/100 Adapter (HAL)"
LAN9E08.DeviceDesc          = "LAN89530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9E09.DeviceDesc          = "LAN89530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9730.DeviceDesc          = "LAN9730 USB 2.0 to Ethernet 10/100 Adapter"
LAN9735.DeviceDesc          = "LAN9730 USB 2.0 to Ethernet 10/100 Adapter"
LAN9530.DeviceDesc          = "LAN9530 USB 2.0 to Ethernet 10/100 Adapter"
LAN9535.DeviceDesc          = "LAN9530 USB 2.0 to Ethernet 10/100 Adapter"


LAN9500.PackageDesc.ntx86   = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter x86 Driver"
LAN9500.Service.DispName    = "LAN9500 USB 2.0 to Ethernet 10/100 Adapter Service"
SMSC_DISK_NAME="LAN9500 USB to Ethernet Driver Files"

;Parameters and values
FlowControl         = "フロー制御"
Disabled            = "無効"
Tx_Enabled          = "送信有効"
Rx_Enabled          = "受信有効"
Rx_And_Tx_Enabled   = "送信/受信有効"

SpeedDuplex         = "速度と半二重/全二重"
SpeedDuplex_AutoNeg = "オートネゴシエーション"
SpeedDuplex_10HD    = "10Mbps/半二重"
SpeedDuplex_10FD    = "10Mbps/全二重"
SpeedDuplex_100HD   = "100Mbps/半二重"
SpeedDuplex_100FD   = "100Mbps/全二重"

NetAddr         = "ネットワークアドレス"

PriorityAndVlan = "優先/VLAN"
PVDisabled      = "優先/VLAN 無効"
PVEnabled       = "優先/VLAN 有効"
VlanID          = "VLAN ID"

USBBwMode       = "USB帯域使用モード"
USBBwMaxTput    = "最大スループット"
USBBwFriendly   = "適切に共有"
USBBwAutomatic  = "自動"

EDPD            = "エナジー検出パワーダウン"
EDPDOFF         = "無効"
EDPDON          = "有効"

AutoMdix        = "自動MDIX"
AMDIXOn         = "オン"
AMDIXOff-Swap   = "オフ/クロス"
AMDIXOff-Normal = "オフ/ストレート"
AMDIXHwStrap    = "ハードウェア制御"

AutoMdixMode    = "自動MDIXモード"
AMDIXModeAuto   = "自動 オン/オフ"
AMDIXModeOn8023 = "802.3タイミングでのオン"
AMDIXModeOnXtnd = "延長タイミングでのオン"

SSuspend        = "セレクティブサスペンド"
SSEnable        = "有効"
SSDisable       = "無効"

SSIdleTimeout   = "セレクティブサスペンド アイドルタイムアウト"

WakePattern     = "ウェイク オン パターンマッチ"
WakeMagicPkt    = "ウェイク オン マジックパケット"
WakeDisable     = "無効"
WakeEnable      = "有効"
