; ux21lcd.inf
; Setup information file for NMV LCD Monitor UX21LCD
;
; Copyright 2004, NEC-Mitsubishi Electronics Display, Inc.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%MITSUBISHI%
CatalogFile=UX21LCD.cat
DriverVer=08/04/2004,4.08.0004.1431

[ControlFlags]
ExcludeFromSelect.nt=Monitor\MEL649B

[DestinationDirs]
UX21LCD.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
UX21LCD.icm=1

[Manufacturer]
%MITSUBISHI%=MITSUBISHI

[MITSUBISHI]
%UX21LCD%=UX21LCD.Install, Monitor\MEL649B

[UX21LCD.Install]
DelReg=DEL_CURRENT_REG
AddReg=UX21LCD.AddReg, 1600, DPMS
CopyFiles=UX21LCD.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

[UX21LCD.AddReg]
HKR,"MODES\1600,1200",Mode1,,"30.0-96.0,48.0-87.0,+,+"
HKR,,ICMProfile,0,"UX21LCD.icm"

[UX21LCD.CopyFiles]
UX21LCD.icm

[Strings]
MITSUBISHI="NEC-Mitsubishi"
UX21LCD="MITSUBISHI TFT UX21LCD"
Disk1="NEC-Mitsubishi Monitor Installation Disk"