; nl19wcxm.inf
; Setup information file for NEC MultiSync 1940WCXM Monitor
;
; Copyright 2005, NEC Display Solutions, Ltd.
;-------------------------------------------------
[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%NECDS%
CatalogFile=nl19wcxm.cat
DriverVer=06/27/2006,1.06.0627.1245

[ControlFlags]
ExcludeFromSelect.nt=Monitor\NEC66CA

[DestinationDirs]
1940WCXM.CopyFiles=23
DefaultDestDir=11

[SourceDisksNames]
1=%Disk1%,,,

[SourceDisksFiles]
nl19wcxm.icm=1

[Manufacturer]
%NECDS%=NECDS,ntamd64

[NECDS]
%1940WCXM%=1940WCXM.Install, Monitor\NEC66CA

[NECDS.ntamd64]
%1940WCXM%=1940WCXM.Install.ntamd64, Monitor\NEC66CA

[1940WCXM.Install]
DelReg=DEL_CURRENT_REG
AddReg=1940WCXM.AddReg, 1440, DPMS
CopyFiles=1940WCXM.CopyFiles

[1940WCXM.Install.ntamd64]
DelReg=DEL_CURRENT_REG
AddReg=1940WCXM.AddReg, 1440, DPMS
CopyFiles=1940WCXM.CopyFiles

[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

[1440]
HKR,,MaxResolution,,"1440,900"

[DPMS]
HKR,,DPMS,,1

[1940WCXM.AddReg]
HKR,"MODES\1440,900",Mode1,,"31.0-82.0,56.0-76.0,+,+"
HKR,,ICMProfile,0,"nl19wcxm.icm"

[1940WCXM.CopyFiles]
nl19wcxm.icm

[Strings]
NECDS="NEC"
1940WCXM="NEC MultiSync 1940WCXM"
Disk1="NEC Monitor Installation Disk"