;
; AVerCamBulkASIC.INF - USB Video Camera for AVerVision Digital Presenter
;
; Copyright (c) AVer Information Incorporated.  All rights reserved.
;               

[Version]
signature="$CHICAGO$"
CatalogFile=usbAverVision.cat       ; This file is required and is supplied by WHQL when driver is certifed.
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
; Provider listed is Microsoft, but should be the organization who wrote this INF. 
Provider=%Msft%
; LayoutFile needed only for Windows 9x/Me
LayoutFile=layout.inf,layout1.inf,layout2.inf
DriverVer= 11/22/2011,6.1.0.13  ; See DDK for detail

[SourceDisksNames]
1=%SourceDiskName%,,,

[SourceDisksFiles]
AVerCamBulkASIC.sys=1
; ======For WJPG Codec begin======
Wb9967.dll=1
w67_ctom.ax=1
; ======For WJPG Codec end  ======

[ControlFlags]
; All PnP devices should be excluded from manual AddDevice Applet list
ExcludeFromSelect=*

[Manufacturer]
%AVerInformationMfg%=AVerInformation

[DestinationDirs]
AVerInformation.USBDCam.Files.Ext = 10,System32\Drivers

[AVerInformation]
%AVerUSBVideo.DeviceDesc%=AVerInformation.USBDCam,USB\VID_07CA&PID_FF03,\
                          USB\VID_07CA&PID_FF03&MI_00,\
                          USB\VID_2574&PID_0003,\
                          USB\VID_2574&PID_0003&MI_00,\
                          USB\VID_2574&PID_0007&MI_00

[AVerInformation.USBDCam]
Include=    ks.inf, kscaptur.inf
Needs=      KS.Registration,KSCAPTUR.Registration
AddReg=     AVerInformation.USBDCam.AddReg,Codec.AddReg
CopyFiles=AVerInformation.USBDCam.Files.Ext,AVerInformation.CopyCodec
UpdateInis= AVerInformation.UpdateIni

; WIA
;SubClass=StillImage
;DeviceType=3
;DeviceSubType=0x1
;Capabilities=0x00000031
;DeviceData=AVerInformation.USBDCam.DeviceData
;ICMProfiles="sRGB Color Space Profile.icm"

; ======For WJPG Codec begin======

[AVerInformation.UpdateIni]
system.ini,drivers32,,"VIDC.WJPG=wb9967.dll"

[Codec.AddReg]
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\icm\vidc.WJPG,Description,0,%CodecNameJPGString%
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\icm\vidc.WJPG,Driver,0,Wb9967.dll

[AVerInformation.CopyCODEC]
wb9967.dll
w67_ctom.ax

; ======For WJPG Codec end  ======

[AVerInformation.USBDCam.NT]
Include=    ks.inf, kscaptur.inf, dshowext.inf
Needs=      KS.Registration,KSCAPTUR.Registration.NT, DSHOWEXT.Registration
AddReg=     AVerInformation.USBDCam.AddReg,Codec.AddReg
CopyFiles=AVerInformation.USBDCam.Files.Ext,AVerInformation.CopyCodec
UpdateInis= AVerInformation.UpdateIni
;WIA
;SubClass=StillImage
;DeviceType=3
;DeviceSubType=0x1
;Capabilities=0x00000031
;DeviceData=AVerInformation.USBDCam.DeviceData
;ICMProfiles="sRGB Color Space Profile.icm"

[AVerInformation.USBDCam.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,AVerCamBulkASIC.sys
HKR,,PageOutWhenUnopened,3,01
; WIA
;HKR,,HardwareConfig,1,1
;HKR,,USDClass,,"{0527d1d0-88c2-11d2-82c7-00c04f8ec183}"

[AVerInformation.USBDCam.DeviceData]
Server=local
UI DLL=sti.dll
UI Class ID={5d8ef5a3-ac13-11d2-a093-00c04f72dc3c}

[AVerInformation.USBDCam.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,AVerInformation.USBDCam.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,AVerInformation.USBDCam.Interface

[AVerInformation.USBDCam.NT.Interfaces]
AddInterface=%KSCATEGORY_CAPTURE%,GLOBAL,AVerInformation.USBDCam.Interface
AddInterface=%KSCATEGORY_VIDEO%,GLOBAL,AVerInformation.USBDCam.Interface

[AVerInformation.USBDCam.Interface]
AddReg=AVerInformation.USBDCam.Intf.AddReg
         
[AVerInformation.USBDCam.Intf.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,FriendlyName,,%AVerUSBVideo.DeviceDesc%
HKR,PageAliases,"{71F96464-78F3-11d0-A18C-00A0C9118956}",1,21,E8,C2,3D, 13,47, d2,11, 0xba, 0x41, 0x0, 0xa0, 0xc9, 0xd, 0x2b, 0x5
HKR,PinFactory\1\Interfaces\{5BB95400-52BB-11d2-BA41-00A0C90D2B05},,,


[AVerInformation.USBDCam.NT.Services]
AddService = DCamUSBAverMedia2,0x00000002,AVerInformation.USBDCam.ServiceInstall

[AVerInformation.USBDCam.ServiceInstall]
DisplayName   = %AVerUSBVideo.DeviceDesc%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %10%\System32\Drivers\AVerCamBulkASIC.sys

[AVerInformation.USBDCam.Files.Ext]
AVerCamBulkASIC.sys

[Strings]

;----------------
; Non-Localizable
;----------------

; note: only register value is case sensitive, key is not.
ProxyVCap.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_VIDEO="{6994AD05-93EF-11D0-A3CC-00A0C9223196}"
SERVICE_KERNEL_DRIVER=1
; PnP should use demand start
SERVICE_DEMAND_START=3
SERVICE_ERROR_NORMAL=1

; IHV's extension DLL
; AVerInformation.ExtensionDLL = "???.dll"

;----------------
; Localizable
;----------------

Msft="AVer"
AVerInformationMfg="AVer Information Inc."
AVerUSBVideo.DeviceDesc="USB Video Camera for AverVision Digital Presenter 2"
SourceDiskName="Installation diskette 1"
CodecNameJPGString="JPEG [WJPG]"
