HP WES7 Add-on (Fiber Allied Telesis NIC)
VERSION  : 15.2.0.5
REVISION : A
PASS	 : 1

DESCRIPTION :

  This softpaq provides a way to update the Fiber Allied Telesis NIC.
  

CONTENTS :
  
WES7_Fiber_Allied_Telesis_NIC_15.2.0.5_A1.exe - Install package that installs the Fiber Allied Telesis NIC.

WES7_Fiber_Allied_Telesis_NIC_15.2.0.5_A1.txt - This file.


SPACE REQUIREMENTS :

  This add-on requires uncompressed free space on the flash memory (Drive C:)
  and uncompressed free space in the temporary folder. These space requirements
  must be met in order to successfully deploy this add-on.

  1) Space required on the flash memory for installation: 951 KB
  2) Space required on the flash memory after installation: 675 KB (with NTFS Compression)
  3) Space required in the temporary folder for installation: 967 KB

  To ensure that the temporary folder always has the required amount of free space
  for installation, HP recommends that the %TEMP% and %TMP% variables be
  temporarily redefined to a network share on the deployment server, and that the
  setup program be executed from the deployment server, otherwise, the add-on may fail
  to deploy correctly.

REMARKS :

  The install package, WES7_Fiber_Allied_Telesis_NIC_15.2.0.5_A1.exe, contains only files for updating the
  Fiber Allied Telesis NIC. It does not execute some commands that are needed to complete the installation
  of the component. To successfully deploy this component to the client, the following steps need
  to be done.

  1) Before installing the add-on, disable the write filter and reboot.
  2) Run the install package, then, when complete, manually reboot the unit.
  3) At this point, the write filter can be re-enabled.

  


Copyright (c) 2013 Hewlett-Packard Development Company, L.P.


