;Copyright (c) 2010, TP-LINK TECHNOLOGIES CO., LTD. All Rights Reserved.                       

[version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
DriverVer   = 10/03/2007,6.1971.1003.2007
CatalogFile.NT = netrtx32.cat

[Manufacturer]
%Realtek%   = Realtek, NT.5.1, NTamd64.5.1, NT.6.0, NTamd64.6.0, NT.6.1, NTamd64.6.1

[ControlFlags]
ExcludeFromSelect     = *

[Realtek]
; DisplayName            Section            DeviceID
; -----------            -------            --------
[Realtek.NT.5.1]
;
[Realtek.NTamd64.5.1]
;
[Realtek.NT.6.0]
%RTL8168.DeviceDesc%  = RTL8168.ndi, PCI\VEN_10EC&DEV_8168
[Realtek.NTamd64.6.0]
;
[Realtek.NT.6.1]
;
[Realtek.NTamd64.6.1]
;
; Realtek
;
; Windows NT specific entry
[R8169C7k.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, JumboNolimit.reg, s5wol.reg, powersavingautophy.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8169.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8168.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, powersavingautopcie.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8136.ndi.NT]
Characteristics = 0x84
BusType         = 5
AddReg          = Speed10_100.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = Offload.reg, s5wol.reg, powersavingautopcie.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 

[RTL8168C.ndi.NT]
Characteristics = 0x84
BusType         = 5
DelReg          = del.reg
AddReg          = Speed.reg, NetworkAddress.reg, flowctrl.reg, PriorityVlanTag.reg, InterruptModeration.reg, TxRxBuf.reg
AddReg          = OffloadChksum.reg, Jumboframe.reg, s5wol.reg, powersavingautophy.reg, powersavingautopcie.reg
AddReg          = OffloadIpv6Lsov2.reg, rtk.reg
CopyFiles       = RTL8169.CopyFiles
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 0		; NdisPhysicalMediumUnspecified 


[RTL8168.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8136.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168C.ndi.NT.HW]
AddReg = RTL8168_8136.MSI.AddReg

[RTL8168_8136.MSI.AddReg]
HKR, "Interrupt Management", 0x00000010 
HKR, "Interrupt Management\MessageSignaledInterruptProperties", 0x00000010
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MSISupported, 0x00010001, 0
HKR, "Interrupt Management\MessageSignaledInterruptProperties", MessageNumberLimit, 0x00010001, 1


[RTL8169.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8168.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8136.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog

[RTL8168C.ndi.NT.Services]
AddService = RTL8169, 2, rtl8169.Service, common.EventLog


;-----------------------------------------------------------------------------
; common base for 10/100/1000 Mb Adapters
;
[Speed.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "6",        0, %1000Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"

HKR,Ndi\params\AutoDisableGigabit,       ParamDesc,  0, %AutoDisableGigabit%
HKR,Ndi\params\AutoDisableGigabit,       default,    0, "0"
HKR,Ndi\params\AutoDisableGigabit,       type,       0, "enum"
HKR,Ndi\params\AutoDisableGigabit\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoDisableGigabit\enum,  "1",        0, %BatteryRe-Link%
HKR,Ndi\params\AutoDisableGigabit\enum,  "2",        0, %AcBatteryRe-Link%
HKR,,AutoDisableGigabit,0,"0"

[Speed10_100.reg]
HKR,Ndi\params\*SpeedDuplex,       ParamDesc,  0, %SpeedDuplex%
HKR,Ndi\params\*SpeedDuplex,       default,    0, "0"
HKR,Ndi\params\*SpeedDuplex,       type,       0, "enum"
HKR,Ndi\params\*SpeedDuplex\enum,  "0",        0, %AutoDetect%
HKR,Ndi\params\*SpeedDuplex\enum,  "1",        0, %10Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "2",        0, %10Mb-Full-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "3",        0, %100Mb-Half-Duplex%
HKR,Ndi\params\*SpeedDuplex\enum,  "4",        0, %100Mb-Full-Duplex%
HKR,,*SpeedDuplex,0,"0"


[NetworkAddress.reg]
HKR,Ndi\params\NetworkAddress,	   ParamDesc,  0, %NetworkAddress%
HKR,Ndi\params\NetworkAddress,	   type,       0, "edit"
HKR,Ndi\params\NetworkAddress,	   default,    0, "000000000000"
HKR,Ndi\params\NetworkAddress,	   LimitText,  0, "12"
HKR,Ndi\params\NetworkAddress,	   UpperCase,  0, "1"
HKR,Ndi\params\NetworkAddress,	   Optional,   0, "1"

[flowctrl.reg]
HKR,Ndi\params\*FlowControl,	   ParamDesc,  0, %FlowControl%
HKR,Ndi\params\*FlowControl,	   default,    0, "1"
HKR,Ndi\params\*FlowControl,	   type,       0, "enum"
HKR,Ndi\params\*FlowControl\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*FlowControl\enum,  "1",        0, %Enabled%
HKR,,*FlowControl,0,"1"


[PriorityVlanTag.reg]
HKR,Ndi\params\*PriorityVLANTag,	ParamDesc,  0, %PriorityVLAN%
HKR,Ndi\params\*PriorityVLANTag,	default,    0, "0"
HKR,Ndi\params\*PriorityVLANTag,	type,       0, "enum"
HKR,Ndi\params\*PriorityVLANTag\enum,	"0",        0, %PriorityVLANDisabled%
HKR,Ndi\params\*PriorityVLANTag\enum,	"3",        0, %PriorityVLANEnabled%
HKR,,*PriorityVLANTag,0,"3"

HKR,Ndi\Params\RegVlanid,   ParamDesc,  0, %VLanID%
HKR,Ndi\Params\RegVlanid,   Type,       0, "int"
HKR,Ndi\Params\RegVlanid,   Default,    0, "0"
HKR,Ndi\Params\RegVlanid,   Min,        0, "0"
HKR,Ndi\Params\RegVlanid,   Max,        0, "4094"
HKR,Ndi\Params\RegVlanid,   Step,       0, "1"
HKR,Ndi\Params\RegVlanid,   Base,       0, "10"
HKR,,RegVlanid,0,"0"



[InterruptModeration.reg]
HKR,Ndi\params\*InterruptModeration,	ParamDesc,  0, %InterruptModeration%
HKR,Ndi\params\*InterruptModeration,	default,    0, "1"
HKR,Ndi\params\*InterruptModeration,	type,       0, "enum"
HKR,Ndi\params\*InterruptModeration\enum,	"0",        0, %Disabled%
HKR,Ndi\params\*InterruptModeration\enum,	"1",        0, %Enabled%
HKR,,*InterruptModeration,0,"1"

[TxRxBuf.reg]
HKR,Ndi\Params\*ReceiveBuffers,       ParamDesc,  0, %ReceiveBuffers%
HKR,Ndi\Params\*ReceiveBuffers,       Type,       0, "int"
HKR,Ndi\Params\*ReceiveBuffers,       Default,    0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Min,        0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Max,        0, "512"
HKR,Ndi\Params\*ReceiveBuffers,       Step,       0, "1"
HKR,Ndi\Params\*ReceiveBuffers,       Base,       0, "10"
HKR,,*ReceiveBuffers,0,"512"

HKR,Ndi\Params\*TransmitBuffers,      ParamDesc,  0, %TransmitBuffers%
HKR,Ndi\Params\*TransmitBuffers,      Type,       0, "int"
HKR,Ndi\Params\*TransmitBuffers,      Default,    0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Min,        0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Max,        0, "128"
HKR,Ndi\Params\*TransmitBuffers,      Step,       0, "1"
HKR,Ndi\Params\*TransmitBuffers,      Base,       0, "10"
HKR,,*TransmitBuffers,0,"128"

[Jumboframe.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"

[JumboNolimit.reg]
HKR,Ndi\params\*JumboPacket,        ParamDesc,  0, %JumboFrame%
HKR,Ndi\params\*JumboPacket,        default,    0, "1514"
HKR,Ndi\params\*JumboPacket,        type,       0, "enum"
HKR,Ndi\params\*JumboPacket\enum,   "1514",     0, %Disabled%
HKR,Ndi\params\*JumboPacket\enum,   "2048",     0, %2KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "3072",     0, %3KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "4096",     0, %4KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "5120",     0, %5KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "6144",     0, %6KBMTU%
HKR,Ndi\params\*JumboPacket\enum,   "7168",     0, %7KBMTU%
HKR,,*JumboPacket,0,"1514"
HKR,,LimitCbJumboFrame,0,"0"


[Offload.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"

[OffloadChksum.reg]
HKR,Ndi\params\*IPChecksumOffloadIPv4,        ParamDesc,  0, %IPChksumOffv4%
HKR,Ndi\params\*IPChecksumOffloadIPv4,        default,    0, "3"
HKR,Ndi\params\*IPChecksumOffloadIPv4,        type,       0, "enum"
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "0",        0, %Disabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "1",        0, %TxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "2",        0, %RxEnabled%
HKR,Ndi\params\*IPChecksumOffloadIPv4\enum,   "3",        0, %RxTxEnabled%
HKR,,*IPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*TCPChecksumOffloadIPv4,       ParamDesc,  0, %TCPChksumOffv4%
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv4,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv4,       ParamDesc,  0, %UDPChksumOffv4%
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv4,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv4\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv4,0,"3"

[s5wol.reg]
HKR,Ndi\params\S5WakeOnLan,       ParamDesc,  0, %S5WakeOnLan%
HKR,Ndi\params\S5WakeOnLan,       default,    0, "1"
HKR,Ndi\params\S5WakeOnLan,       type,       0, "enum"
HKR,Ndi\params\S5WakeOnLan\enum,  "0",        0, %Disabled%
HKR,Ndi\params\S5WakeOnLan\enum,  "1",        0, %Enabled%
HKR,,S5WakeOnLan,0,"1"

[powersavingautophy.reg]
HKR,Ndi\params\AutoLinkDownPhyOff,       ParamDesc,  0, %AutoLinkDownPhyOff%
HKR,Ndi\params\AutoLinkDownPhyOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPhyOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPhyOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPhyOff,0,"0"

[powersavingautopcie.reg]
HKR,Ndi\params\AutoLinkDownPcieMacOff,       ParamDesc,  0, %AutoLinkDownPcieMacOff%
HKR,Ndi\params\AutoLinkDownPcieMacOff,       default,    0, "0"
HKR,Ndi\params\AutoLinkDownPcieMacOff,       type,       0, "enum"
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "0",        0, %Disabled%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "1",        0, %Battery%
HKR,Ndi\params\AutoLinkDownPcieMacOff\enum,  "2",        0, %AcBattery%
HKR,,AutoLinkDownPcieMacOff,0,"0"

[OffloadIpv6Lsov2.reg]
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       ParamDesc,  0, %TCPChksumOffv6%
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*TCPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*TCPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*TCPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*UDPChecksumOffloadIPv6,       ParamDesc,  0, %UDPChksumOffv6%
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       default,    0, "3"
HKR,Ndi\params\*UDPChecksumOffloadIPv6,       type,       0, "enum"
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "1",        0, %TxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "2",        0, %RxEnabled%
HKR,Ndi\params\*UDPChecksumOffloadIPv6\enum,  "3",        0, %RxTxEnabled%
HKR,,*UDPChecksumOffloadIPv6,0,"3"

HKR,Ndi\params\*LsoV2IPv4,	ParamDesc,  0, %LSOv2v4%
HKR,Ndi\params\*LsoV2IPv4,	default,    0, "0"
HKR,Ndi\params\*LsoV2IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv4\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv4\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv4,0,"0"

HKR,Ndi\params\*LsoV2IPv6,	ParamDesc,  0, %LSOv2v6%
HKR,Ndi\params\*LsoV2IPv6,	default,    0, "1"
HKR,Ndi\params\*LsoV2IPv6,	type,       0, "enum"
HKR,Ndi\params\*LsoV2IPv6\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*LsoV2IPv6\enum,  "1",        0, %Enabled%
HKR,,*LsoV2IPv6,0,"1"

HKR,Ndi\params\*RSS,	ParamDesc,  0, %RSS%
HKR,Ndi\params\*RSS,	default,    0, "1"
HKR,Ndi\params\*RSS,	type,       0, "enum"
HKR,Ndi\params\*RSS\enum,  "0",        0, %Disabled%
HKR,Ndi\params\*RSS\enum,  "1",        0, %Enabled%
HKR,,*RSS,0,"1"

HKR,Ndi\params\*LsoV1IPv4,	ParamDesc,  0, %LSOv4%
HKR,Ndi\params\*LsoV1IPv4,	default,    0, "1"
HKR,Ndi\params\*LsoV1IPv4,	type,       0, "enum"
HKR,Ndi\params\*LsoV1IPv4\enum,  "0",       0, %Disabled%
HKR,Ndi\params\*LsoV1IPv4\enum,  "1",       0, %Enabled%
HKR,,*LsoV1IPv4,0,"1"


[del.reg]
HKR,Ndi\params\JumboFrame
HKR,,JumboFrame


;-----------------------------------------------------------------------------
; rtk NT specific
;

[rtk.reg]
HKR, Ndi,                       Service,    0, "RTL8169"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces,            UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces,            LowerRange, 0, "ethernet"


[rtl8169.Service]
DisplayName     = %rtl8169.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\Rtlh86.sys
LoadOrderGroup  = NDIS


[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; DestinationDirs
;
[RTL8169.CopyFiles]
Rtlh86.sys,,,2

[SourceDisksNames]
1 = %DiskDescription%,Rtlh86.sys,,


[SourceDisksFiles]
Rtlh86.sys = 1,, ; on distribution disk 1


[DestinationDirs]
RTL8169.CopyFiles  = 12
DefaultDestDir     = 11

[Strings]
Realtek                  = "TP-LINK TECHNOLOGIES CO., LTD."

AutoDetect               = "Auto Negotiation"
SpeedDuplex              = "Speed & Duplex"
10Mb-Half-Duplex         = "10 Mbps Half Duplex"
10Mb-Full-Duplex         = "10 Mbps Full Duplex"
100Mb-Half-Duplex        = "100 Mbps Half Duplex"
100Mb-Full-Duplex        = "100 Mbps Full Duplex"
1000Mb-Full-Duplex       = "1.0 Gbps Full Duplex"
NetworkAddress		 = "Network Address"
IPChksumOffv4            = "IPv4 Checksum Offload"
TCPChksumOffv4           = "TCP Checksum Offload (IPv4)"
UDPChksumOffv4           = "UDP Checksum Offload (IPv4)"
TCPChksumOffv6           = "TCP Checksum Offload (IPv6)"
UDPChksumOffv6           = "UDP Checksum Offload (IPv6)"
Enabled                  = "Enabled"
Disabled                 = "Disabled"
TxEnabled                = "Tx Enabled"
RxEnabled                = "Rx Enabled"
RxTxEnabled              = "Rx & Tx Enabled"
LSOv4                    = "Large Send Offload (IPv4)"
LSOv2v4                  = "Large Send Offload v2 (IPv4)"
LSOv2v6                  = "Large Send Offload v2 (IPv6)"
FlowControl              = "Flow Control"
PriorityVLAN             = "Priority & VLAN"
PriorityVLANDisabled     = "Priority & VLAN Disabled"
PriorityVLANEnabled      = "Priority & VLAN Enabled"
InterruptModeration      = "Interrupt Moderation"
ReceiveBuffers           = "Receive Buffers"
TransmitBuffers          = "Transmit Buffers"
AutoDisableGigabit       = "Auto Disable Gigabit (PowerSaving)"
AutoLinkDownPhyOff       = "Auto Disable PHY (PowerSaving)"
BatteryRe-Link           = "Re-Link, Battery"
AcBatteryRe-Link         = "Re-Link, Battery or AC"
Battery                  = "Enabled, Battery"
AcBattery                = "Enabled, Battery or AC"
JumboFrame               = "Jumbo Frame"
2KBMTU                   = "2KB MTU"
3KBMTU                   = "3KB MTU"
4KBMTU                   = "4KB MTU"
5KBMTU                   = "5KB MTU"
6KBMTU                   = "6KB MTU"
7KBMTU                   = "7KB MTU"
S5WakeOnLan              = "Shutdown Wake-On-Lan"
AutoLinkDownPcieMacOff   = "Auto Disable PCIe (PowerSaving)"
S3S4WolLinkSpeed         = "Sleep WOL Link Speed"
RSS                      = "Receive Side Scaling"
VLanID                   = "VLan ID"

RTL8168.DeviceDesc       = "TP-LINK Gigabit PCI-E Network Adapter"

rtl8169.Service.DispName = "TP-LINK Gigabit PCI-E Network Adapter Driver"

DiskDescription 	 = "TP-LINK Driver Disk 1"

;;;;; InfVer = 1.105
