; Copyright (c) 2009-2015  Intel Corporation  
; **********************************************************************************************  
; **********************************************************************************************  
; **    Filename:  iaAHCIB.inf 
; **    Revision:  DRIVER_INFO 
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Enterprise Driver  
; **               Installs: RSTe AHCI Controller Miniport 
; **********************************************************************************************  
[Version]  
Signature="$Windows NT$"  
Provider=%INTEL%  
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}  
Class=SCSIAdapter  
CatalogFile=iaAHCIB.cat
DriverVer=11/20/2015,4.5.0.1234
; 
[PackageInfo]  
Name=AHCIB  
; 
[SourceDisksNames]  
1 = %DiskId1%,,,""  
[DestinationDirs]  
DefaultDestDir = 12  
; 
[ControlFlags]  
ExcludeFromSelect = *  
; 
[Manufacturer]  
%INTEL% = INTEL, NTamd64.6.2, NTamd64.6.3, NTamd64.10.0
; 
[iaStorB_Service_Inst] 
ServiceType    = %SERVICE_KERNEL_DRIVER%  
StartType      = %SERVICE_BOOT_START%  
ErrorControl   = %SERVICE_ERROR_NORMAL%  
ServiceBinary  = %12%\iaStorB.sys 
LoadOrderGroup = SCSI miniport  
AddReg         = pnpsafe_pci_addreg  
; 
[iaStorB_EventLog_Inst] 
AddReg = iaStorB_EventLog_AddReg 
; 
[iaStorB_EventLog_AddReg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorB.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7  
; 
;********************************************************  
;*  
;* 64-BIT X86 ARCHITECTURE  
;*  
;* This section specifies the 64-bit architecture specific INF file entries  
;* required to install a driver as a 64-bit compatible driver.  
;*  
;******************************************************************************  
[SourceDisksFiles.amd64]   
iaStorB.sys = 1,,,  
; 
[INTEL.NTamd64.10.0] 
;windows_10_64-bit and later 
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_8D62&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_1F32&CC_0106
;
[INTEL.NTamd64.6.3] 
;windows_8.1_64-bit 
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_8D62&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_1F32&CC_0106
;
[INTEL.ntamd64.6.2] 
;windows_8_64-bit
%PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_8D62&CC_0106
%PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc% = iaStorB_inst, PCI\VEN_8086&DEV_1F32&CC_0106
;
[iaStorB_inst.ntamd64]
CopyFiles=@iaStorB.sys
;
[iaStorB_inst.ntamd64.HW]
AddReg = msi_addreg 
AddReg = storport_addreg 
; 
[iaStorB_inst.ntamd64.Services] 
AddService = iaStorB, %SPSVCINST_ASSOCSERVICE%, iaStorB_Service_Inst, iaStorB_EventLog_Inst 
; 
[pnpsafe_pci_addreg] 
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars  
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb 
HKR, Parameters\PnpInterface,  5,                           %REG_TYPE_DWORD%,  0x00000001  
HKR, Parameters,               BusType,                     %REG_TYPE_DWORD%,  0x0000000b 
; Tell Storport in Win7/Srv08R2(KB982018) that driver can report 4K sector size (not needed in Win8) 
HKR, Parameters\Device,        EnableQueryAccessAlignment,  %REG_TYPE_DWORD%,  0x00000001 
; 
[Strings]  
;  
; Localizable Strings  
;  
diskId1 = "RSTe AHCI Installation Disk"  
;server 
PCI\VEN_8086&DEV_8D62&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ series chipset sSATA AHCI Controller"
PCI\VEN_8086&DEV_1F32&CC_0106.DeviceDesc    = "Intel(R) C600+/C220+ series chipset sSATA AHCI Controller"
; 
INTEL = "Intel Corporation" 
; Non-Localizable Strings  
;  
SPSVCINST_ASSOCSERVICE = 0x00000002  
REG_MULTI_SZ           = 0x00010000  
REG_EXPAND_SZ          = 0x00020000  
REG_TYPE_DWORD         = 0x00010001  
SERVICE_KERNEL_DRIVER  = 1  
SERVICE_BOOT_START     = 0  
SERVICE_ERROR_NORMAL   = 1 
; 
; MSI enables.  
[msi_addreg]   
HKR, Interrupt Management, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported,       %REG_TYPE_DWORD%,   1   
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   1  
; 
[storport_addreg] 
;;; Enables/Disables Idle Power Management for StorPort 
HKR, "StorPort", "EnableIdlePowerManagement", %REG_TYPE_DWORD%, 0x00000001
; 
[DefaultInstall]
CopyFiles=@iaStorB.sys
AddReg = msi_addreg
AddReg = storport_addreg
