;/*++
;
;Copyright (c) N-Trig.  All rights reserved.
;
;Module Name:
;
;    NtrigDigi.INF
;
;--*/

[Version]
Signature="$WINDOWS NT$"
Class=Digitizers
ClassGuid={745a17a0-74d3-11d0-b6fe-00a0c90f57da}
Provider=%N-Trig%
DriverVer=06/30/2009,1.26.8.49
CatalogFile.NTx86  = NtrigDigi86.cat


[ControlFlags]
ExcludeFromSelect = *

[Manufacturer]
%StdMfg%=Standard,NTx86.6.1.1

[Standard.NTx86.6.1.1]
%NtrigDevice%=HID_Device, HID\VID_1B96&PID_0001&MI_01&Col02

[HID_Device.NT]
Include = input.inf
Needs = HID_Inst.NT
CopyFiles=HID_Device.NT.Copy

[HID_Device.NT.HW]
Include = input.inf
Needs = HID_Inst.NT

[HID_Device.NT.CoInstallers]
AddReg=HID_Device_CoInstaller_AddReg
CopyFiles=CoInstallers_CopyFiles

[HID_Device_CoInstaller_AddReg]
HKR,,CoInstallers32,0x00010000, "WUDFCoInstaller.dll"

[CoInstallers_CopyFiles]

[HID_Device.NT.Wdf]
UmdfImpersonationLevel = Impersonation
UmdfService = NtrigDigi, HID_Device_wdfsect
UmdfServiceOrder = NtrigDigi
UmdfMethodNeitherAction = Copy
UmdfKernelModeClientPolicy = AllowKernelModeClients

[HID_Device_wdfsect]
UmdfLibraryVersion=1.9.0
DriverCLSID="{a732f3b7-b7d2-461c-82b3-12d8f56287bb}"
ServiceBinary=%12%\UMDF\NtrigDigi.dll

[HID_Device.NT.Services]
AddService = WUDFRd, 0x000001fa, WUDFRD_Service_Inst

[WUDFRD_Service_Inst]
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\WUDFRd.sys

[DestinationDirs]
HID_Device.NT.Copy=12,UMDF

[HID_Device.NT.Copy]
NtrigDigi.dll,,0x0100
SensorInterfaceTrackCoreDLL.dll,,0x0100

[SourceDisksNames]
1=%ntrigdigidisk%

[SourceDisksFiles]
NtrigDigi.dll = 1
SensorInterfaceTrackCoreDLL.dll = 1

[Strings]
ntrigdigidisk="ntrigdigidisk"
N-Trig= "N-Trig"
StdMfg = "N-Trig"
NtrigDevice = "N-Trig MultiTouch HID Device"
