
[version]
Signature  = "$CHICAGO$"
Class      = Net
Compatible = 1
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
provider   = %PC_CARD%
LayoutFile = layout.inf
DriverVer  = 01/17/2000

[Manufacturer]
%PC_CARD%  = PC_CARD

[PC_CARD]
%PC_CARD.DeviceDesc%  = le10cc.ndi, PCMCIA\Ethernet-Adapter-D51F

;----------------------------------------------------------------------------
; Win 2000 main sections
;
[le10cc.ndi.NT]
Characteristics = 0x4
BusType         = 8
AddReg          = le10.ndi.reg
CopyFiles       = le10.ndis5.CopyFiles

[le10cc.ndi.NT.Services]
AddService = le10, 2, le10.Service, le10.AddEventLog

;----------------------------------------------------------------------------
;    Win 2000 Drivers
;
[le10.ndi.reg]
HKR, Ndi,               Service,    0, "le10"
HKR, Ndi\Interfaces,    LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces,    UpperRange, 0, "ndis5"
HKR,               ,    Pcmcia    , 0, "2"

HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00

[le10.ndis5.CopyFiles]
eh10nds.sys,,,2

[le10.Service]
DisplayName     =   %Service.DispName%
ServiceType     =   1 ;%SERVICE_KERNEL_DRIVER%
StartType       =   3 ;%SERVICE_AUTO_START%
ErrorControl    =   1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   =   %12%\eh10nds.sys
LoadOrderGroup  =   NDIS
AddReg          =   TextModeFlags.reg

[le10.AddEventLog]
AddReg = le10.AddEventLog.reg

[le10.AddEventLog.reg]
HKR, , EventMessageFile,0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported,  0x00010001, 7

[TextModeFlags.reg]
HKR, , TextModeFlags, 0x00010001, 0x0001


;----------------------------------------------------------------------------
; Win 9x main sections
;
[le10cc.ndi]
AddReg    = le10X.ndi.reg, ne2000.ndi.reg, Clone.params.reg
LogConfig = le10cc.LogConfigOverride

[le10cc.LogConfigOverride]
IRQConfig=3,4,5,7,10,11,12,13,15
IOConfig=20@200-3FF%FFE0(3FF::)
ConfigPriority = HARDRECONFIG

[le10X.ndi.reg]
HKR,Ndi,DeviceID,,"PCMCIA-Ethernet-Adapter-D51F"
HKR,Ndi,CardType,,"PCMCIA"


;****************************************************************************
; Win 9x Drivers
; Base section for ne2000 users
;
[ne2000.ndi.reg]
; key,subkey,valuname,type,value
HKR,,DevLoader,,*ndis
HKR,,DeviceVxDs,,eh10nds.sys
HKR,,Driver,,"eh10nds.sys"
HKR,,EnumPropPages,,"netdi.dll,EnumPropPages"
; NDIS Info
HKR,NDIS,LogDriverName,,"le10"
HKR,NDIS,MajorNdisVersion,1,03
HKR,NDIS,MinorNdisVersion,1,0A
; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"
; Install sectioins
HKR,Ndi\Install,ndis3,,"le10X.ndis3"

;Install NDIS3
[le10X.ndis3]
CopyFiles = le10X.ndis3.CopyFiles

[le10X.ndis3.CopyFiles]
eh10nds.sys,,,2

;extra params for clones
[Clone.params.reg]
; Resources
HKR,,InterruptNumber,1,04,00,00,00
HKR,,IOBaseAddress,1,02,00,00,00
HKR,NDI\params\InterruptNumber,resc,1,04,00,00,00
HKR,Ndi\params\interruptNumber,ParamDesc,,"Interrupt Level"
HKR,NDI\params\InterruptNumber,flag,1,60,00,00,00
HKR,NDI\params\IOBaseAddress,resc,1,02,00,00,00
HKR,NDI\params\IOBaseAddress,ParamDesc,,"I/O Base Address"
HKR,NDI\params\IOBaseAddress,flag,1,20,00,00,00

;
;----------------------------------------------------------------------------
; Destination Directories
;
[DestinationDirs]
DefaultDestDir        = 11 ; LDID_SYS
le10X.ndis3.CopyFiles = 11
le10.ndis5.CopyFiles  = 12


[Strings]
Service.DispName =   "PCMCIA Ethernet Card NT Driver"

PC_CARD   =   "PC Card Series Products"
PC_CARD.DeviceDesc  =   "PCMCIA Ethernet Card"
