[Version]
Signature  = "$CHICAGO$"
Compatible = 1
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %SUPCOM%

DriverVer   = 06/26/2013, 1.1.1.0

[Manufacturer]
%SUPCOM%   = TL9200

[ControlFlags]
ExcludeFromSelect = USB\VID_E202&PID_9200

[TL9200]
%TL9200.DeviceDesc% = TL9200.Ndi,USB\VID_E202&PID_9200


;*******************************************************************************

[TL9200.Ndi]
AddReg   = TL9200.Reg, TL9200.Params
;DeviceID = USB\VID_0FE6&PID_9700
CopyFiles = TL9200.ndis.copyfiles

;*******************************************************************************
; NT main sections

[TL9200.Ndi.NT]
AddReg          = TL9200.NT.Reg, TL9200.Params
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15 ; ISA for pass InfCheck.exe
;The BusType for usb devices is 15 ?????
CopyFiles       = TL9200.ndis.copyfiles.NT


[TL9200.Ndi.NT.Services]
AddService = TL9200, 2, TL9200.Service, Common.EventLog


[TL9200.ndis.copyfiles]
TL9200.sys,,,2

[TL9200.ndis.copyfiles.NT]
TL9200.sys,,,2




[TL9200.Reg]
HKR,Ndi,DeviceID,,USB\VID_E202&PID_9200
HKR,,AdapterName,,TL9200
HKR,Ndi,CardType,,"PNP"

HKR,,DevLoader,,*ndis,*ntkern,*ndis
HKR,,DeviceVxDs,,TL9200.sys

; NDIS Info
HKR,NDIS,MajorNdisVersion,1,05
HKR,NDIS,MinorNdisVersion,1,00
HKR,NDIS,LogDriverName,,TL9200

; Interfaces
HKR,Ndi\Interfaces,DefUpper,,"ndis3"
HKR,Ndi\Interfaces,DefLower,,"ethernet"
HKR,Ndi\Interfaces,UpperRange,,"ndis3"
HKR,Ndi\Interfaces,LowerRange,,"ethernet"

; Install sections
HKR,Ndi\Install,,,"TL9200.Install"

HKR,Ndi,HelpText,,"TL9200 USB2.0 To Fast Ethernet Adapter"


;*******************************************************************************
; Driver parameters
;*******************************************************************************

[TL9200.Params]
HKR, ,TxPacketDesc,    0, "46"   ; 0x2E
HKR, ,RxPacketDesc,    0, "1"   ; 0x01
;HKR, ,NetworkAddress,    0, "00123456789A"   


HKR,Ndi\Params\ConnectionType,ParamDesc,,"ConnectionType"
HKR,Ndi\Params\ConnectionType,default,,"15"
HKR,Ndi\Params\ConnectionType,type,,"enum"
HKR,Ndi\Params\ConnectionType\enum,15,,"AutoSense"
HKR,Ndi\Params\ConnectionType\enum,4,,"10BaseT"
HKR,Ndi\Params\ConnectionType\enum,5,,"10BaseT Full_Duplex"
HKR,Ndi\Params\ConnectionType\enum,8,,"100BaseTX"
HKR,Ndi\Params\ConnectionType\enum,9,,"100BaseTX Full_Duplex"
HKR,Ndi\Params\ConnectionType,flag,1,"20","00","00","00"


;for network address
HKR,Ndi\Params\NetworkAddress,ParamDesc,,"Network address"
HKR,Ndi\Params\NetworkAddress,type,,"edit"
HKR,Ndi\Params\NetworkAddress,default,,""
HKR,Ndi\Params\NetworkAddress,Optional,,"1"
HKR,Ndi\Params\NetworkAddress,LimitText,,"12"
;*******************************************************************************
; Install section for Windows 2000
;*******************************************************************************

[TL9200.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "TL9200"
HKR,,                Platform,   0, "1"


[TL9200.Service]
DisplayName    = %TL9200.Service.DispName%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\TL9200.sys
LoadOrderGroup = NDIS,NTKERN,NDIS
AddReg         = TextModeFlags.Reg


[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000, %%SystemRoot%%\System32\netevent.dll
HKR, , TypesSupported  , 0x00010001, 7

[TextModeFlags.Reg]
HKR, , TextModeFlags, 0x00010001, 0x0001


;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
TL9200.ndis.copyfiles    = 11
TL9200.ndis.copyfiles.NT = 12
DefaultDestDir           = 11


[SourceDisksNames]
; Cabinet file names and associated disks
; <cab#> = <disk#>,<cabinet filename>, ID (Unused, must be 0)
1=%DISKNAME%,,,

[SourceDisksFiles]
;<file> = <cabinet number>,<subdir>,<filename>,<size>
;Note: File is not in a cabinet if cab# is 0
TL9200.sys = 1
;TL9200.inf = 1



;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
SUPCOM = "Corechip Semiconductor, Inc."

;Source Disk Name
DISKNAME = "Tlink TL9200 USB2.0 To Fast Ethernet Adapter Driver Disk"

TL9200.DeviceDesc       = "Tlink TL9200 USB2.0 To Fast Ethernet Adapter"
TL9200.Service.DispName = "Tlink TL9200 USB2.0 To Fast Ethernet Adapter"

