;
; USB DVB-T Adapter
; 7048
;
[Version]
Signature="$CHICAGO$"
Class = Media
ClassGuid = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Drv_Provider%

CatalogFile=BDA_Capture_225.cat

DriverVer=09/27/2006,3.0.1.6	

[SourceDisksNames]
1=%DiskName1%,,0

[SourceDisksFiles]
BDA_Capture_225.sys = 1

[Manufacturer]
%Mnfct%=VID

[VID]
; The Vendor ID =14AA, and the Product ID =0226
%DevModel.DeviceDesc%=DevModel.Dev,USB\VID_13D3&PID_3217&MI_00

[DestinationDirs]
DevModel.Files.Ext = 10,System32\Drivers

[DevModel.Dev.NT]
Include=ks.inf,kscaptur.inf, bda.inf
Needs=Stream.Registration,KS.Registration,KSCAPTUR.Registration.NT,BDA.Registration.NT,BDA.Installation.NT
CopyFiles=DevModel.Files.Ext
AddReg=DevModel.AddReg

[DevModel.Dev.NT.Services]
Addservice = %SVCKEY%, 0x00000002, DevModel.AddService

[DevModel.Dev.NT.Interfaces]
AddInterface=%KSCATEGORY_BDATUNER%,%KSNAME_BDATUNER_FILTER%,TunerDemod,
AddInterface=%KSCATEGORY_BDARECEIVER%,%KSNAME_BDARECIVE_FILTER%,CaptureDev,

[TunerDemod]
AddReg=TunerDemod.AddReg
[CaptureDev]
AddReg=CaptureDev.AddReg

[TunerDemod.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,FriendlyName,,%DevModel.NAME%
HKR,,DeviceName,,%DevModel.DeviceDesc%
HKLM,SOFTWARE\Wideviewer\Tuner,delay,0x00010001,%DELAYINTERVAL%

[CaptureDev.AddReg]
HKR,,CLSID,,%ProxyVCap.CLSID%
HKR,,FriendlyName,,%DevModel.CapNAME%
HKR,,DeviceName,,%DevModel.DeviceDesc%

[DevModel.AddService]
DisplayName    = %DevModel.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %10%\System32\Drivers\BDA_Capture_225.sys
LoadOrderGroup = Base

[DevModel.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,BDA_Capture_225.sys

[DevModel.Files.Ext]
BDA_Capture_225.sys

;---------------------------------------------------------------;

[Strings]
ProxyVCap.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"

KSCATEGORY_BDATUNER="{71985F48-1CA1-11d3-9CC8-00C04F7971E0}"
KSNAME_BDATUNER_FILTER="{9878BB92-0AD3-4d5c-8D73-D703FB30FB46}"

KSCATEGORY_BDARECEIVER="{FD0A5AF4-B41D-11d2-9C95-00C04F7971E0}"
KSNAME_BDARECIVE_FILTER="{4EFDBE46-E7F5-4bf5-B935-EAE8E0C96540}"

SVCKEY="BDA_Capture_225"
;SYSFILE="BDA_Capture_225.sys"
;INFFILE="BDA_Capture_225.inf"
;CATALOGFILE="BDA_Capture_225.cat"

DELAYINTERVAL=1000

Mnfct="DTV"
Drv_Provider ="DTV"
DevModel.DeviceDesc="USB Digital-TV Receiver."
DevModel.NAME="USB Digital-TV Receiver."
DevModel.CapNAME="USB Digital-TV Device Capture."
DevModel.SvcDesc="USB Digital-TV receiver. Driver 3.0.1.6"
DiskName1="USB Digital-TV receiver. Installation Disk"






