////////////////////////////////////////////////////////////////////////////////
;//
;//                           (C) Pinnacle Systems GmbH 2006
;//      All rights are reserved.  Reproduction in whole or in part is prohibited
;//      without the written consent of the copyright owner.
;//
;//      Pinnacle Systems, Inc. reserves the right to make changes without notice at any time.
;//      Pinnacle Systems, Inc. makes no warranty, expressed, implied or statutory, including
;//      but not limited to any implied warranty of merchantibility of fitness
;//      for any particular purpose, or that the use will not infringe any
;//      third party patent, copyright or trademark.
;//      Pinnacle Systems, Inc. must not be liable for any loss or damage arising from its use.
;//
;////////////////////////////////////////////////////////////////////////////////

;----------------------------------------------------------------------------------------------------
;
; PCTV310cAV.inf  -- This file contains installation information for
;                  "Pinnacle Systems PCTV 310c"
;
; Copyright (c) 2006 Pinnacle Systems
;----------------------------------------------------------------------------------------------------


[Version]
signature=$Windows NT$
Class=Media
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
Provider=%Company%
DriverVer=03/21/2007,3.1.1.24
CatalogFile.ntx86=PCTV310cAVSim.cat
CatalogFile.ntia64=PCTV310cAVSimia64.cat
CatalogFile.ntamd64=PCTV310cAVSimamd64.cat
DriverPackageType=PlugAndPlay
DriverPackageDisplayName="Pinnacle Systems PCTV 310c" 

[Manufacturer]
%Company%=Pinnacle,,NTamd64,NTia64

[SourceDisksNames]
1=%DISK_NAME%,,,""

[SourceDisksFiles]
AVSim.sys=1,\x86

[SourceDisksFiles.ia64]
AVSim.sys=1,\ia64

[SourceDisksFiles.amd64]
AVSim.sys=1,\amd64

[ControlFlags]
ExcludeFromSelect =* 


[Pinnacle.NTia64]
;---------------------------------------
; CB788 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=PCTV310c.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881% =PCTV310c.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=PCTV310c.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB


[Pinnacle.NTamd64]
;---------------------------------------
; CB788 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=PCTV310c.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881%=PCTV310c.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=PCTV310c.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB


[Pinnacle]
;---------------------------------------
; CB788 Hybrid DVB-T/Global TV Tuner Cardbus , Analog TV/DVB-T using Zarlink mt352 demod with XCevie XC3028 tuner
;---------------------------------------
%AVSim.Audio%	=PCTV310c.Install,					PCI\VEN_14F1&DEV_8801&SUBSYS_178812AB
%AVSim.Audio881%=PCTV310c.Install,					PCI\VEN_14F1&DEV_8811&SUBSYS_178812AB
%AVSim.TS%		=PCTV310c.Install,					PCI\VEN_14F1&DEV_8802&SUBSYS_178812AB


;;---------------------
;; Installation Section
;;---------------------
[PCTV310c.Install.NT]
CopyFiles=  PCTV310c.CopyDrivers

[DestinationDirs]
PCTV310c.CopyDrivers=12

[PCTV310c.CopyDrivers]
AVSim.sys



;
; Services installation
;

[PCTV310c.Install.NT.Services]
AddService = AVSim,2,VID.ServiceInstall

[VID.ServiceInstall]
DisplayName		= %SERVICE_DISPLAY_NAME%
Description		= %SERVICE_DESCRIPTION%
ServiceType		= %SERVICE_KERNEL_DRIVER%
StartType		= %SERVICE_DEMAND_START%
ErrorControl	= %SERVICE_ERROR_NORMAL%
ServiceBinary	= %12%\AVSim.sys

;---------------------------------------------------------------
;                S t r i n g s
;---------------------------------------------------------------
[Strings]
;---------------------------------------------------------------
;				S y s t e m   D e f i n e s
;---------------------------------------------------------------
SERVICE_BOOT_START				= 0x0
SERVICE_SYSTEM_START			= 0x1
SERVICE_AUTO_START				= 0x2
SERVICE_DEMAND_START			= 0x3
SERVICE_DISABLED				= 0x4

SERVICE_KERNEL_DRIVER			= 0x1

SERVICE_ERROR_IGNORE			= 0x0
SERVICE_ERROR_NORMAL			= 0x1
SERVICE_ERROR_SEVERE			= 0x2
SERVICE_ERROR_CRITICAL			= 0x3

SERVICE_DISPLAY_NAME			= "Cx2388x Multifunction Helper driver"
SERVICE_DESCRIPTION				= "Cx2388x Multifunction Helper driver"

;---------------------------------------------------------------
;             *L o c a l i z a b l e*
;---------------------------------------------------------------
;.....................
;  Installation 
;.....................
Company							= "Pinnacle Systems"
DISK_NAME						= "PCTV 310c Driver Setup Disk"

;.....................
;  Devices
;.....................
AVSim.Audio						= "Pinnacle PCTV 310c Audio AVStream Device"
AVSim.Audio881					= "Pinnacle PCTV 310c Audio Capture Device"
AVSim.TS						= "Pinnacle PCTV 310c TS Capture Device"



