
[Version]
signature           = "$CHICAGO$"
Class               = MEDIA
ClassGUID           = {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider            = %PROVIDER%
CatalogFile.NTx86   = 3xHybrid.cat
CatalogFile.NTAMD64 = 3xHybr64.cat
DriverVer 	    = 10/13/2010, 1.3.4.5020

[Manufacturer]
%PROVIDER%  = SupportedBoards, NTx86, NTAMD64

;---> 32 BIT SUPPORT <---
[SupportedBoards.NTx86]
;%PHILIPS_33.DeviceDesc% = PHILIPS_33.NTx86,PCI\VEN_1131&DEV_7133
%PHILIPS_33.DeviceDesc% = PHILIPS_33.NTx86,PCI\VEN_1131&DEV_7133&SUBSYS_6F37107D


;---> 64 BIT SUPPORT <---
[SupportedBoards.NTAMD64]
;%PHILIPS_33.DeviceDesc% = PHILIPS_33.NTAMD64,PCI\VEN_1131&DEV_7133
%PHILIPS_33.DeviceDesc% = PHILIPS_33.NTAMD64,PCI\VEN_1131&DEV_7133&SUBSYS_6F37107D

[SourceDisksNames]
1 = %INSTALLATION_DISK%,,


[SourceDisksFiles]
3xHybrid.sys           = 1
3xHybr64.sys           = 1
NXPMV32.dll            = 1
NXPMV64.dll            = 1
;34CoInstaller.dll      = 1


[DestinationDirs]
SectionX32.CopyDll.NTx86      = 11
SectionX64.CopyDll.NTAMD64    = 11
SectionX32.CopyDriver.NTx86   = 10,system32\drivers
SectionX64.CopyDriver.NTAMD64 = 10,system32\drivers


[SectionX32.CopyDll.NTx86]
NXPMV32.dll
;34CoInstaller.dll

[SectionX64.CopyDll.NTAMD64]
NXPMV64.dll

[SectionX32.CopyDriver.NTx86]
3xHybrid.sys


[SectionX64.CopyDriver.NTAMD64]
3xHybr64.sys



;======================================
;
;       Initialization Entries
;
;======================================

;******** SAA7130 x32 ***
[PHILIPS_30.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[PHILIPS_30.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, PHILIPS_30.AddReg

[PHILIPS_30.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86


;******** SAA7130 x64 ***
[PHILIPS_30.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[PHILIPS_30.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, PHILIPS_30.AddReg

[PHILIPS_30.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64


;******** SAA7133 x32 ***
[PHILIPS_33.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[PHILIPS_33.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, PHILIPS_33.AddReg

[PHILIPS_33.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86


;******** SAA7133 x64 ***
[PHILIPS_33.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[PHILIPS_33.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, PHILIPS_33.AddReg

[PHILIPS_33.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64


;******** SAA7134 x32 ***
[PHILIPS_34.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[PHILIPS_34.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, PHILIPS_34.AddReg

[PHILIPS_34.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86


;******** SAA7134 x64 ***
[PHILIPS_34.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[PHILIPS_34.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, PHILIPS_34.AddReg

[PHILIPS_34.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64


;******** PHILIPS PROTEUS x32 ***
[PHILIPS_PROTEUS.NTx86.CoInstallers]
CopyFiles     = SectionX32.CopyDll.NTx86
AddReg        = SectionX32.DllAddReg.NTx86

[PHILIPS_PROTEUS.NTx86]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX32.CopyDriver.NTx86, SectionX32.CopyDll.NTx86
AddReg        = SectionX32.AddReg.NTx86, PHILIPS_PROTEUS.AddReg

[PHILIPS_PROTEUS.NTx86.Services]
AddService    = %SERVICE_NAME_X32%, 0x00000002, SectionX32.ServiceInstall.NTx86


;******** PHILIPS PROTEUS x64 ***
[PHILIPS_PROTEUS.NTAMD64.CoInstallers]
CopyFiles     = SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.DllAddReg.NTAMD64

[PHILIPS_PROTEUS.NTAMD64]
Include       = ks.inf, wdmaudio.inf, kscaptur.inf, bda.inf
Needs         = KS.Registration, WDMAUDIO.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
CopyFiles     = SectionX64.CopyDriver.NTAMD64, SectionX64.CopyDll.NTAMD64
AddReg        = SectionX64.AddReg.NTAMD64, PHILIPS_PROTEUS.AddReg

[PHILIPS_PROTEUS.NTAMD64.Services]
AddService    = %SERVICE_NAME_X64%, 0x00000002, SectionX64.ServiceInstall.NTAMD64


;******** GENERAL x32 ***
[SectionX32.ServiceInstall.NTx86]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\3xHybrid.sys
;
HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x0
;
HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x0
;
;HKR, "Parameters","TUNING_SPEED_LEVEL",0x00010001,0x5
;
HKR, "Parameters","C1_BLANKING_TIME",0x00010001, 50
HKR, "Parameters","BLANKING_TIME",0x00010001, 50
;
HKR, "Parameters","EnableAutoOffset",0x00010001,1
HKR, "Parameters","AutoOffsetLevel",0x00010001,0x2
;******** GENERAL x64 ***
[SectionX64.ServiceInstall.NTAMD64]
DisplayName   = %DISPLAY_NAME%
Description   = %SERVICE_DESCRIPTION%
ServiceType   = %SERVICE_KERNEL_DRIVER%
StartType     = %SERVICE_DEMAND_START%
ErrorControl  = %SERVICE_ERROR_IGNORE%
ServiceBinary = %12%\3xHybr64.sys
;
HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x0
;
HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x0
;
;HKR, "Parameters","TUNING_SPEED_LEVEL",0x00010001,0x5
;
HKR, "Parameters","C1_BLANKING_TIME",0x00010001, 50
HKR, "Parameters","BLANKING_TIME",0x00010001, 50
;
HKR, "Parameters","EnableAutoOffset",0x00010001,1
HKR, "Parameters","AutoOffsetLevel",0x00010001,0x2

;======================================
;
;           Registry Entries
;
;======================================
; [StartName=driver-object-name]
; [AddReg=add-registry-section[, add-registry-section] ...]
; [DelReg=del-registry-section[, del-registry-section] ...]
; [BitReg=bit-registry-section[,bit-registry-section] ...]
; [LoadOrderGroup=load-order-group-name]
; [Dependencies=depend-on-item-name[,depend-on-item-name]...]

;
;******** General DLL Registry Entries ***
;

[SectionX32.DllAddReg.NTx86]
HKR,,CoInstallers32,0x00010000,"34CoInstaller.dll, CoInstallerEntry"


[SectionX64.DllAddReg.NTAMD64]

[SectionX32.Register.NTx86]
11,,NXPMV32.dll,1 ;//FLG_REGSVR_DLLREGISTER

[SectionX64.Register.NTAMD64]
11,,NXPMV64.dll,1 ;//FLG_REGSVR_DLLREGISTER

;******** General Driver Registry Entries ***
;

[SectionX32.AddReg.NTx86]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,3xHybrid.sys

; --- Registry Entries For Audio Capture ---
;HKR,,Driver,,3xHybrid.sys
;HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
;HKR,Drivers,SubClasses,,"wave,mixer"
;HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
;HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
;HKR,Drivers\wave\wdmaud.drv,Description,,%PHILIPS.AudioDeviceDesc%
;HKR,Drivers\mixer\wdmaud.drv,Description,,%PHILIPS.AudioDeviceDesc%

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

HKR, "Audio","I2S Output",0x00010001,0x00
HKR, "Parameters","TDA18271C1_Freeze_AGC",0x00010001,0x00
HKR, "Parameters","TDA18271_Freeze_AGC",0x00010001,0x00
;
HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x0
;
HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x0
;
;HKR, "Parameters","TUNING_SPEED_LEVEL",0x00010001,0x0
;
HKR, "Parameters","C1_BLANKING_TIME",0x00010001, 50
HKR, "Parameters","BLANKING_TIME",0x00010001, 50
;
HKR, "Parameters","EnableAutoOffset",0x00010001,1
HKR, "Parameters","AutoOffsetLevel",0x00010001,0x2
[SectionX32.DelReg.NTAMD64]
; *** Sample of how to clean up the registry before writing new keys
;     when the driver is being updated ***
;;;HKLM,SYSTEM\CurrentControlSet\Services\%SERVICE_NAME_X32%  ;// Sample line!!! NEVER use it!!!
HKR, "Parameters"      ; Full registry key with all subkeys/data will be deleted
HKR, "I2C Devices"     ; Full registry key with all subkeys/data will be deleted
HKR, "VideoDecoder"    ; Full registry key with all subkeys/data will be deleted
HKR, "AudioDecoder"    ; Full registry key with all subkeys/data will be deleted


[SectionX64.AddReg.NTAMD64]

HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,3xHybr64.sys

; --- Registry Entries For Audio Capture ---
;HKR,,Driver,,3xHybr64.sys
;HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
;HKR,Drivers,SubClasses,,"wave,mixer"
;HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
;HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv
;HKR,Drivers\wave\wdmaud.drv,Description,,"Philips Audio Capture Device"
;HKR,Drivers\mixer\wdmaud.drv,Description,,"Philips Audio Capture Device"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audioinput"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_ITU_PIN%,"Name",,"Analog ITU Video"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_I2S_PIN%,"Name",,"I2S Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_AUDIO_CAP_PIN%,"Name",,"~Audio"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_CAP_PIN%,"Name",,"~Capture"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_ANLG_VIDEO_PRE_PIN%,"Name",,"~Preview"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_AES_PIN%,"Name",,"MPEG Audio ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_VES_PIN%,"Name",,"MPEG Video ES"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%AVSTREAM_MPEG_PS_PIN%,"Name",, "MPEG2 Program"

HKR, "Audio","I2S Output",0x00010001,0x00
HKR, "Parameters","TDA18271C1_Freeze_AGC",0x00010001,0x00
HKR, "Parameters","TDA18271_Freeze_AGC",0x00010001,0x00
;
HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271_BlankVideo",0x00010001,0x0
;
HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x01
;HKR, "Parameters","TDA18271C1_BlankVideo",0x00010001,0x0
;
;HKR, "Parameters","TUNING_SPEED_LEVEL",0x00010001,0x0
;
HKR, "Parameters","C1_BLANKING_TIME",0x00010001, 50
HKR, "Parameters","BLANKING_TIME",0x00010001, 50
;
HKR, "Parameters","EnableAutoOffset",0x00010001,1
HKR, "Parameters","AutoOffsetLevel",0x00010001,0x2
;
;******** Board - Specific Registry Entries ***
;

;---- SAA7130 ----
[PHILIPS_30.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%
; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters","SmallXBar",0x00010001,0x01

HKR, "Audio","I2S Output",0x00010001,0x00
HKR, "Parameters","TDA18271C1_Freeze_AGC",0x00010001,0x00
HKR, "Parameters","TDA18271_Freeze_AGC",0x00010001,0x00

;---- SAA7133 ----
[PHILIPS_33.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%
; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters","SmallXBar",0x00010001,0x01

HKR, "Audio","I2S Output",0x00010001,0x00
HKR, "Parameters","TDA18271C1_Freeze_AGC",0x00010001,0x00
HKR, "Parameters","TDA18271_Freeze_AGC",0x00010001,0x00

;---- SAA7134 ----
[PHILIPS_34.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%
; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters","SmallXBar",0x00010001,0x01

HKR, "Audio","I2S Output",0x00010001,0x00
HKR, "Parameters","TDA18271C1_Freeze_AGC",0x00010001,0x00
HKR, "Parameters","TDA18271_Freeze_AGC",0x00010001,0x00

;---- Proteus ----
[PHILIPS_PROTEUS.AddReg]
; Prefix will be displayed in front of the device name on every filter
HKR, "Parameters","Prefix",,%PHILIPS_CUSTOM_TUNERNAME%

; SmallXBar=0: XBar inputs => Tuner, Composite1, S-Video1, Composite2, S-Video2
; SmallXBar=1: XBar inputs => Tuner, Composite1, S-Video1
HKR, "Parameters", "SmallXBar",0x00010001,1

HKR, "I2C Devices", "Force Registry Settings",0x00010001,0x01
HKR, "VideoDecoder", "Tuner Channel",0x00010001,0x01
HKR, "VideoDecoder", "CVBS Channel",0x00010001,0x00
HKR, "VideoDecoder", "SVHS Channel",0x00010001,0x06
;HKR, "VideoDecoder", "FM Radio Channel",0x00010001,0x00

HKR, "AudioDecoder", "Tuner Channel",0x00010001,0x01
HKR, "AudioDecoder", "CVBS Channel",0x00010001,0x02
HKR, "AudioDecoder", "SVHS Channel",0x00010001,0x02
;HKR, "AudioDecoder", "FM Radio Channel",0x00010001,0x02
;HKR, "AudioDecoder", "XTAL",0x00010001,0x0                ;Default = 32MHz

HKR, "I2C Devices", "Number of I2C Devices",0x00010001,0x01
HKR, "I2C Devices", "Device 0, Data1",0x00010001,0x03  ; Tuner ID
HKR, "I2C Devices", "Device 0, Data2",0x00010001,0xC0  ; Tuner slave addr.
HKR, "I2C Devices", "Device 0, Data3",0x00010001,0x86  ; Tuner IF PLL slave addr.
;HKR, "I2C Devices", "Device 0, Data4",0x00010001,0x0   ; Demod slave addr.
;HKR, "I2C Devices", "Device 0, Data5",0x00010001,0x0   ; Size of add. data
;HKR, "I2C Devices", "Device 0, Data6",0x00010001,0x0   ; Add. data #1
;HKR, "I2C Devices", "Device 0, Data7",0x00010001,0x0   ; Add. data #2
;HKR, "I2C Devices", "Device 0, Data8",0x00010001,0x0   ; Add. data #3


;======================================
;
;           Strings Defines
;
;======================================

[Strings]
;-------------------------------
; Capture Filter Pin Name GUIDs
;-------------------------------
AVSTREAM_ANLG_AUDIO_IN_PIN   = "{7BB284B9-714D-493d-A101-B1B028E782BD}"
AVSTREAM_ANLG_AUDIO_OUT_PIN  = "{5582E657-E596-42b5-9DB3-541B27A2355F}"
AVSTREAM_ANLG_VIDEO_ITU_PIN  = "{82631A2E-403C-4581-A4B0-EC173D004410}"
AVSTREAM_ANLG_AUDIO_I2S_PIN  = "{C2E46358-F032-4d88-B802-06B59D162730}"
AVSTREAM_ANLG_VIDEO_CAP_PIN  = "{16FFBD0A-F770-4692-A2FF-DD394DFE9564}"
AVSTREAM_ANLG_VIDEO_PRE_PIN  = "{A19F6121-9CF7-4081-8053-256668FCBE1F}"
AVSTREAM_ANLG_AUDIO_CAP_PIN  = "{BA9E27B1-CF44-490e-8EAB-5F662E5FFE74}"
AVSTREAM_MPEG_AES_PIN        = "{9DEC84B9-BCEF-4aac-997E-43EDD0A2D6C7}"
AVSTREAM_MPEG_VES_PIN        = "{181CF87E-7741-47ba-8629-22347E03C64C}"
AVSTREAM_MPEG_PS_PIN         = "{DDA87B83-65DB-4aec-82D0-79FBE67D2BB6}"


;--------------------
; System Defines
;--------------------
SERVICE_BOOT_START       = 0x0
SERVICE_SYSTEM_START     = 0x1
SERVICE_AUTO_START       = 0x2
SERVICE_DEMAND_START     = 0x3
SERVICE_DISABLED         = 0x4

SERVICE_KERNEL_DRIVER    = 0x1
SERVICE_ERROR_IGNORE     = 0x0
SERVICE_ERROR_NORMAL     = 0x1
SERVICE_ERROR_SEVERE     = 0x2
SERVICE_ERROR_CRITICAL   = 0x3
FLG_REGSVR_DLLREGISTER   = 0x00000001


;***********************************************************
;                      !!! ATTENTION !!!
; Customer Strings:
;   The following strings MUST be changed, if the driver has
;   been customized, to not interfere with the original one.
;
;************************************************************

;--- Driver names for 32/64 bit OS ---
DRIVER_NAME_X32               = "3xHybrid.sys"
DRIVER_NAME_X64               = "3xHybr64.sys"

;--- Catalog file (signature) names for 32/64 bit OS ---
SIGNATURE_NAME_X32            = "3xHybrid.cat"
SIGNATURE_NAME_X64            = "3xHybr64.cat"

;--- Coinstaller DLL name for 32/64 bit OS ---
COINSTALLER_NAME_X32          = "34CoInstaller.dll"
COINSTALLER_NAME_X64          = "3xCoInstX64.dll"

;--- Service names linked to the driver binary ---
SERVICE_NAME_X32              = "3xHybrid"
SERVICE_NAME_X64              = "3xHybr64"
SERVICE_DESCRIPTION           = "WinFast DTV1800 H Plus BDA Capture Driver"

;--- Name displayed in the device manager ---
DISPLAY_NAME                  = "WinFast DTV1800 H Plus"

;--- General names ---
PROVIDER                      = "Leadtek"
INSTALLATION_DISK             = "WinFast DTV1800 H Plus Driver Installation Disk"


;***********************************************************
;
; Generic Strings:
;   Board Description (-> Displayed within e.g. Graphedit)
;
;***********************************************************

;*** Specific Names ***
;-----------------
;PHILIPS.AudioDeviceDesc       = "WinFast DTV1800 H Plus Audio Capture Device"
PHILIPS_CUSTOM_TUNERNAME      = "WinFast DTV1800 H Plus"
PHILIPS_33.DeviceDesc         = "WinFast DTV1800 H Plus"

