;*******************************************************************************
; Installation inf file for MOD7700 driver - 
; supported OS Windows XP (32), Windows Vista (32&64)
;*******************************************************************************
;mod 06272008: add CTX1918 by mr
;mod 09292008: change driver version by mr
;mod 10242008: add CTX1921 + rc by mr
;mod 11142008: change device names 
;mod 04202009: add CTX1923 by mr
;mod 04222009: change DriverVer date for WHQL reason
;mod 06032009: change driver version by mr
;mod 08312009: change driver version by mr
;mod 09242009: add CTX1926 by mr

[Version]
signature			= "$CHICAGO$"
Class				= Media
ClassGUID			= {4d36e96c-e325-11ce-bfc1-08002be10318}
Provider			= %ctx%
DriverVer			= 09/24/2009,3.15.0.0
CatalogFile.NTx86		= mod7700.cat
CatalogFile.NTamd64	= mod77-64.cat


[Manufacturer]
%MfgName% = ctx,NTx86,NTamd64


[ctx.NTx86]
%MOD7000_a.DeviceDesc% 	= MOD7000_a.NTx86,USB\VID_1660&PID_0959			; STK7700PH,CX25843,XC3028,usb Stick
%MOD7000_b.DeviceDesc% 	= MOD7000_a.NTx86,USB\VID_1660&PID_0960			; STK7700PH, CX25843, XC3028,express card
%MOD7000_d.DeviceDesc% 	= MOD7000_a.NTx86,USB\VID_1660&PID_0962			; STK7700PH,CX25843,XC3028,usb rund

%MOD7000_e.DeviceDesc% 	= MOD7000_e.NTx86,USB\VID_1660&PID_0972			; STK7070PD,antenna diversity, usb
%MOD7000_i.DeviceDesc% 	= MOD7000_e.NTx86,USB\VID_1660&PID_0970			; STK7070PD,antenna diversity, usb

%MOD7000_f.DeviceDesc% 	= MOD7000_f.NTx86,PCI\VEN_1932&DEV_1E3C&SUBSYS100116BE	; PCI7710D,antenna diversity, mini card

%MOD7000_g.DeviceDesc% 	= MOD7000_g.NTx86,USB\VID_1660&PID_0976			; STK7070PD,usb

%MOD7000_h.DeviceDesc% 	= MOD7000_h.NTx86,USB\VID_1660&PID_0981			; STK7700P1,MT2060, mini card

%MOD7000_k.DeviceDesc% 	= MOD7000_g.NTx86,USB\VID_1660&PID_0987			; STK7070PD,mini card

%MOD7000_c.DeviceDesc% 	= MOD7000_i.NTx86,USB\VID_1660&PID_0961			; STK7700PH,CX25843,XC3028L,mini card

%MOD7000_m.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_0997			;STK7770P, usb-stick
%MOD7000_n.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_0999			;STK7770P, minicard
%MOD7000_o.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_0995			;STK7770P, Express Card 54
%MOD7000_p.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_0996			;STK7770P, Express Card 34
%MOD7000_q.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_1918			;STK7770P, usb rund
%MOD7000_r.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_1921			;STK7770P, usb-stick mini
%MOD7000_s.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_1923			;STK7770P, express card 54
%MOD7000_t.DeviceDesc%	=MOD7000_m.NTx86,USB\VID_1660&PID_1926			;STK7770P, express card 34

[ctx.NTamd64]
%MOD7000_a.DeviceDesc% 	= MOD7000_a.NTamd64,USB\VID_1660&PID_0959			; STK7700PH,CX25843,XC3028,usb Stick
%MOD7000_b.DeviceDesc% 	= MOD7000_a.NTamd64,USB\VID_1660&PID_0960			; STK7700PH, CX25843, XC3028,express card
%MOD7000_c.DeviceDesc% 	= MOD7000_i.NTamd64,USB\VID_1660&PID_0961			; STK7700PH,CX25843,XC3028L,mini card
%MOD7000_d.DeviceDesc% 	= MOD7000_a.NTamd64,USB\VID_1660&PID_0962			; STK7700PH,CX25843,XC3028,usb rund

%MOD7000_e.DeviceDesc% 	= MOD7000_e.NTamd64,USB\VID_1660&PID_0972			; STK7070PD,antenna diversity, usb
%MOD7000_i.DeviceDesc% 	= MOD7000_e.NTamd64,USB\VID_1660&PID_0970			; STK7070PD,antenna diversity, usb

%MOD7000_f.DeviceDesc% 	= MOD7000_f.NTamd64,PCI\VEN_1932&DEV_1E3C&SUBSYS100116BE	; PCI7710D,antenna diversity, mini card

%MOD7000_g.DeviceDesc% 	= MOD7000_g.NTamd64,USB\VID_1660&PID_0976			; STK7070PD,usb

%MOD7000_h.DeviceDesc% 	= MOD7000_h.NTamd64,USB\VID_1660&PID_0981			; STK7700P1,MT2060, mini card

%MOD7000_k.DeviceDesc% 	= MOD7000_g.NTamd64,USB\VID_1660&PID_0987			; STK7070PD,mini card
%MOD7000_m.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_0997			;STK7770P, usb-stick
%MOD7000_n.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_0999			;STK7770P, minicard
%MOD7000_o.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_0995			;STK7770P, Express Card 54
%MOD7000_p.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_0996			;STK7770P, Express Card 34
%MOD7000_q.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_1918			;STK7770P, usb rund
%MOD7000_r.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_1921			;STK7770P, usb-stick mini
%MOD7000_s.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_1923			;STK7770P, express card 54
%MOD7000_t.DeviceDesc%	=MOD7000_m.NTamd64,USB\VID_1660&PID_1926			;STK7770P, express card 34


[DestinationDirs]
SECTION32.CopyDrivers.NTx86	= 12,
SECTION64.CopyDrivers.NTamd64	= 12,


[SourceDisksNames]
1 = %INSTALLATION_DISK%,,


[SourceDisksFiles]
mod7700.sys	= 1
mod77-64.sys	= 1


[ControlFlags]
ExcludeFromSelect    = *
ExcludeFromSelect.NT = *

[SECTION32.CopyDrivers.NTx86]
mod7700.sys

[SECTION64.CopyDrivers.NTamd64]
mod77-64.sys

;*******************************************************************************
;Entries for 32 bit
;*******************************************************************************

[MOD7000_a.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_e.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_f.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_g.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_h.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_i.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_m.NTx86]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86
;--------------------------------------------------------------------------------------------------------------------------------------
[MOD7000_a.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_e.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_f.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_g.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_h.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_i.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86

[MOD7000_m.NTx86.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg
CopyFiles  = SECTION32.CopyDrivers.NTx86
;--------------------------------------------------------------------------------------------------------------------------
[MOD7000_a.NTx86.NT.HW]
AddReg = MOD7000_a_DEVICE_AddReg

[MOD7000_e.NTx86.NT.HW]
AddReg = MOD7000_e_DEVICE_AddReg

[MOD7000_f.NTx86.NT.HW]
AddReg = MOD7000_f_DEVICE_AddReg

[MOD7000_g.NTx86.NT.HW]
AddReg = MOD7000_g_DEVICE_AddReg

[MOD7000_h.NTx86.NT.HW]
AddReg = MOD7000_h_DEVICE_AddReg

[MOD7000_i.NTx86.NT.HW]
AddReg = MOD7000_i_DEVICE_AddReg

[MOD7000_m.NTx86.NT.HW]
AddReg = MOD7000_m_DEVICE_AddReg
;-------------------------------------------------------------------------------

[MOD7000_a.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_e.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_f.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_g.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_h.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_i.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService

[MOD7000_m.NTx86.NT.Services]
Addservice = mod7700, 0x00000002, MOD7000.AddService
;-------------------------------------------------------------------------------

[MOD7000.AddService]
DisplayName    = %MOD7000.FriendlyName%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\mod7700.sys
LoadOrderGroup = Base
AddReg         = MOD7000.Service.AddReg

[MOD7000.Service.AddReg]
HKR,,DigitalJmp,0x00010001,0x00
HKR,"parameters","ReducedScanning",0x0000001,0x00

[MOD7000.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,mod7700.sys
HKR,,PageOutWhenUnopened,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audio input"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"

;***************************end 32 bit section**********************************

;*******************************************************************************
; entries for 64 bit
;*******************************************************************************
[MOD7000_a.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_e.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_f.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_g.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_h.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_i.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_m.NTamd64]
Include    = ks.inf, kscaptur.inf, bda.inf
Needs      = KS.Registration, KSCAPTUR.Registration, BDA.Installation, BDA.Registration,
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64
;-------------------------------------------------------------------------------

[MOD7000_a.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_e.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_f.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_g.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_h.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_i.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64

[MOD7000_m.NTamd64.NT]
Include    = ks.inf, kscaptur.inf, bda.inf, wdmaudio.inf
Needs      = KS.Registration.NT, KSCAPTUR.Registration.NT, BDA.Installation.NT
AddReg     = MOD7000.AddReg.NTamd64
CopyFiles  = SECTION64.CopyDrivers.NTamd64
;-------------------------------------------------------------------------------

[MOD7000_a.NTamd64.NT.HW]
AddReg = MOD7000_a_DEVICE_AddReg

[MOD7000_e.NTamd64.NT.HW]
AddReg = MOD7000_e_DEVICE_AddReg

[MOD7000_f.NTamd64.NT.HW]
AddReg = MOD7000_f_DEVICE_AddReg

[MOD7000_g.NTamd64.NT.HW]
AddReg = MOD7000_g_DEVICE_AddReg

[MOD7000_h.NTamd64.NT.HW]
AddReg = MOD7000_h_DEVICE_AddReg

[MOD7000_i.NTamd64.NT.HW]
AddReg = MOD7000_i_DEVICE_AddReg

[MOD7000_m.NTamd64.NT.HW]
AddReg = MOD7000_m_DEVICE_AddReg
;-------------------------------------------------------------------------------

[MOD7000_a.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_e.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_f.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_g.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_h.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_i.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64

[MOD7000_m.NTamd64.NT.Services]
Addservice = mod7764, 0x00000002, MOD7000.AddService.NTamd64
;---------------------------------------------------------------------------------------

[MOD7000.AddService.NTamd64]
DisplayName    = %MOD7000.FriendlyName%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\mod77-64.sys
LoadOrderGroup = Base
AddReg         = MOD7000.Service.AddReg.NTamd64

[MOD7000.Service.AddReg.NTamd64]
HKR,,DigitalJmp,0x00010001,0x00
HKR,"parameters","ReducedScanning",0x0000001,0x00

[MOD7000.AddReg.NTamd64]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,mod77-64.sys
HKR,,PageOutWhenUnopened,3,01
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D}
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{FF7451BA-42F1-4a9e-9908-E12406A48D6D},Name,,"Tuner Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F}
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{7969986E-A637-4e4e-8AC8-0BD9A02DFC1F},Name,,"Demodulator Node"
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81}
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Display,0x00010001,0
HKLM,System\CurrentControlSet\Control\MediaCategories\{54B37042-5CED-48dd-BF4B-16FF7D6E8C81},Name,,"Antenna In Pin"

; add audio input and output pinnames
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_IN_PIN%,"Name",,"Analog Audio input"
HKLM,SYSTEM\CurrentControlSet\Control\MediaCategories\%HOOK_ANLG_AUDIO_OUT_PIN%,"Name",,"Audio"
;*********************** end of 64 bit section *********************************

;*******************************************************************************
;fuer 32 & 64 bit gültig, einzelne Produkt-ID's
;*******************************************************************************
[MOD7000_a_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001E98
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_e_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001EBE
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_f_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001E3C
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_g_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001EBC
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_h_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001E78
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_i_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001EFE
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"

[MOD7000_m_DEVICE_AddReg]
HKR,,"ProductId",0x00010001,0x00001E80
HKR,,"MaskDevicePath",0x00010001,0x00000000
HKR,,"BdaDigCaptureFilterName",0,"BDA Digital Capture"
HKR,,"BdaDigTunerFilterName",0,"BDA Digital Tuner"
HKR,,"AnlgTunerFilterName",0,"BDA Analog TV Tuner"
HKR,,"AnlgCaptureFilterName",0,"BDA Analog Capture"
HKR,,"AnlgXBarFilterName",0,"BDA Analog Xbar"
HKR,,"AnlgTVAudioFilterName",0,"BDA Analog TV Audio"
HKR,,"ControlFilterName",0,"Control Filter"
HKR,,"AnlgAudioCaptureFilterName",0,"BDA Analog Audio Capture"


[Strings]

;Pin Id
HOOK_ANLG_AUDIO_IN_PIN  = "{356A9E15-B6B8-4066-A381-B531C606A200}"
HOOK_ANLG_AUDIO_OUT_PIN = "{0A95FEC0-4617-4f93-9861-91C9E59E1C09}"


ctx              	= "CTX"
MfgName              	= "TV Device"
MOD7000_a.DeviceDesc 	= "Hybrid USB device"
MOD7000_b.DeviceDesc 	= "Hybrid Express Card device"
MOD7000_c.DeviceDesc 	= "Hybrid Mini Card device"
MOD7000_d.DeviceDesc 	= "Hybrid USB device"
MOD7000_e.DeviceDesc 	= "TV Antenna diversity USB device"
MOD7000_f.DeviceDesc 	= "TV Antenna diversity Mini PCI device"
MOD7000_g.DeviceDesc 	= "TV USB device"
MOD7000_h.DeviceDesc 	= "TV Mini Card device"
MOD7000_i.DeviceDesc 	= "TV Antenna diversity USB device"
MOD7000_k.DeviceDesc 	= "TV Mini Card device"
MOD7000_m.DeviceDesc 	= "TV USB device"
MOD7000_n.DeviceDesc 	= "TV Mini Card device"
MOD7000_o.DeviceDesc 	= "TV Express Card"
MOD7000_p.DeviceDesc 	= "TV Express Card"
MOD7000_q.DeviceDesc	= "TV USB Device"
MOD7000_r.DeviceDesc	= "TV USB-Stick"
MOD7000_s.DeviceDesc	= "TV Express Card"
MOD7000_t.DeviceDesc	= "TV Express Card"
MOD7000.FriendlyName 	= "Tv Tuner device"
INSTALLATION_DISK    	= "CTX Installation Disk"

;
; The following items should be moved to KS_registration - TCP
;

MediaCategories         = "SYSTEM\CurrentControlSet\Control\MediaCategories"
    

;
; ServiceType values
SERVICE_KERNEL_DRIVER			= 0x00000001
SERVICE_FILE_SYSTEM_DRIVER		= 0x00000002
SERVICE_ADAPTER					= 0x00000004
SERVICE_RECOGNIZER_DRIVER		= 0x00000008
SERVICE_WIN32_OWN_PROCESS		= 0x00000010
SERVICE_WIN32_SHARE_PROCESS		= 0x00000020
SERVICE_INTERACTIVE_PROCESS		= 0x00000100
SERVICE_INTERACTIVE_SHARE_PROCESS	= 0x00000120

; StartType values
SERVICE_BOOT_START          = 0x00000000
SERVICE_SYSTEM_START        = 0x00000001
SERVICE_AUTO_START          = 0x00000002
SERVICE_DEMAND_START        = 0x00000003
SERVICE_DISABLED            = 0x00000004

; ErrorControl values
SERVICE_ERROR_IGNORE        = 0x00000000
SERVICE_ERROR_NORMAL        = 0x00000001
SERVICE_ERROR_SEVERE        = 0x00000002
SERVICE_ERROR_CRITICAL      = 0x00000003

; Characteristic flags
NCF_VIRTUAL                 = 0x0001
NCF_WRAPPER                 = 0x0002
NCF_PHYSICAL                = 0x0004
NCF_HIDDEN                  = 0x0008
NCF_NO_SERVICE              = 0x0010
NCF_NOT_USER_REMOVABLE      = 0x0020
NCF_HAS_UI                  = 0x0080
NCF_MODEM                   = 0x0100

; Registry types
REG_MULTI_SZ                = 0x10000
REG_EXPAND_SZ               = 0x20000
REG_DWORD                   = 0x10001

; Win9x Compatible Types
REG_BINARY                  = 17
REG_SZ                      = 0

; Service install flags
SPSVCINST_TAGTOFRONT        = 0x1
SPSVCINST_ASSOCSERVICE      = 0x2

