; AmUHubftr.inf
;
; Installation inf for the Device that needs flitering adapter.
;
; (c) Copyright 1999 Microsoft
;

[Version]
Signature="$Windows NT$"
Provider=%AM%
ClassGUID={36FC9E60-C465-11CF-8056-444553540000}
Class=USB
; Uncomment the following line when you have a valid catalog file.
;         If you use bogus catalog file installation will fail.
CatalogFile=AmUHubftr.cat
DriverVer=12/20/2013,2.0.11.0

[DestinationDirs]
DefaultDestDir   = 12

;
; Driver information
;

[Manufacturer]
%GenericHub.DeviceDesc%   = DDK_Ex.Mfg

[DDK_Ex.Mfg]
%GenericHub.DeviceDesc%=AmUHubftr, USB\VID_058F&PID_6254&rev_0100

;
; General installation section
;

[AmUHubftr]
; perform port related actions from msmouse.inf
Include=usbhub3.inf
Needs=Generic.Install

; Copy the driver over
CopyFiles=AmUHubftr.CopyFiles

; The feature score provides a way to rank drivers
FeatureScore=0

;
; File sections
;

[AmUHubftr.CopyFiles]
AmUHubftr.sys


;
; Service Installation
;

[AmUHubftr.Services]
AddService = AmUHubftr,  , AmUHubftr_Service_Inst
; Install the port driver and mouclass from msmouse.inf
Include=usbhub3.inf
Needs=Generic.Install.NT.Services

[AmUHubftr_Service_Inst]
DisplayName    = %AmUHubftr.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 3                  ; SERVICE_DEMAND_START
ErrorControl   = 1                  ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\AmUHubftr.sys

[AmUHubftr.HW]
; Add the device upper filter
AddReg = AmUHubftr.HW.AddReg

; run the directives need by the port driver
Include=usbhub3.inf
Needs=Generic.Install.NT.HW

[AmUHubftr.HW.AddReg]
HKR,,"LowerFilters",0x00010000,"AmUHubftr"
;HKR,,"UsbIoctlTimeoutValue",0x10001,10000

;
; Source file information
;

; use [SourceDisksNames.x86] for x86 only installs
; use [SourceDisksNames.alpha] for alpha only installs

[SourceDisksNames]
1 = %DiskId1%,,,

[SourceDisksFiles]
AmUHubftr.sys = 1,,


[Strings]

;
; Non-Localizable Strings
;

REG_SZ         = 0x00000000
REG_MULTI_SZ   = 0x00010000
REG_EXPAND_SZ  = 0x00020000
REG_BINARY     = 0x00000001
REG_DWORD      = 0x00010001
SERVICEROOT    = "System\CurrentControlSet\Services"

;
; Localizable Strings
;

DiskId1 = "Generic USB Hub Driver"
AmUHubftr.SvcDesc="AM USB Hub Driver"
GenericHub.DeviceDesc = "Generic USB Hub"
AM = "Alcor Micro, Corp."
