Wami Rack 20 EWDM Driver
Hardware Compatiable | AGP VGA is required. ( Please avoid using PCI VGA ) Ultra DMA - 33 , 66 harddisk is required. ("DMA" switch in Harddisk property should be turned ON ) Must install most recent mother board patch available for newer mother boards such as Intel 815, AMD 750...
get Intel patch
get AMD patch
get VIA patch ( or here )

Support OS | Win 98 SE Win ME Win 2000 ( Win95 and WIn98 are not supported )
Include Driver | MME ( CakeWalk, WaveLab,CoolEditor ...) ASIO ( Cubase, Nuendo, Logic.. ) Multi Client Audio YES DirectSound YES DVD 5.1ch out YES
GSIF
GIGA-WIRE
Latency | ASIO : min = 3 ms, max = 24 ms MME : min = 3 ms, max = 24 ms
v 1.0 Release Note | First release
v 1.1 Release Note | Add GSIF
v 1.3 Release Note | Add GIGA-WIRE
v 1.31 Release Note | Fixed : ASIO not working on WIn2000
Bug Report : EgoSys