; EETI Vendor INF File for USB HID Multi-touch devices
;
; (c) Copyright 2009 eGalax_eMPIA Technology Inc.
; 

[Version]
Signature            = "$Windows NT$"
Provider             = %ProviderName%
Class                = HIDClass
CLASSGUID            = {745a17a0-74d3-11d0-b6fe-00a0c90f57da};
DriverVer            = 08/11/2009,1.0.0.0                    
CatalogFile.NT       = pcap7302.cat

[ControlFlags]
ExcludeFromSelect=*

;[SourceDisksNames]
;1=%SourceDisk%,,1

[Manufacturer]
%ManufacturerName% = EETIHID,NT.6.0,NTx86,NTamd64

; Match on a hardware ID generated by the device, for x86 and x64.

[EETIHID.NT.6.0]
%HIDDevice1%       = HIDSelSusp1.NT.6.0, USB\VID_0EEF&PID_7302

[EETIHID.NTx86]
%HIDDevice1%       = HIDSelSusp1.NT.6.0, USB\VID_0EEF&PID_7302

[EETIHID.NTamd64]
%HIDDevice1%       = HIDSelSusp1.NT.6.0, USB\VID_0EEF&PID_7302


; Windows Vista-specific sections -------------------------

[HIDSelSusp1.NT.6.0]
include     = input.inf
needs       = HID_SelSus_Inst.NT

[HIDSelSusp1.NT.6.0.HW]
include     = input.inf
needs       = HID_SelSus_Inst.NT.HW

[HIDSelSusp1.NT.6.0.Services]
include     = input.inf
needs       = HID_SelSus_Inst.NT.Services

[Strings]
; While strings are localizable, in this sample INF, we have
; not created any localized strings.
ProviderName     = "EETI"
HIDDevice1       = "EETI PCAP MultiTouch Digitizer"
ManufacturerName = "EETI"
BthRadio1        = "Selective Suspend HID from EETI"
SourceDisk       = "EETI source disk"