Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
Invalid keyboard code specified
;Copyright (C) JMicron Technology Corp.

[Version]
Signature="$Windows NT$"
Provider=%JMICRON%
ClassGUID={4D36E97B-E325-11CE-BFC1-08002BE10318}
Class=SCSIAdapter
DriverVer=09/17/2012, 1.17.65.11
CatalogFile=jraid.cat

[DestinationDirs]
DefaultDestDir = 12 ; DIRID_DRIVERS
JRAID.Copy     = 12
JRAID.Del      = 12

[Manufacturer]
%JMICRON%=JM.Mfg

[JM.Mfg]
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2360
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2361
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2362
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2363
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2364
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2366
%PCI\VEN_197B&DEV_2363.DeviceDesc% = JM , PCI\VEN_197B&DEV_2369
%PCI\VEN_197B&DEV_237x.DeviceDesc% = JM , PCI\VEN_197B&DEV_2373

[JM]
CopyFiles=JRAID.Copy
;Reboot

[JRAID.Copy]
jraid.sys

[JM.Services]
AddService = JRAID, 2, JM_Service_Inst, JM_EventLog_Inst

[JM_Service_Inst]
ServiceType    = 1      ; SERVICE_KERNEL_DRIVER
StartType      = 0      ; SERVICE_BOOT_START
ErrorControl   = 1      ; SERVICE_ERROR_NORMAL
;LoadOrderGroup = SCSI Miniport
LoadOrderGroup = System Bus Extender
ServiceBinary  = %12%\jraid.sys
AddReg         = pnp_pci_addreg

[pnp_pci_addreg]
HKR, "Parameters\PnpInterface", "5", 0x00010001, 0x00000001
HKR, "Parameters\Device", "CreateInitiatorLU", 0x00010001, 0x00000001
HKR, "Parameters", "BusType", 0x00010001, 0x00000008
HKR, "Private", "UseBigUnCache", 0x00010001, 0x00000000

[JM_EventLog_Inst]
AddReg = JM_EventLog_AddReg

[JM_EventLog_AddReg]
HKR,,EventMessageFile,0x00020000,"%SystemRoot%\System32\IoLogMsg.dll;%SystemRoot%\System32\drivers\jraid.sys"
HKR,,TypesSupported,0x00010001,7

[SourceDisksNames]
1 = %DISKNAME%,,,,

[SourceDisksFiles]
jraid.sys = 1
JMInsDrv.dll = 1

; [JMPROCESSOR] is designed for pseudo devices
;[JMPROCESSOR]
;AddReg = JMPROCESSOR_ADDREG

;[JMPROCESSOR.Services]
;AddService = , 0x00000002

;[JMPROCESSOR_ADDREG]


;
; [Driver.Uninst] is designed for removing driver files by JmInsdrv.dll;
; This section  is only executed during uninstall with setup program.
;
[Driver.Uninst]
DelFiles=JRAID.Del
DelReg=Uninst.DelReg

[JRAID.Del]
jraid.sys,,,1
jgogo.sys,,,1

[Uninst.DelReg]
HKLM,System\CurrentControlSet\Services\JRAID
HKLM,System\CurrentControlSet\Services\JGOGO


[strings]
JMICRON="JMicron Technology Corp."
PCI\VEN_197B&DEV_2363.DeviceDesc="JMicron JMB36X Controller"
PCI\VEN_197B&DEV_237x.DeviceDesc="JMicron JMB37X Controller"
PCI\VEN_197B&DEV_2368.DeviceDesc="JMicron JMB368 IDE Controller"
;SCSI\ProcessorJMicron_RAIDController______.DeviceDesc="JMicron JMB36X RAID Processor"
DISKNAME="JMicron Driver Diskette"

