;VERSION 2.210 FOR F/W 2.210


[Version]
Signature="$CHICAGO$"
Class=MEDIA
provider=%AOpen%
LayoutFile=layout.inf

[CTInfVersion]
InfName=AOP_WAV.INF
InfVersion=1.0

[ControlFlags]
ExcludeFromSelect=AOpen

[ClassInstall]
Addreg=Class.AddReg

[Class.AddReg]
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[DestinationDirs]
UPDATEINFFILE=17,OTHER\

[Manufacturer]
%CLMfgName%=AOpen

[AOpen]
%Rockwell.DeviceDesc1%=ROCKWELL,MODEMWAVE\AOpen_FM56-RU
%Rockwell.DeviceDesc2%=ROCKWELL,MODEMWAVE\AOpen_FM56-RU
%Rockwell.DeviceDesc3%=ROCKWELL,MODEMWAVE\56modem

[PreCopySection]
HKR,,NoSetupUI,,1

[DestinationDirs]
MSSERWAVE.CopyList = 11 ; LDID_SYS

[ROCKWELL]
DelFiles=UPDATEINFFILE
AddReg=MSSERWAVE.AddReg, ROCKWELL.AddReg

[MSSERWAVE.CopyList]
serwave.vxd,,
serwvdrv.drv,,
vmodctl.dll,,

[ROCKWELL.AddReg]
HKR,Drivers\wave\serwvdrv.drv,Description,,%ROCKWELL.VoiceModem%
HKR,Config,XformModule,  , "umdmxfrm.dll"
HKR,Config,XformID,     1, 01, 00, 00, 00

[MSSERWAVE.AddReg]
HKR,,DevLoader,,mmdevldr.vxd
HKR,Drivers,MIGRATED,,0
HKR,Drivers\wave,,,
HKR,,Driver,,serwave.vxd
HKR,Drivers\wave\serwvdrv.drv,Driver,,serwvdrv.drv
HKR,Drivers,SubClasses,,"wave"

[UPDATEINFFILE]
<Filename>,%AOpen%AOP_WAV.INF

[Strings]
TMR="AOpen"
CLMfgName="AOpen"
Rockwell.DeviceDesc1="AOpen Voice Modem Wave Device"
Rockwell.DeviceDesc2="AOpen Voice Modem Wave Device"
Rockwell.DeviceDesc3="AOpen Voice Modem Wave Device"
