
       Оптимизированный драйвер INTEL Graphics 10.18.15.4177 для использования в PE_7x64, PE_8x64.

    Драйвер пригоден для установщика DevInst, SDI или стандартного обновления устройств.

    Для стандартного обновления устройств распакуйте драйвер до уровня каталогов с файлами.

--------------------------------------------------------------------------------------------------

      Драйвер INTEL Graphics 10.18.15.4177 Windows 7/8 (64 bit), каталог IG1018154177_NT6x64.     

    DriverVer=03/23/2015, 10.18.15.4177. Отключены OpenCL, OpenGL, ControlPanel, WiDi Miracast.

    Product Support:

     6th Generation Intel® Core™ processor family (codename Skylake)
     5th Generation Intel® Core™ processor family (codename Broadwell)
     4th Generation Intel® Core™ processor family (codename Haswell)     ;;;закоментировано 
     CherryView Intel® processor family (Braswell)

    Для Windows 8.1 используется секция igfx_SoftwareDX11Settings вместо igfx_SoftwareDX12Settings

--------------------------------------------------------------------------------------------------

     ; BDW HW
     iBDWULTGT1	     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics" 
     iBDWULTGT2      = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics 5500" 
     iBDWULTGT3      = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics 6000" 
     iBDWULXGT1      = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics" 
     iBDWULXGT2      = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics 5300" 
     iBDWHALOGT2     = "(PE64) Intel(R) 5th Generation Broadwell HD Graphics 5600" 
     iBDWHALOGT3     = "(PE64) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics 6200" 
     iBDWGT3SRVR     = "(PE64) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics P6300" 
     iBDWGT2SRVR     = "(PE64) Intel(R) 5th Generation Broadwell Iris(TM) Pro Graphics P6300" 
     iBDWULTGT328W   = "(PE64) Intel(R) 5th Generation Broadwell Iris(TM) Graphics 6100" 
     
     ; CHV HW  
     iCHVGM0         = "(PE64) Intel(R) CherryView (Braswell) HD Graphics" 
     iCHVGM1         = "(PE64) Intel(R) CherryView (Braswell) HD Graphics" 
     
     ; SKL HW
     iSKLULTGT1      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULT GT1"  
     iSKLULTGT15     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULT GT1.5"  
     iSKLULTGT2      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULT GT2" 
     iSKLULXGT1      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULX GT1" 
     iSKLULXGT15     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULX GT1.5" 
     iSKLULXGT2      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULX GT2" 
     iSKLDTGT2       = "(PE64) Intel(R) 6th Generation Skylake HD Graphics DT GT2" 
     iSKLULTGT3      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULT GT3" 
     iSKLULTGT2f     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics ULT GT2f" 
     iSKLDTGT15      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics DT GT1.5" 
     iSKLDTGT1       = "(PE64) Intel(R) 6th Generation Skylake HD Graphics DT GT1" 
     iSKLHaloGT4     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics Halo GT4" 
     iSKLDTGT4       = "(PE64) Intel(R) 6th Generation Skylake HD Graphics DT GT4" 
     iSKLHaloGT2     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics Halo GT2" 
     iSKLHaloGT3     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics Halo GT3" 
     iSKLHaloGT1     = "(PE64) Intel(R) 6th Generation Skylake HD Graphics Halo GT1" 
     iSKLSRVGT1      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics SRV GT1" 
     iSKLSRVGT2      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics SRV GT2" 
     iSKLSRVGT3      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics SRV GT3" 
     iSKLSRVGT4      = "(PE64) Intel(R) 6th Generation Skylake HD Graphics SRV GT4" 
     iSKLWSGT2       = "(PE64) Intel(R) 6th Generation Skylake HD Graphics WS GT2" 
     iSKLWSGT4       = "(PE64) Intel(R) 6th Generation Skylake HD Graphics WS GT4" 

--------------------------------------------------------------------------------------------------

      В случае установки драйвера  видеоадаптера  через диспетчер устройств,  необходимо выполнить

    детект PnP устройств или запустить утилиту типа Resolution Changer SX2 для того чтобы заменить

    пока еще работающий стандартный VGA драйвер  (иначе появляется ошибка при изменении параметров

    экрана).  При подключении  посредством  DevInst.exe автоматически  устанавливается оптимальное

    разрешение и частота регенерации для обнаруженного типа монитора.

==================================================================================================
 07-Jan-2016 nat27 http://forum.ru-board.com/topic.cgi?forum=62&topic=24098&start=71&limit=1&m=1#1
==================================================================================================
  